{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":3915,"n_cols":91,"rows_kept":2250,"cut":true,"hidden":false,"merged":[[3898,4,3898,6],[3899,3,3899,5],[3900,4,3900,5],[3900,7,3900,8],[3900,12,3900,13],[3900,15,3900,16],[3900,18,3900,19],[3900,24,3900,25],[3900,27,3900,28],[3900,30,3900,31],[3900,36,3900,37],[3900,39,3900,40],[3900,42,3900,43],[3900,48,3900,49],[3900,51,3900,52],[3900,54,3900,55],[3900,60,3900,61],[3900,63,3900,64],[3900,68,3900,69],[3900,71,3900,72],[3900,74,3900,75],[3901,4,3901,6],[3901,8,3901,9],[3901,11,3901,13],[3901,17,3901,19],[3901,21,3901,23],[3902,4,3902,6],[3903,7,3903,9],[3903,11,3903,12],[3903,14,3903,16],[3904,3,3904,5],[3904,12,3904,14],[3891,57,3891,58],[3891,60,3891,62],[3891,66,3891,68],[3891,70,3891,72],[3892,4,3892,6],[3893,7,3893,9],[3893,11,3893,12],[3893,14,3893,16],[3894,3,3894,5],[3894,12,3894,14],[3896,7,3896,8],[3896,14,3896,15],[3896,17,3896,18],[3896,25,3896,26],[3896,28,3896,29],[3896,36,3896,37],[3896,39,3896,40],[3896,47,3896,48],[3896,50,3896,51],[3896,58,3896,59],[3896,65,3896,66],[3896,70,3896,71],[3897,4,3897,5],[3897,11,3897,12],[3897,14,3897,15],[3897,22,3897,23],[3897,25,3897,26],[3897,33,3897,34],[3897,36,3897,37],[3897,44,3897,45],[3897,47,3897,48],[3897,55,3897,56],[3897,62,3897,63],[3897,67,3897,68],[3897,70,3897,72],[3886,3,3886,5],[3886,12,3886,14],[3888,7,3888,8],[3888,14,3888,15],[3888,17,3888,18],[3888,25,3888,26],[3888,28,3888,29],[3888,36,3888,37],[3888,43,3888,44],[3888,48,3888,49],[3889,4,3889,5],[3889,11,3889,12],[3889,14,3889,15],[3889,22,3889,23],[3889,25,3889,26],[3889,33,3889,34],[3889,40,3889,41],[3889,45,3889,46],[3889,48,3889,50],[3889,54,3889,56],[3890,3,3890,5],[3891,4,3891,5],[3891,7,3891,8],[3891,12,3891,13],[3891,15,3891,16],[3891,18,3891,19],[3891,24,3891,25],[3891,27,3891,28],[3891,30,3891,31],[3891,36,3891,37],[3891,39,3891,40],[3891,44,3891,45],[3891,47,3891,48],[3891,50,3891,51],[3891,53,3891,55],[3877,6,3877,7],[3877,9,3877,10],[3877,14,3877,15],[3877,17,3877,18],[3877,22,3877,23],[3877,25,3877,26],[3877,30,3877,31],[3877,33,3877,34],[3877,42,3877,44],[3878,12,3878,14],[3878,18,3878,20],[3878,25,3878,27],[3880,7,3880,8],[3880,14,3880,15],[3880,21,3880,22],[3880,26,3880,27],[3881,4,3881,5],[3881,11,3881,12],[3881,18,3881,19],[3881,23,3881,24],[3882,3,3882,5],[3883,4,3883,5],[3883,7,3883,8],[3883,12,3883,13],[3883,15,3883,16],[3883,20,3883,21],[3883,23,3883,24],[3883,26,3883,27],[3883,31,3883,33],[3883,35,3883,37],[3884,4,3884,6],[3885,7,3885,9],[3885,11,3885,12],[3885,14,3885,16],[3873,6,3873,7],[3873,9,3873,10],[3873,14,3873,15],[3873,17,3873,18],[3873,20,3873,21],[3873,26,3873,27],[3873,29,3873,30],[3873,32,3873,33],[3873,38,3873,39],[3873,41,3873,42],[3873,46,3873,47],[3873,49,3873,50],[3873,52,3873,53],[3873,55,3873,57],[3873,59,3873,60],[3873,62,3873,64],[3873,66,3873,68],[3874,6,3874,7],[3874,9,3874,10],[3874,14,3874,15],[3874,17,3874,18],[3874,22,3874,23],[3874,25,3874,26],[3874,30,3874,31],[3874,33,3874,34],[3874,42,3874,44],[3875,12,3875,14],[3875,18,3875,20],[3875,25,3875,27],[3876,6,3876,7],[3876,9,3876,10],[3876,12,3876,13],[3876,15,3876,16],[3876,18,3876,19],[3876,24,3876,25],[3876,27,3876,28],[3876,30,3876,31],[3876,36,3876,37],[3876,39,3876,40],[3876,44,3876,45],[3876,47,3876,48],[3876,52,3876,54],[3876,56,3876,58],[3863,62,3863,63],[3863,67,3863,68],[3867,6,3867,7],[3867,9,3867,10],[3867,14,3867,15],[3867,17,3867,18],[3867,22,3867,23],[3867,25,3867,26],[3867,28,3867,29],[3868,6,3868,7],[3868,9,3868,10],[3868,14,3868,15],[3868,17,3868,18],[3868,26,3868,28],[3867,31,3867,33],[3869,12,3869,14],[3869,18,3869,20],[3869,25,3869,27],[3870,6,3870,7],[3870,9,3870,10],[3870,12,3870,13],[3870,15,3870,16],[3870,20,3870,21],[3870,23,3870,24],[3870,28,3870,30],[3871,6,3871,7],[3871,9,3871,10],[3871,14,3871,15],[3871,17,3871,18],[3871,26,3871,28],[3872,12,3872,14],[3872,18,3872,20],[3872,25,3872,27],[3861,4,3861,5],[3861,7,3861,8],[3861,10,3861,11],[3861,15,3861,16],[3861,18,3861,19],[3861,21,3861,22],[3861,26,3861,27],[3861,29,3861,30],[3861,34,3861,35],[3861,37,3861,38],[3861,40,3861,41],[3861,45,3861,46],[3861,50,3861,51],[3862,4,3862,5],[3862,9,3862,10],[3862,12,3862,13],[3862,20,3862,21],[3862,23,3862,24],[3862,31,3862,32],[3862,34,3862,35],[3862,42,3862,43],[3862,45,3862,46],[3862,53,3862,54],[3862,60,3862,61],[3863,4,3863,5],[3863,11,3863,12],[3863,14,3863,15],[3863,22,3863,23],[3863,25,3863,26],[3863,33,3863,34],[3863,36,3863,37],[3863,44,3863,45],[3863,47,3863,48],[3863,55,3863,56],[2013,59,2013,60],[2015,44,2015,47],[2015,58,2015,61],[2006,67,2008,67],[2007,71,2007,72],[2010,74,2010,75],[2013,72,2013,73],[2015,71,2015,74],[2081,41,2083,41],[2081,54,2083,54],[2081,67,2083,67],[2082,45,2082,46],[2082,58,2082,59],[2082,71,2082,72],[2085,48,2085,49],[2085,61,2085,62],[2085,74,2085,75],[2088,46,2088,47],[2088,59,2088,60],[2088,72,2088,73],[2090,44,2090,47],[2090,58,2090,61],[2090,71,2090,74],[3753,6,3753,8],[3754,4,3754,6],[3756,4,3756,6],[3756,34,3756,37],[3714,1,3714,80],[3716,26,3716,27],[3717,18,3717,19],[3720,45,3720,46],[3724,2,3724,3],[3724,18,3724,19],[3726,42,3726,43],[3727,30,3727,31],[3727,38,3727,39],[3729,34,3729,35],[3736,40,3736,42],[3736,46,3736,48],[3736,29,3736,32],[3736,34,3736,36],[3704,5,3704,7],[3704,32,3704,33],[3704,34,3704,35],[3705,23,3705,25],[3706,5,3706,7],[3725,68,3725,69],[3734,30,3734,31],[3734,33,3734,34],[3734,38,3734,39],[3740,4,3740,5],[3740,11,3740,14],[3740,34,3740,36],[3741,4,3741,6],[3742,4,3742,6],[3742,10,3742,11],[3746,6,3746,8],[3721,61,3723,61],[3722,65,3722,66],[3753,12,3753,13],[3754,10,3754,11],[3756,8,3756,9],[3756,11,3756,12],[3737,4,3737,6],[3761,6,3761,8],[3761,12,3761,13],[3762,4,3762,6],[3751,14,3751,16],[3753,15,3753,17],[3753,23,3753,25],[3754,13,3754,15],[3754,21,3754,23],[3755,3,3755,5],[3756,14,3756,16],[3756,18,3756,19],[3756,23,3756,25],[3756,27,3756,28],[3763,3,3763,5],[3764,14,3764,16],[3764,18,3764,19],[3764,23,3764,25],[3764,27,3764,28],[3764,32,3764,34],[3764,36,3764,37],[3764,39,3764,41],[3764,45,3764,48],[3765,4,3765,6],[3762,10,3762,11],[3764,4,3764,6],[3764,8,3764,9],[3764,11,3764,12],[3728,66,3728,67],[3730,64,3730,67],[3724,28,3724,33],[3724,36,3724,41],[3732,16,3732,17],[3733,13,3733,14],[3733,16,3733,17],[3733,19,3733,20],[3733,24,3733,25],[3733,42,3733,43],[3733,45,3733,46],[3733,50,3733,51],[3736,22,3736,23],[3738,10,3738,11],[3734,4,3734,5],[3734,7,3734,8],[3734,10,3734,11],[3734,15,3734,16],[3734,18,3734,19],[3734,23,3734,24],[3740,40,3740,42],[3740,46,3740,48],[3741,12,3741,14],[3741,20,3741,22],[3742,13,3742,15],[3742,21,3742,23],[3746,15,3746,17],[3746,19,3746,20],[3746,24,3746,26],[3746,28,3746,29],[3746,31,3746,33],[3748,14,3748,16],[3749,16,3749,18],[3749,20,3749,21],[3749,25,3749,27],[3749,29,3749,30],[3749,34,3749,36],[3738,4,3738,6],[3749,6,3749,8],[3731,33,3731,36],[3732,8,3732,9],[3766,7,3766,9],[3766,11,3766,12],[3766,14,3766,16],[3767,3,3767,5],[3767,12,3767,14],[3717,33,3717,34],[3721,50,3723,50],[3722,54,3722,55],[3725,57,3725,58],[3728,55,3728,56],[3730,53,3730,56],[3683,30,3683,32],[3685,5,3685,7],[3686,5,3686,7],[3688,7,3688,8],[3688,10,3688,11],[3688,20,3688,22],[3698,4,3698,6],[3699,11,3699,13],[3699,17,3699,19],[3699,21,3699,23],[3699,25,3699,26],[3699,28,3699,30],[3699,32,3699,33],[3699,35,3699,37],[3700,5,3700,7],[3700,9,3700,10],[3700,12,3700,13],[3700,15,3700,16],[3700,18,3700,19],[3700,23,3700,25],[3702,4,3702,6],[3703,24,3703,26],[3703,32,3703,33],[3757,4,3757,6],[3758,7,3758,9],[3758,11,3758,12],[3758,14,3758,16],[3759,3,3759,5],[3759,12,3759,14],[3761,15,3761,17],[3761,23,3761,25],[3762,13,3762,15],[3762,21,3762,23],[3762,29,3762,31],[3762,35,3762,37],[3732,11,3732,12],[3733,8,3733,9],[3733,31,3733,32],[3733,34,3733,35],[3733,37,3733,38],[3736,4,3736,5],[3736,9,3736,12],[3736,14,3736,15],[3736,17,3736,20],[3746,10,3746,11],[3749,10,3749,11],[3749,13,3749,14],[3737,12,3737,14],[3737,20,3737,22],[3738,13,3738,15],[3738,21,3738,23],[3740,16,3740,17],[3740,21,3740,24],[3740,26,3740,27],[3740,29,3740,32],[3682,11,3682,12],[3682,18,3682,19],[3682,23,3682,25],[3682,27,3682,28],[3682,30,3682,31],[3682,38,3682,39],[3682,43,3682,44],[3682,46,3682,48],[3703,34,3703,35],[3703,36,3703,37],[3703,38,3703,39],[3690,20,3690,22],[3690,26,3690,27],[3692,4,3692,6],[3693,5,3693,7],[3693,9,3693,10],[3693,14,3693,16],[3693,18,3693,19],[3693,23,3693,25],[3693,27,3693,28],[3693,30,3693,31],[3693,35,3693,37],[3693,39,3693,41],[3694,5,3694,7],[3695,8,3695,10],[3695,12,3695,13],[3695,15,3695,17],[3696,4,3696,6],[3696,13,3696,15],[3707,23,3707,25],[3708,6,3708,8],[3709,23,3709,25],[3711,5,3711,6],[3711,8,3711,10],[3711,12,3711,13],[3711,15,3711,17],[3711,21,3711,23],[3711,27,3711,29],[3711,33,3711,35],[3711,37,3711,39],[3703,6,3703,8],[3703,10,3703,12],[3703,14,3703,15],[3703,17,3703,19],[3703,21,3703,22],[3705,5,3705,7],[3705,9,3705,11],[3705,13,3705,14],[3705,16,3705,18],[3705,20,3705,21],[3707,5,3707,7],[3707,9,3707,11],[3707,13,3707,14],[3707,16,3707,18],[3707,20,3707,21],[3709,5,3709,7],[3709,9,3709,11],[3709,13,3709,14],[3709,16,3709,18],[3709,20,3709,21],[3683,13,3683,14],[3683,16,3683,18],[3683,20,3683,21],[3683,27,3683,28],[3648,33,3648,34],[3648,36,3648,37],[3642,41,3642,43],[3642,48,3642,49],[3642,50,3642,51],[3642,52,3642,53],[3653,1,3653,80],[3655,24,3655,25],[3656,10,3656,15],[3658,56,3658,58],[3659,56,3659,58],[3660,4,3660,6],[3660,39,3662,39],[3660,57,3660,59],[3661,43,3661,44],[3664,46,3664,47],[3665,9,3665,11],[3665,24,3665,26],[3666,16,3666,17],[3667,44,3667,45],[3669,42,3669,45],[3670,42,3670,45],[3676,15,3676,16],[3676,36,3676,38],[3676,46,3676,47],[3676,51,3676,53],[3676,61,3676,63],[3677,15,3677,17],[3678,17,3678,19],[3678,23,3678,24],[3644,8,3644,9],[3644,11,3644,12],[3644,14,3644,15],[3644,41,3644,43],[3645,4,3645,6],[3646,8,3646,9],[3646,11,3646,12],[3646,14,3646,15],[3646,41,3646,43],[3647,5,3647,7],[3648,8,3648,9],[3648,11,3648,12],[3648,14,3648,15],[3648,41,3648,43],[3644,5,3644,6],[3644,17,3644,18],[3644,20,3644,21],[3650,4,3650,5],[3650,7,3650,9],[3650,11,3650,12],[3650,14,3650,16],[3650,20,3650,22],[3650,26,3650,28],[3650,32,3650,34],[3644,48,3644,49],[3644,50,3644,51],[3524,51,3524,53],[3434,4,3434,6],[3434,12,3434,14],[3434,26,3434,28],[3434,32,3434,34],[3435,4,3435,6],[3435,12,3435,14],[3435,32,3435,34],[3435,38,3435,40],[3440,8,3440,10],[3440,12,3440,13],[3440,15,3440,17],[3440,19,3440,20],[3440,24,3440,25],[3440,36,3440,37],[3441,45,3441,46],[3454,15,3454,16],[3454,18,3454,20],[3454,22,3454,23],[3454,25,3454,27],[3454,29,3454,30],[3455,11,3455,13],[3455,15,3455,16],[3455,18,3455,20],[3455,22,3455,23],[3455,25,3455,27],[3459,15,3459,16],[3458,3,3458,5],[3459,25,3459,27],[3460,22,3460,24],[3459,4,3459,6],[3459,8,3459,9],[3478,23,3478,24],[3476,27,3476,28],[3465,23,3465,24],[3467,12,3467,14],[3467,16,3467,17],[3467,19,3467,21],[3467,23,3467,24],[3469,12,3469,14],[3469,16,3469,17],[3469,19,3469,21],[3469,23,3469,24],[3441,24,3441,25],[3441,31,3441,32],[3441,48,3441,50],[3441,39,3441,41],[3440,41,3440,43],[3443,4,3443,6],[3444,4,3444,6],[3441,12,3441,13],[3489,13,3489,14],[3489,24,3489,25],[3477,6,3477,11],[3476,18,3476,23],[3483,36,3485,36],[3488,5,3488,7],[3499,10,3499,12],[3504,13,3504,15],[3504,17,3504,18],[3504,22,3504,24],[3504,28,3504,30],[3503,32,3503,34],[3505,36,3505,38],[3408,36,3408,38],[3408,40,3408,42],[3403,8,3403,10],[3404,29,3404,31],[3405,9,3405,11],[3406,29,3406,31],[3408,8,3408,9],[3408,11,3408,13],[3408,15,3408,16],[3408,18,3408,20],[3408,24,3408,26],[3408,30,3408,32],[3487,56,3487,57],[3490,41,3490,42],[3490,54,3490,55],[3474,1,3474,80],[3499,14,3499,15],[3523,6,3523,8],[3523,10,3523,11],[3523,18,3523,20],[3523,22,3523,23],[3523,30,3523,32],[3523,38,3523,40],[3523,44,3523,45],[3441,8,3441,10],[3436,4,3436,6],[3436,12,3436,14],[3518,20,3518,21],[3518,23,3518,25],[3518,27,3518,28],[3505,4,3505,6],[3505,16,3505,18],[3505,28,3505,30],[3492,40,3492,43],[3492,53,3492,56],[3499,21,3499,23],[3503,38,3503,40],[3503,49,3503,51],[3504,4,3504,6],[3504,8,3504,9],[3494,40,3494,43],[3501,18,3501,19],[3503,8,3503,9],[3503,17,3503,18],[3503,20,3503,21],[3503,23,3503,24],[3503,42,3503,43],[3436,44,3436,46],[3441,15,3441,17],[3503,28,3503,30],[3488,21,3488,23],[3478,12,3478,13],[3404,9,3404,10],[3404,12,3404,13],[3404,15,3404,16],[3404,18,3404,20],[3404,22,3404,23],[3404,25,3404,27],[3483,63,3483,65],[3465,26,3465,28],[3466,4,3466,6],[3467,5,3467,7],[3467,9,3467,10],[3467,26,3467,28],[3406,9,3406,10],[3406,12,3406,13],[3406,15,3406,16],[3406,18,3406,20],[3406,22,3406,23],[3406,25,3406,27],[3289,59,3289,61],[3291,8,3291,9],[3291,13,3291,14],[3291,16,3291,17],[3291,22,3291,23],[3291,25,3291,26],[3291,28,3291,29],[3291,34,3291,35],[3291,37,3291,38],[3291,46,3291,47],[3291,51,3291,52],[3291,56,3291,58],[3317,60,3317,62],[3323,62,3323,64],[3337,35,3337,37],[3337,39,3337,40],[3337,42,3337,43],[3337,45,3337,46],[3337,48,3337,49],[3333,21,3333,23],[3333,25,3333,26],[3400,44,3400,45],[3400,46,3400,47],[3401,8,3401,10],[3401,40,3401,41],[3401,42,3401,43],[3402,29,3402,31],[3402,25,3402,27],[3341,24,3341,25],[3397,31,3397,33],[3396,8,3396,9],[3396,13,3396,14],[3396,22,3396,23],[3396,25,3396,26],[3396,28,3396,29],[3343,27,3343,29],[3317,64,3317,66],[3378,33,3378,34],[3397,8,3397,9],[3397,13,3397,14],[3397,18,3397,19],[3397,21,3397,22],[3397,24,3397,25],[3397,27,3397,29],[3385,7,3385,9],[3386,8,3386,9],[3346,1,3346,80],[3353,4,3353,6],[3377,48,3377,50],[3342,8,3342,10],[3342,12,3342,13],[3342,15,3342,16],[3351,56,3351,58],[3352,56,3352,58],[3353,57,3353,59],[3342,51,3342,52],[3341,27,3341,28],[3325,67,3325,69],[3303,4,3303,6],[3304,4,3304,6],[3322,57,3322,58],[3323,35,3323,36],[3323,38,3323,39],[3323,46,3323,47],[3323,53,3323,54],[3323,58,3323,59],[3314,34,3314,35],[3314,39,3314,40],[3315,35,3315,36],[3315,40,3315,41],[3315,43,3315,45],[3315,49,3315,51],[3317,29,3317,30],[3317,32,3317,33],[3301,4,3301,6],[3295,6,3295,7],[3295,9,3295,10],[3295,12,3295,13],[3295,15,3295,16],[3295,18,3295,19],[3296,6,3296,8],[3319,14,3319,16],[3320,3,3320,5],[3320,12,3320,14],[3306,19,3306,20],[3306,24,3306,25],[3307,4,3307,6],[3307,12,3307,14],[3307,20,3307,21],[3307,25,3307,26],[3309,4,3309,6],[3309,8,3309,9],[3309,13,3309,15],[3310,4,3310,6],[3311,7,3311,9],[3311,11,3311,12],[3311,14,3311,16],[3312,3,3312,5],[3312,12,3312,14],[3316,3,3316,5],[3317,38,3317,39],[3317,41,3317,42],[3317,44,3317,45],[3317,47,3317,49],[3315,4,3315,6],[3315,12,3315,14],[3315,16,3315,17],[3315,24,3315,25],[3317,26,3317,27],[3318,4,3318,6],[3319,7,3319,9],[3319,11,3319,12],[3317,54,3317,56],[3317,4,3317,6],[3317,8,3317,9],[3317,13,3317,15],[3317,17,3317,18],[3317,20,3317,21],[3287,54,3287,55],[3287,59,3287,60],[3287,64,3287,65],[3287,69,3287,71],[3288,8,3288,9],[3288,13,3288,14],[3288,16,3288,17],[3288,21,3288,22],[3288,24,3288,25],[3288,33,3288,34],[3288,38,3288,40],[3240,37,3240,38],[3242,16,3242,17],[3249,12,3249,14],[3249,44,3249,46],[3251,20,3251,21],[3251,32,3251,33],[3253,28,3253,29],[3241,33,3241,34],[3232,65,3232,67],[3233,4,3233,6],[3234,7,3234,9],[3234,11,3234,12],[3234,14,3234,16],[3235,3,3235,5],[3235,12,3235,14],[3251,40,3251,41],[3244,8,3244,9],[3264,10,3264,11],[3265,14,3265,15],[3266,16,3266,17],[3266,21,3266,22],[3268,8,3268,9],[3268,13,3268,14],[3268,16,3268,17],[3268,19,3268,20],[3268,24,3268,25],[3269,10,3269,11],[3269,18,3269,19],[3269,21,3269,22],[3269,29,3269,30],[3270,12,3270,13],[3270,20,3270,21],[3270,23,3270,24],[3270,31,3270,32],[3270,36,3270,37],[3278,58,3278,59],[3278,61,3278,62],[3278,64,3278,65],[3278,69,3278,70],[3272,8,3272,9],[3272,13,3272,14],[3272,16,3272,17],[3272,19,3272,20],[3273,40,3273,41],[3273,47,3273,48],[3274,12,3274,13],[3274,20,3274,21],[3274,23,3274,24],[3274,31,3274,32],[3274,34,3274,35],[3274,42,3274,43],[3280,37,3280,38],[3280,40,3280,41],[3230,50,3230,52],[3231,3,3231,5],[3232,4,3232,5],[3232,7,3232,8],[3232,10,3232,11],[3232,16,3232,17],[3232,19,3232,20],[3232,22,3232,23],[3232,28,3232,29],[3232,31,3232,32],[3232,34,3232,35],[3232,40,3232,41],[3232,43,3232,44],[3232,48,3232,50],[3232,52,3232,53],[3232,55,3232,57],[3232,61,3232,63],[3227,3,3227,5],[3227,12,3227,14],[3229,7,3229,8],[3229,10,3229,11],[3229,18,3229,19],[3229,21,3229,22],[3229,29,3229,30],[3229,32,3229,33],[3229,40,3229,41],[3230,4,3230,5],[3230,7,3230,8],[3230,15,3230,16],[3230,18,3230,19],[3230,26,3230,27],[3230,29,3230,30],[3230,37,3230,38],[3230,44,3230,46],[3223,3,3223,5],[3224,4,3224,5],[3224,7,3224,8],[3224,10,3224,11],[3224,16,3224,17],[3224,19,3224,20],[3224,22,3224,23],[3224,28,3224,29],[3224,31,3224,32],[3224,36,3224,38],[3224,40,3224,41],[3224,43,3224,45],[3224,49,3224,51],[3224,53,3224,55],[3225,4,3225,6],[3226,7,3226,9],[3226,11,3226,12],[3226,14,3226,16],[3216,37,3216,39],[3216,41,3216,43],[3217,4,3217,6],[3218,7,3218,9],[3218,11,3218,12],[3218,14,3218,16],[3219,3,3219,5],[3219,12,3219,14],[3221,7,3221,8],[3221,10,3221,11],[3221,18,3221,19],[3221,21,3221,22],[3221,29,3221,30],[3222,4,3222,5],[3222,7,3222,8],[3222,15,3222,16],[3222,18,3222,19],[3222,26,3222,27],[3222,33,3222,35],[3222,39,3222,41],[3213,7,3213,8],[3213,10,3213,11],[3213,18,3213,19],[3214,4,3214,5],[3214,7,3214,8],[3214,15,3214,16],[3214,22,3214,24],[3214,28,3214,30],[3215,3,3215,5],[3216,4,3216,5],[3216,7,3216,8],[3216,10,3216,11],[3216,16,3216,17],[3216,19,3216,20],[3216,24,3216,26],[3216,28,3216,29],[3216,31,3216,33],[3205,7,3205,8],[3206,4,3206,5],[3206,11,3206,13],[3206,17,3206,19],[3207,3,3207,5],[3208,4,3208,5],[3208,7,3208,8],[3208,12,3208,14],[3208,16,3208,17],[3208,19,3208,21],[3208,25,3208,27],[3208,29,3208,31],[3209,4,3209,6],[3210,7,3210,9],[3210,11,3210,12],[3210,14,3210,16],[3211,3,3211,5],[3211,12,3211,14],[3193,6,3193,7],[3193,9,3193,10],[3193,14,3193,15],[3193,17,3193,18],[3193,22,3193,23],[3193,25,3193,26],[3193,34,3193,36],[3194,14,3194,16],[3194,20,3194,22],[3196,4,3196,6],[3197,4,3197,6],[3198,4,3198,6],[3199,4,3199,6]],"bounds":{"rows_first":1000,"rows_last":250,"rows_between":1000,"halvings":1},"merged_total":11246,"flags":["merged_cut"]}
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI (6 adet tekil yüklü)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not: Kirişin eğilme dayanımı hesapları için \"celik2016_tali_kiris_hesapları\" excel dosyasında \"profil_kiris_hesabi\" sayfasını kullanabilirsiniz."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"çeşitli I profiller"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,20,null,"KN",null,null,20,null,"KN",null,null,20,null,"KN",null,null,20,null,"KN",null,null,20,null,"KN",null,null,20,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"profil","A(cm²)","h (mm.)","b (mm.)","s (mm.)","t (mm.)","Jx (cm4.)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I profiller","normal I 80",7.57,80,42,3.9,5.9,77.8]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK41","v":1.1569488132086301},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 100",10.6,100,50,4.5,6.8,171]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"+BV33","v":424.96153846153857},null,null,"KNm",null,"(max moment)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 120",14.2,120,58,5.0999999999999996,7.7,328]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O5,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(U12,BD12)","v":143},null,null,"KN",null,"(max kesme kuvveti)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 140",18.2,140,66,5.7,8.6,573]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 160",22.8,160,74,6.3,9.5,935]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O5,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 180",27.9,180,82,6.9,10.4,1450]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E22","v":133},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E25","v":143},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 200",33.4,200,90,7.5,11.3,2140]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,"m","m",null,2.5,null,"m",null,null,1.5,null,"m",null,null,1,null,"m",null,null,3.5,null,"m",null,null,1.5,null,"m",null,null,0.5,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 220",39.5,220,98,8.1,12.2,3060]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O5,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 240",46.1,240,106,8.6999999999999993,13.1,4250]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",{"$f":"+W13+AB13+AG13+AL13+AQ13+AV13+BA13","v":12},null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 260",53.3,260,113,9.4,14.1,5740]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 280",61,280,119,10.1,15.2,7590]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O5,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O5,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 300",69,300,125,10.8,16.2,9800]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 320",77.7,320,131,11.5,17.3,12510]
[null,null,"MESNET TEPKİLERİ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 340",86.7,340,137,12.2,18.3,15700]
[null,null,"MB = 0    (sağ mesnette moment sıfır şartından)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 360",97,360,143,13,19.5,19610]
[null,null,"A","*",{"$f":"+AL15","v":12},null,"-",{"$f":"+Z5","v":20},null,"*",{"$f":"+AB13+AG13+AL13+AQ13+AV13+BA13","v":10.5},null,"-",{"$f":"+AE5","v":20},null,"*",{"$f":"+AG13+AL13+AQ13+AV13+BA13","v":8},null,"-",{"$f":"+AJ5","v":20},null,"*",{"$f":"+AL13+AQ13+AV13+BA13","v":6.5},null,"-",{"$f":"+AO5","v":20},null,"*",{"$f":"+AQ13+AV13+BA13","v":5.5},null,"-",{"$f":"+AT5","v":20},null,"*",{"$f":"+AV13+BA13","v":2},null,"-",{"$f":"+AY5","v":20},null,"*",{"$f":"+BA13","v":0.5},null,"-",{"$f":"+AL6","v":13},null,"*",{"$f":"+AL15","v":12},null,"*",{"$f":"+AL15/2","v":6},null,"=",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 380",107,380,149,13.7,20.5,24010]
[null,null,"A =",null,{"$f":"(H21*K21+N21*Q21+T21*W21+Z21*AC21+AF21*AI21+AL21*AO21+AR21*AU21*AX21)/E21","v":133},null,"KN",null,"(sol mesnet tepkisi)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 400",118,400,155,14.4,21.6,29210]
[null,null,"Fy = 0    (düşey denge denklemi yazılırsa)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 425",132,425,163,15.3,23,36970]
[null,null,"A","+","B","-",{"$f":"+Z5","v":20},null,"-",{"$f":"+AE5","v":20},null,"-",{"$f":"+AJ5","v":20},null,"*",{"$f":"+AO5","v":20},null,"-",{"$f":"+AT5","v":20},null,"-",{"$f":"+AY5","v":20},null,"-",{"$f":"+AL6","v":13},null,"*",{"$f":"+AL15","v":12},null,"=",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 450",147,450,170,16.2,24.3,45850]
[null,null,"B =",null,{"$f":"(G24+J24+M24+P24+S24+V24+Y24*AB24-E22)","v":143},null,"KN",null,"(sağ mesnet tepkisi)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 475",163,475,178,17.100000000000001,25.6,46480]
[null,null,"ARA KESİT TESİRLERİ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 500",179,500,185,18,27,68740]
[null,null,"Mx =",null,{"$f":"+U12","v":133},null," *  x  -",null,{"$f":"+Z5","v":20},null,"*(  x -",null,{"$f":"+W13","v":1.5},null,")-",{"$f":"+AE5","v":20},null,"*(  x -",null,{"$f":"+W13+AB13","v":4},null,")-",{"$f":"+AJ5","v":20},null,"*(  x -",null,{"$f":"+W13+AB13+AG13","v":5.5},null,")-",{"$f":"+AO5","v":20},null,"*(  x -",null,{"$f":"+W13+AB13+AG13+AL13","v":6.5},null,")-",{"$f":"+AT5","v":20},null,"*(  x -",null,{"$f":"+W13+AB13+AG13+AL13+AQ13","v":10},null,")-",{"$f":"+AY5","v":20},null,"*(  x -",null,{"$f":"+W13+AB13+AG13+AL13+AQ13+AV13","v":11.5},null,")-",{"$f":"+AL6","v":13},null,"*","x²"," /",2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 550",212,550,200,19,30,99180]
[null,null,"x=",{"$f":"+AL15/2","v":6},null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D28<=AL15,\"\",\"azalt.\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"normal I 600",254,600,215,21.6,32.4,139000]
[null,null,"Mx =",null,{"$f":"+E27","v":133},null,"*",{"$f":"+D28","v":6},null,"-",{"$f":"IF((N29-Q29)<=0,0,+I27)","v":20},null,"*(",{"$f":"+H29","v":6},null,"-",{"$f":"+M27","v":1.5},null,")-",{"$f":"IF((W29-Z29)<=0,0,+P27)","v":20},null,"*(",{"$f":"+N29","v":6},null,"-",{"$f":"+T27","v":4},null,")-",{"$f":"IF((AF29-AI29)<=0,0,+W27)","v":20},null,"*(",{"$f":"+W29","v":6},null,"-",{"$f":"+AA27","v":5.5},null,")-",{"$f":"IF((AO29-AR29)<=0,0,+AD27)","v":0},null,"*(",{"$f":"+AF29","v":6},null,"-",{"$f":"+AH27","v":6.5},null,")-",{"$f":"IF((AX29-BA29)<=0,0,+AK27)","v":0},null,"*(",{"$f":"+AO29","v":6},null,"-",{"$f":"+AO27","v":10},null,")-",{"$f":"IF((BG29-BJ29)<=0,0,+AR27)","v":0},null,"*(",{"$f":"+AX29","v":6},null,"-",{"$f":"+AV27","v":11.5},null,")-",{"$f":"+AY27","v":13},null,"*",{"$f":"+BG29","v":6},null,"²/",2,"=",{"$f":"E29*H29-K29*(N29-Q29)-T29*(W29-Z29)-AC29*(AF29-AI29)-AL29*(AO29-AR29)-AU29*(AX29-BA29)-BD29*(BG29-BJ29)-BM29*BP29^2/BS29","v":424},null,null,"KNm",null,null,null,null,null,null,null,"IPE profiller","IPE 80",7.64,80,46,3.8,5.2,80.099999999999994]
[null,null,"Vx =",null,{"$f":"+E29","v":133},null,"-",{"$f":"+K29","v":20},null,"-",{"$f":"+T29","v":20},null,"-",{"$f":"+AC29","v":20},null,"-",{"$f":"+AL29","v":0},null,"-",{"$f":"+AU29","v":0},null,"-",{"$f":"+BD29","v":0},null,"-",{"$f":"+BM29","v":13},null,"*",{"$f":"+BP29","v":6},null,"=",{"$f":"+E30-H30-K30-N30-Q30-T30-W30-Z30*AC30","v":-5},null,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 100",10.3,100,55,4.0999999999999996,5.7,171]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 120",13.2,120,64,4.4000000000000004,6.3,318]
[null,null,"x=",{"$f":"(E30-H30-K30-N30-Q30-T30-W30)/Z30","v":5.615384615384615},null,null,"m. ' deki max moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 140",16.399999999999999,140,73,4.7,6.9,541]
[null,null,"Mmax =",null,null,{"$f":"+E27","v":133},null,"*",{"$f":"+D32","v":5.615384615384615},null,"-",{"$f":"IF((O33-R33)<=0,0,+I27)","v":20},null,"*(",{"$f":"+I33","v":5.615384615384615},null,"-",{"$f":"+M27","v":1.5},null,")-",{"$f":"IF((X33-AA33)<=0,0,+P27)","v":20},null,"*(",{"$f":"+O33","v":5.615384615384615},null,"-",{"$f":"+T27","v":4},null,")-",{"$f":"IF((AG33-AJ33)<=0,0,+W27)","v":20},null,"*(",{"$f":"+X33","v":5.615384615384615},null,"-",{"$f":"+AA27","v":5.5},null,")-",{"$f":"IF((AP33-AS33)<=0,0,+AD27)","v":0},null,"*(",{"$f":"+AG33","v":5.615384615384615},null,"-",{"$f":"+AH27","v":6.5},null,")-",{"$f":"IF((AY33-BB33)<=0,0,+AK27)","v":0},null,"*(",{"$f":"+AP33","v":5.615384615384615},null,"-",{"$f":"+AO27","v":10},null,")-",{"$f":"IF((BH33-BK33)<=0,0,+AR27)","v":0},null,"*(",{"$f":"+AY33","v":5.615384615384615},null,"-",{"$f":"+AV27","v":11.5},null,")-",{"$f":"+AY27","v":13},null,"*",{"$f":"+BH33","v":5.615384615384615},null,"²/",2,"=",{"$f":"F33*I33-L33*(O33-R33)-U33*(X33-AA33)-AD33*(AG33-AJ33)-AM33*(AP33-AS33)-AV33*(AY33-BB33)-BE33*(BH33-BK33)-BN33*BQ33^2/BT33","v":424.96153846153857},null,null,"KNm",null,null,null,null,null,null,null,"IPE 160",20.100000000000001,160,82,5,7.4,869]
[null,null,"L / 2 =",null,{"$f":"+AL15/2","v":6},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 180",23.9,180,91,5.3,8,1320]
[null,null,"MB =",null,{"$f":"+E29","v":133},null,"*",{"$f":"+E34","v":6},null,"-",{"$f":"IF((N35-Q35)<=0,0,+I27)","v":20},null,"*(",{"$f":"+H35","v":6},null,"-",{"$f":"+M27","v":1.5},null,")-",{"$f":"IF((W35-Z35)<=0,0,+P27)","v":20},null,"*(",{"$f":"+N35","v":6},null,"-",{"$f":"+T27","v":4},null,")-",{"$f":"IF((AF35-AI35)<=0,0,+W27)","v":20},null,"*(",{"$f":"+W35","v":6},null,"-",{"$f":"+AA27","v":5.5},null,")-",{"$f":"IF((AO35-AR35)<=0,0,+AD27)","v":0},null,"*(",{"$f":"+AF35","v":6},null,"-",{"$f":"+AH27","v":6.5},null,")-",{"$f":"IF((AX35-BA35)<=0,0,+AK27)","v":0},null,"*(",{"$f":"+AO35","v":6},null,"-",{"$f":"+AO27","v":10},null,")-",{"$f":"IF((BG35-BJ35)<=0,0,+AR27)","v":0},null,"*(",{"$f":"+AX35","v":6},null,"-",{"$f":"+AV27","v":11.5},null,")-",{"$f":"+AY27","v":13},null,"*",{"$f":"+BG35","v":6},null,"²/",2,"=",{"$f":"E35*H35-K35*(N35-Q35)-T35*(W35-Z35)-AC35*(AF35-AI35)-AL35*(AO35-AR35)-AU35*(AX35-BA35)-BD35*(BG35-BJ35)-BM35*BP35^2/BS35","v":424},null,null,"KNm",null,null,null,null,null,null,null,null,"IPE 200",28.5,200,100,5.6,8.5,1940]
[null,null,"L / 4 =",null,{"$f":"+AL15/4","v":3},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 220",33.4,220,110,5.9,9.1999999999999993,2770]
[null,null,"MA =",null,{"$f":"+E35","v":133},null,"*",{"$f":"+E36","v":3},null,"-",{"$f":"IF((N37-Q37)<=0,0,+I27)","v":20},null,"*(",{"$f":"+H37","v":3},null,"-",{"$f":"+Q35","v":1.5},null,")-",{"$f":"IF((W37-Z37)<=0,0,+P27)","v":0},null,"*(",{"$f":"+N37","v":3},null,"-",{"$f":"+Z35","v":4},null,")-",{"$f":"IF((AF37-AI37)<=0,0,+W27)","v":0},null,"*(",{"$f":"+W37","v":3},null,"-",{"$f":"+AI35","v":5.5},null,")-",{"$f":"IF((AO37-AR37)<=0,0,+AD27)","v":0},null,"*(",{"$f":"+AF37","v":3},null,"-",{"$f":"+AR35","v":6.5},null,")-",{"$f":"IF((AX37-BA37)<=0,0,+AK27)","v":0},null,"*(",{"$f":"+AO37","v":3},null,"-",{"$f":"+BA35","v":10},null,")-",{"$f":"IF((BG37-BJ37)<=0,0,+AR27)","v":0},null,"*(",{"$f":"+AX37","v":3},null,"-",{"$f":"+BJ35","v":11.5},null,")-",{"$f":"+BM35","v":13},null,"*",{"$f":"+BG37","v":3},null,"²/",2,"=",{"$f":"E37*H37-K37*(N37-Q37)-T37*(W37-Z37)-AC37*(AF37-AI37)-AL37*(AO37-AR37)-AU37*(AX37-BA37)-BD37*(BG37-BJ37)-BM37*BP37^2/BS37","v":310.5},null,null,"KNm",null,null,null,null,null,null,null,null,"IPE 240",39.1,240,120,6.2,9.8000000000000007,3890]
[null,null,"3 * L / 4 =",null,null,{"$f":"3*AL15/4","v":9},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 270",45.9,270,135,6.6,10.199999999999999,5790]
[null,null,"MC =",null,null,{"$f":"+E37","v":133},null,"*",{"$f":"+F38","v":9},null,"-",{"$f":"IF((O39-R39)<=0,0,+I27)","v":20},null,"*(",{"$f":"+I39","v":9},null,"-",{"$f":"+Q37","v":1.5},null,")-",{"$f":"IF((X39-AA39)<=0,0,+P27)","v":20},null,"*(",{"$f":"+O39","v":9},null,"-",{"$f":"+Z37","v":4},null,")-",{"$f":"IF((AG39-AJ39)<=0,0,+W27)","v":20},null,"*(",{"$f":"+X39","v":9},null,"-",{"$f":"+AI37","v":5.5},null,")-",{"$f":"IF((AP39-AS39)<=0,0,+AD27)","v":20},null,"*(",{"$f":"+AG39","v":9},null,"-",{"$f":"+AR37","v":6.5},null,")-",{"$f":"IF((AY39-BB39)<=0,0,+AK27)","v":0},null,"*(",{"$f":"+AP39","v":9},null,"-",{"$f":"+BA37","v":10},null,")-",{"$f":"IF((BH39-BK39)<=0,0,+AR27)","v":0},null,"*(",{"$f":"+AY39","v":9},null,"-",{"$f":"+BJ37","v":11.5},null,")-",{"$f":"+BM37","v":13},null,"*",{"$f":"+BH39","v":9},null,"²/",2,"=",{"$f":"F39*I39-L39*(O39-R39)-U39*(X39-AA39)-AD39*(AG39-AJ39)-AM39*(AP39-AS39)-AV39*(AY39-BB39)-BE39*(BH39-BK39)-BN39*BQ39^2/BT39","v":300.5},null,null,"KNm",null,null,null,null,null,null,null,"IPE 300",53.8,300,150,7.1,10.7,8360]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 330",62.6,330,160,7.5,11.5,11770]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(BV33)","v":424.96153846153857},null,null," /(",2.5,null,"*",{"$f":"+H41","v":424.96153846153857},null,null,"+",3,"*",{"$f":"ABS(BU37)","v":310.5},null,null,"+",4,"*",{"$f":"ABS(BU35)","v":424},null,null,"+",3,"*",{"$f":"ABS(BV39)","v":300.5},null,null,")=",{"$f":"E41*H41/(L41*O41+S41*U41+Y41*AA41+AE41*AG41)","v":1.1569488132086301},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 360",72.7,360,170,8,12.7,16270]
[null,null,"SEHİM HESABI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 400",84.5,400,180,8.6,13.5,23130]
[null,null,"E * I / 108 dy / dx =",null,null,null,null,null,{"$f":"+E27","v":133},null,"*  x²  /",null,2,"-",{"$f":"+I27","v":20},null,"*(  x -",null,{"$f":"+M27","v":1.5},null,")² / 2 -",null,{"$f":"+P27","v":20},null,"*(  x -",null,{"$f":"+T27","v":4},null,")² / 2 -",null,{"$f":"+W27","v":20},null,"*(  x -",null,{"$f":"+AA27","v":5.5},null,")² / 2 -",null,{"$f":"+AD27","v":20},null,"*(  x -",null,{"$f":"+AH27","v":6.5},null,")² / 2 -",null,{"$f":"+AK27","v":20},null,"*(  x -",null,{"$f":"+AO27","v":10},null,")² / 2 -",null,{"$f":"+AR27","v":20},null,"*(  x -",null,{"$f":"+AV27","v":11.5},null,")² / 2",null,"-",{"$f":"+AY27","v":13},null,"*","x3"," /",6,"+","C1",null,null,"(integral)",null,null,null,null,null,null,null,null,null,null,"IPE 450",98.8,450,190,9.4,14.6,33740]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+I43","v":133},null,"*  x3  /",null,6,"-",{"$f":"+O43","v":20},null,"*(  x -",null,{"$f":"+S43","v":1.5},null,")3 / 6 -",null,{"$f":"+W43","v":20},null,"*(  x -",null,{"$f":"+AA43","v":4},null,")3 / 6 -",null,{"$f":"+AE43","v":20},null,"*(  x -",null,{"$f":"+AI43","v":5.5},null,")3 / 6 -",null,{"$f":"+AM43","v":20},null,"*(  x -",null,{"$f":"+AQ43","v":6.5},null,")3 / 6 -",null,{"$f":"+AU43","v":20},null,"*(  x -",null,{"$f":"+AY43","v":10},null,")3 / 6 -",null,{"$f":"+BC43","v":20},null,"*(  x -",null,{"$f":"+BG43","v":11.5},null,")3 / 6",null,"-",{"$f":"+BL43","v":13},null,"*","x4"," /",24,null," + C1 * x + C2",null,null,null,null,null,"(integral)",null,null,null,null,null,null,null,null,"IPE 500",116,500,200,10.199999999999999,16,48200]
[null,null,"x = 0 ; y = 0 ; C2 = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 550",134,550,210,11.1,17.2,67120]
[null,null,"x=",{"$f":"+AL15","v":12},null,"m",";","y = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",156,600,220,12,19,92080]
[null,null,{"$f":"+H44","v":133},null,"*",{"$f":"+D46","v":12},null,"3/",6,"-",{"$f":"+N44","v":20},null,"*(",{"$f":"+D46","v":12},null,"-",{"$f":"+R44","v":1.5},null,")3/",6,"-",{"$f":"+V44","v":20},null,"*(",{"$f":"+N47","v":12},null,"-",{"$f":"+Z44","v":4},null,")3/",6,"-",{"$f":"+AD44","v":20},null,"*(",{"$f":"+Y47","v":12},null,"-",{"$f":"+AH44","v":5.5},null,")3/",6,"-",{"$f":"+AL44","v":20},null,"*(",{"$f":"+AJ47","v":12},null,"-",{"$f":"+AP44","v":6.5},null,")3/",6,"-",{"$f":"+AT44","v":20},null,"*(",{"$f":"+AU47","v":12},null,"-",{"$f":"+AX44","v":10},null,")3/",6,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) profiller","IPBL (HE-A) 100",21.2,96,100,5,8,349]
[null,null,null,"-",{"$f":"+BB44","v":20},null,"*(",{"$f":"+BF47","v":12},null,"-",{"$f":"+BF44","v":11.5},null,")3/",6,"-",{"$f":"+BK44","v":13},null,"*",{"$f":"+H48","v":12},null," 4/",24,null,"+",{"$f":"+BF47","v":12},null,"*","C1","=",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 120",25.3,114,120,5,8,606]
[null,null,"C1 =",null,{"$f":"-(C47*F47^3/I47-K47*(N47-Q47)^3/T47-V47*(Y47-AB47)^3/AE47-AG47*(AJ47-AM47)^3/AP47-AR47*(AU47-AX47)^3/BA47-BC47*(BF47-BI47)^3/BL47-E48*(H48-K48)^3/N48-P48*S48^4/V48)/Y48","v":-1667.458333333333},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 140",31.4,133,140,5.5,8.5,1030]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+H44","v":133},null,"*  x3  /",null,6,"-",{"$f":"+N44","v":20},null,"*(  x -",null,{"$f":"+R44","v":1.5},null,")3 / 6 -",null,{"$f":"+V44","v":20},null,"*(  x -",null,{"$f":"+Z44","v":4},null,")3 / 6 -",null,{"$f":"+AD44","v":20},null,"*(  x -",null,{"$f":"+AH44","v":5.5},null,")3 / 6 -",null,{"$f":"+AL44","v":20},null,"*(  x -",null,{"$f":"+AP44","v":6.5},null,")3 / 6 -",null,{"$f":"+AT44","v":20},null,"*(  x -",null,{"$f":"+AX44","v":10},null,")3 / 6 -",null,{"$f":"+BB44","v":20},null,"*(  x -",null,{"$f":"+BF44","v":11.5},null,")3 / 6",null,"-",{"$f":"+P48","v":13},null,"*","x4"," /",24,null,"+",{"$f":"+E49","v":-1667.458333333333},null,null,"*","x",null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 160",38.799999999999997,152,160,6,9,1670]
[null,null,"y = (",null,{"$f":"+H50","v":133},null,"*  x3  /",null,6,"-",{"$f":"+N50","v":20},null,"*(  x -",null,{"$f":"+R50","v":1.5},null,")3 / 6 -",null,{"$f":"+V50","v":20},null,"*(  x -",null,{"$f":"+Z50","v":4},null,")3 / 6 -",null,{"$f":"+AD50","v":20},null,"*(  x -",null,{"$f":"+AH50","v":5.5},null,")3 / 6 -",null,{"$f":"+AL50","v":20},null,"*(  x -",null,{"$f":"+AP50","v":6.5},null,")3 / 6 -",null,{"$f":"+AT50","v":20},null,"*(  x -",null,{"$f":"+AX50","v":10},null,")3 / 6 -",null,{"$f":"+BB50","v":20},null,"*(  x -",null,{"$f":"+BF50","v":11.5},null,")3 / 6",null,"-",{"$f":"+BK50","v":13},null,"*","x4"," /",24,null,"+",{"$f":"+BS50","v":-1667.458333333333},null,null,"*","x ) * 108 / ( E * I )",null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 180",45.3,171,180,6,9.5,2510]
[null,null,"x=",{"$f":"+AL15/2","v":6},null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D52<=AL15,\"\",\"azalt.\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 200",53.8,190,200,6.5,10,3690]
[null,null,"y = (",null,{"$f":"+E51","v":133},null,"*",{"$f":"+D52","v":6},null,"3/",6,"-",{"$f":"IF((P53-S53)<=0,0,+K51)","v":20},null,"*(",{"$f":"+D52","v":6},null,"-",{"$f":"+O51","v":1.5},null,")3/",6,"-",{"$f":"IF((AA53-AD53)<=0,0,+S51)","v":20},null,"*(",{"$f":"+P53","v":6},null,"-",{"$f":"+W51","v":4},null,")3/",6,"-",{"$f":"IF((AL53-AO53)<=0,0,+AA51)","v":20},null,"*(",{"$f":"+AA53","v":6},null,"-",{"$f":"+AE51","v":5.5},null,")3/",6,"-",{"$f":"IF((AW53-AZ53)<=0,0,+AI51)","v":0},null,"*(",{"$f":"+AL53","v":6},null,"-",{"$f":"+AM51","v":6.5},null,")3/",6,"-",{"$f":"IF((BH53-BK53)<=0,0,+AQ51)","v":0},null,"*(",{"$f":"+AW53","v":6},null,"-",{"$f":"+AU51","v":10},null,")3/",6,"-",{"$f":"IF((BS53-BV53)<=0,0,+AY51)","v":0},null,"*(",{"$f":"+BH53","v":6},null,"-",{"$f":"+BC51","v":11.5},null,")3/",6,"-",null,null,null,null,null,null,"IPBL (HE-A) 220",64.3,210,220,7,11,5410]
[null,null,null,"-",{"$f":"+BH51","v":13},null,"*",{"$f":"+BS53","v":6},null,"4/",24,null,"+",{"$f":"+BP51","v":-1667.458333333333},null,null,"*",{"$f":"+BH53","v":6},null,")* 108 / (",null,null,{"$f":"+Z18","v":200000},null,null,"*",{"$f":"+Z17","v":92080},null,null,")",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 240",76.8,230,240,7.5,12,7760]
[null,null,"y =",null,{"$f":"-(E53*H53^3/K53-M53*(P53-S53)^3/V53-X53*(AA53-AD53)^3/AG53-AI53*(AL53-AO53)^3/AR53-AT53*(AW53-AZ53)^3/BC53-BE53*(BH53-BK53)^3/BN53-BP53*(BS53-BV53)^3/BY53-E54*H54^4/K54+N54*R54)*100000000/(W54*AA54)","v":33.935617578916876},null,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 260",86.8,250,260,7.5,12.5,10450]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"+AL15*1000","v":12000},null,null," /",300,null,"=",{"$f":"+H56/L56","v":40},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 280",97.3,270,280,8,13,13670]
[null,null,"y=",{"$f":"+E55","v":33.935617578916876},null,null,"mm",null,{"$f":"IF(D57<M57,\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O56","v":40},null,null,"mm",null,{"$f":"IF(D57<M57,\"uygun.\",\"uygun değil.\")","v":"uygun."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 300",113,290,300,8.5,14,18260]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 320",124,310,300,9,15.5,22930]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 340",133,330,300,9.5,16.5,27690]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI (5 adet tekil yüklü)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 360",143,350,300,10,17.5,33090]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 400",159,390,300,11,19,45070]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 450",178,440,300,11.5,21,63720]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,20,null,"KN",null,null,20,null,"KN",null,null,20,null,"KN",null,null,20,null,"KN",null,null,20,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 500",198,490,300,12,23,86970]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 550",212,540,300,12.5,24,111900]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 600",226,590,300,13,25,141200]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK99","v":1.1372064276885043},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 650",242,640,300,13.5,26,175200]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O63,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"+BM91","v":460},null,null,"KNm",null,"(max moment)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 700",260,690,300,14.5,27,215300]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(U70,AY70)","v":160},null,null,"KN",null,"(max kesme kuvveti)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 800",286,790,300,15,28,303400]
[null,null,null,0,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O63,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 900",321,890,300,16,30,422100]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E80","v":160},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E83","v":160},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBL (HE-A) 1000",347,990,300,16.5,31,553800]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,"m",null,null,2.5,null,"m",null,null,1.5,null,"m",null,null,1.5,null,"m",null,null,2.5,null,"m",null,null,1.5,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) profiller","IPB (HE-B) 100",26,100,100,6,10,450]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O63,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 120",34,120,120,6.5,11,864]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",{"$f":"+W71+AB71+AG71+AL71+AQ71+AV71","v":11},null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 140",43,140,140,7,12,1510]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 160",54.3,160,160,8,13,2490]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O63,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O63,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 180",65.3,180,180,8.5,14,3830]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 200",78.099999999999994,200,200,9,15,5700]
[null,null,"MESNET TEPKİLERİ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 220",91,220,220,9.5,16,8090]
[null,null,"MB = 0    (sağ mesnette moment sıfır şartından)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 240",106,240,240,10,17,11260]
[null,null,"A","*",{"$f":"+AJ73","v":11},null,"-",{"$f":"+Z63","v":20},null,"*",{"$f":"+AB71+AG71+AL71+AQ71+AV71","v":9.5},null,"-",{"$f":"+AE63","v":20},null,"*",{"$f":"+AG71+AL71+AQ71+AV71","v":7},null,"-",{"$f":"+AJ63","v":20},null,"*",{"$f":"+AL71+AQ71+AV71","v":5.5},null,"-",{"$f":"+AO63","v":20},null,"*",{"$f":"+AQ71+AV71","v":4},null,"-",{"$f":"+AT63","v":20},null,"*",{"$f":"+AV71","v":1.5},null,"-",{"$f":"+AL64","v":20},null,"*",{"$f":"+AJ73","v":11},null,"*",{"$f":"+AJ73/2","v":5.5},null,"=",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 260",118,260,260,10,17.5,14920]
[null,null,"A =",null,{"$f":"(H79*K79+N79*Q79+T79*W79+Z79*AC79+AF79*AI79+AL79*AO79*AR79)/E79","v":160},null,"KN",null,"(sol mesnet tepkisi)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 280",131,280,280,10.5,18,19270]
[null,null,"Fy = 0    (düşey denge denklemi yazılırsa)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 300",149,300,300,11,19,25170]
[null,null,"A","+","B","-",{"$f":"+Z63","v":20},null,"-",{"$f":"+AE63","v":20},null,"-",{"$f":"+AJ63","v":20},null,"*",{"$f":"+AO63","v":20},null,"-",{"$f":"+AT63","v":20},null,"-",{"$f":"+AL64","v":20},null,"*",{"$f":"+AJ73","v":11},null,"=",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 320",161,320,300,11.5,20.5,30820]
[null,null,"B =",null,{"$f":"(G82+J82+M82+P82+S82+V82*Y82-E80)","v":160},null,"KN",null,"(sağ mesnet tepkisi)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 340",171,340,300,12,21.5,36660]
[null,null,"ARA KESİT TESİRLERİ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 360",181,360,300,12.5,22.5,43190]
[null,null,"Mx =",null,{"$f":"+U70","v":160},null," *  x  -",null,{"$f":"+Z63","v":20},null,"*(  x -",null,{"$f":"+W71","v":1.5},null,")-",{"$f":"+AE63","v":20},null,"*(  x -",null,{"$f":"+W71+AB71","v":4},null,")-",{"$f":"+AJ63","v":20},null,"*(  x -",null,{"$f":"+W71+AB71+AG71","v":5.5},null,")-",{"$f":"+AO63","v":20},null,"*(  x -",null,{"$f":"+W71+AB71+AG71+AL71","v":7},null,")-",{"$f":"+AT63","v":20},null,"*(  x -",null,{"$f":"+W71+AB71+AG71+AL71+AQ71","v":9.5},null,")-",{"$f":"+AL64","v":20},null,"*","x²"," /",2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 400",198,400,300,13.5,24,57680]
[null,null,"x=",{"$f":"+AJ73/2","v":5.5},null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D86<=AJ73,\"\",\"azalt.\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 450",218,450,300,14,26,79890]
[null,null,"Mx =",null,{"$f":"+E85","v":160},null,"*",{"$f":"+D86","v":5.5},null,"-",{"$f":"IF((N87-Q87)<=0,0,+I85)","v":20},null,"*(",{"$f":"+H87","v":5.5},null,"-",{"$f":"+M85","v":1.5},null,")-",{"$f":"IF((W87-Z87)<=0,0,+P85)","v":20},null,"*(",{"$f":"+N87","v":5.5},null,"-",{"$f":"+T85","v":4},null,")-",{"$f":"IF((AF87-AI87)<=0,0,+W85)","v":0},null,"*(",{"$f":"+W87","v":5.5},null,"-",{"$f":"+AA85","v":5.5},null,")-",{"$f":"IF((AO87-AR87)<=0,0,+AD85)","v":0},null,"*(",{"$f":"+AF87","v":5.5},null,"-",{"$f":"+AH85","v":7},null,")-",{"$f":"IF((AX87-BA87)<=0,0,+AK85)","v":0},null,"*(",{"$f":"+AO87","v":5.5},null,"-",{"$f":"+AO85","v":9.5},null,")-",{"$f":"+AR85","v":20},null,"*",{"$f":"+AX87","v":5.5},null,"²/",2,"=",{"$f":"E87*H87-K87*(N87-Q87)-T87*(W87-Z87)-AC87*(AF87-AI87)-AL87*(AO87-AR87)-AU87*(AX87-BA87)-BD87*BG87^2/BJ87","v":467.5},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 500",239,500,300,14.5,28,107200]
[null,null,"Vx =",null,{"$f":"+E87","v":160},null,"-",{"$f":"+K87","v":20},null,"-",{"$f":"+T87","v":20},null,"-",{"$f":"+AC87","v":0},null,"-",{"$f":"+AL87","v":0},null,"-",{"$f":"+AU87","v":0},null,"-",{"$f":"+BD87","v":20},null,"*",{"$f":"+BG87","v":5.5},null,"=",{"$f":"+E88-H88-K88-N88-Q88-T88-W88*Z88","v":10},null,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 550",254,550,300,15,29,136700]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 600",270,600,300,15.5,30,171000]
[null,null,"x=",{"$f":"(E88-H88-K88-N88-Q88-T88)/W88","v":6},null,null,"m. ' deki max moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 650",286,650,300,16,31,210600]
[null,null,"Mmax =",null,null,{"$f":"+E85","v":160},null,"*",{"$f":"+D90","v":6},null,"-",{"$f":"IF((O91-R91)<=0,0,+I85)","v":20},null,"*(",{"$f":"+I91","v":6},null,"-",{"$f":"+M85","v":1.5},null,")-",{"$f":"IF((X91-AA91)<=0,0,+P85)","v":20},null,"*(",{"$f":"+O91","v":6},null,"-",{"$f":"+T85","v":4},null,")-",{"$f":"IF((AG91-AJ91)<=0,0,+W85)","v":20},null,"*(",{"$f":"+X91","v":6},null,"-",{"$f":"+AA85","v":5.5},null,")-",{"$f":"IF((AP91-AS91)<=0,0,+AD85)","v":0},null,"*(",{"$f":"+AG91","v":6},null,"-",{"$f":"+AH85","v":7},null,")-",{"$f":"IF((AY91-BB91)<=0,0,+AK85)","v":0},null,"*(",{"$f":"+AP91","v":6},null,"-",{"$f":"+AO85","v":9.5},null,")-",{"$f":"+AR85","v":20},null,"*",{"$f":"+AY91","v":6},null,"²/",2,"=",{"$f":"F91*I91-L91*(O91-R91)-U91*(X91-AA91)-AD91*(AG91-AJ91)-AM91*(AP91-AS91)-AV91*(AY91-BB91)-BE91*BH91^2/BK91","v":460},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 700",306,700,300,17,32,256900]
[null,null,"L / 2 =",null,{"$f":"+AJ73/2","v":5.5},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 800",334,800,300,17.5,33,359100]
[null,null,"MB =",null,{"$f":"+E85","v":160},null,"*",{"$f":"+E92","v":5.5},null,"-",{"$f":"IF((N93-Q93)<=0,0,+I85)","v":20},null,"*(",{"$f":"+H93","v":5.5},null,"-",{"$f":"+M85","v":1.5},null,")-",{"$f":"IF((W93-Z93)<=0,0,+P85)","v":20},null,"*(",{"$f":"+N93","v":5.5},null,"-",{"$f":"+T85","v":4},null,")-",{"$f":"IF((AF93-AI93)<=0,0,+W85)","v":0},null,"*(",{"$f":"+W93","v":5.5},null,"-",{"$f":"+AA85","v":5.5},null,")-",{"$f":"IF((AO93-AR93)<=0,0,+AD85)","v":0},null,"*(",{"$f":"+AF93","v":5.5},null,"-",{"$f":"+AH85","v":7},null,")-",{"$f":"IF((AX93-BA93)<=0,0,+AK85)","v":0},null,"*(",{"$f":"+AO93","v":5.5},null,"-",{"$f":"+AO85","v":9.5},null,")-",{"$f":"+AR85","v":20},null,"*",{"$f":"+AX93","v":5.5},null,"²/",2,"=",{"$f":"E93*H93-K93*(N93-Q93)-T93*(W93-Z93)-AC93*(AF93-AI93)-AL93*(AO93-AR93)-AU93*(AX93-BA93)-BD93*BG93^2/BJ93","v":467.5},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 900",371,900,300,18.5,35,494100]
[null,null,"L / 4 =",null,{"$f":"+AJ73/4","v":2.75},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPB (HE-B) 1000",400,1000,300,19,36,644700]
[null,null,"MA =",null,{"$f":"+E93","v":160},null,"*",{"$f":"+E94","v":2.75},null,"-",{"$f":"IF((N95-Q95)<=0,0,+I85)","v":20},null,"*(",{"$f":"+H95","v":2.75},null,"-",{"$f":"+Q93","v":1.5},null,")-",{"$f":"IF((W95-Z95)<=0,0,+P85)","v":0},null,"*(",{"$f":"+N95","v":2.75},null,"-",{"$f":"+Z93","v":4},null,")-",{"$f":"IF((AF95-AI95)<=0,0,+W85)","v":0},null,"*(",{"$f":"+W95","v":2.75},null,"-",{"$f":"+AI93","v":5.5},null,")-",{"$f":"IF((AO95-AR95)<=0,0,+AD85)","v":0},null,"*(",{"$f":"+AF95","v":2.75},null,"-",{"$f":"+AR93","v":7},null,")-",{"$f":"IF((AX95-BA95)<=0,0,+AK85)","v":0},null,"*(",{"$f":"+AO95","v":2.75},null,"-",{"$f":"+BA93","v":9.5},null,")-",{"$f":"+AR85","v":20},null,"*",{"$f":"+AX95","v":2.75},null,"²/",2,"=",{"$f":"E95*H95-K95*(N95-Q95)-T95*(W95-Z95)-AC95*(AF95-AI95)-AL95*(AO95-AR95)-AU95*(AX95-BA95)-BD95*BG95^2/BJ95","v":339.375},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) profiller","IPBv (HE-M) 100",53.2,120,106,12,20,1140]
[null,null,"3 * L / 4 =",null,null,{"$f":"3*AJ73/4","v":8.25},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 120",66.400000000000006,140,126,12.5,21,2020]
[null,null,"MC =",null,{"$f":"+E95","v":160},null,"*",{"$f":"+F96","v":8.25},null,"-",{"$f":"IF((N97-Q97)<=0,0,+I85)","v":20},null,"*(",{"$f":"+H97","v":8.25},null,"-",{"$f":"+Q95","v":1.5},null,")-",{"$f":"IF((W97-Z97)<=0,0,+P85)","v":20},null,"*(",{"$f":"+N97","v":8.25},null,"-",{"$f":"+Z95","v":4},null,")-",{"$f":"IF((AF97-AI97)<=0,0,+W85)","v":20},null,"*(",{"$f":"+W97","v":8.25},null,"-",{"$f":"+AI95","v":5.5},null,")-",{"$f":"IF((AO97-AR97)<=0,0,+AD85)","v":20},null,"*(",{"$f":"+AF97","v":8.25},null,"-",{"$f":"+AR95","v":7},null,")-",{"$f":"IF((AX97-BA97)<=0,0,+AK85)","v":0},null,"*(",{"$f":"+AO97","v":8.25},null,"-",{"$f":"+BA95","v":9.5},null,")-",{"$f":"+BD95","v":20},null,"*",{"$f":"+AX97","v":8.25},null,"²/",2,"=",{"$f":"E97*H97-K97*(N97-Q97)-T97*(W97-Z97)-AC97*(AF97-AI97)-AL97*(AO97-AR97)-AU97*(AX97-BA97)-BD97*BG97^2/BJ97","v":339.375},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 140",80.599999999999994,160,146,13,22,3290]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 160",97.1,180,166,14,23,5100]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(BM91)","v":460},null,null," /(",2.5,null,"*",{"$f":"+H99","v":460},null,null,"+",3,"*",{"$f":"ABS(BL95)","v":339.375},null,null,"+",4,"*",{"$f":"ABS(BL93)","v":467.5},null,null,"+",3,"*",{"$f":"ABS(BL97)","v":339.375},null,null,")=",{"$f":"E99*H99/(L99*O99+S99*U99+Y99*AA99+AE99*AG99)","v":1.1372064276885043},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 180",113,200,186,14.5,24,7480]
[null,null,"SEHİM HESABI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 200",131,220,206,15,25,10640]
[null,null,"E * I / 108 dy / dx =",null,null,null,null,null,{"$f":"+E85","v":160},null,"*  x²  /",null,2,"-",{"$f":"+I85","v":20},null,"*(  x -",null,{"$f":"+M85","v":1.5},null,")² / 2 -",null,{"$f":"+P85","v":20},null,"*(  x -",null,{"$f":"+T85","v":4},null,")² / 2 -",null,{"$f":"+W85","v":20},null,"*(  x -",null,{"$f":"+AA85","v":5.5},null,")² / 2 -",null,{"$f":"+AD85","v":20},null,"*(  x -",null,{"$f":"+AH85","v":7},null,")² / 2 -",null,{"$f":"+AK85","v":20},null,"*(  x -",null,{"$f":"+AO85","v":9.5},null,")² / 2",null,"-",{"$f":"+AR85","v":20},null,"*","x3"," /",6,"+","C1",null,null,"(integral)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 220",149,240,226,15.5,26,14600]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+I101","v":160},null,"*  x3  /",null,6,"-",{"$f":"+O101","v":20},null,"*(  x -",null,{"$f":"+S101","v":1.5},null,")3 / 6 -",null,{"$f":"+W101","v":20},null,"*(  x -",null,{"$f":"+AA101","v":4},null,")3 / 6 -",null,{"$f":"+AE101","v":20},null,"*(  x -",null,{"$f":"+AI101","v":5.5},null,")3 / 6 -",null,{"$f":"+AM101","v":20},null,"*(  x -",null,{"$f":"+AQ101","v":7},null,")3 / 6 -",null,{"$f":"+AU101","v":20},null,"*(  x -",null,{"$f":"+AY101","v":9.5},null,")3 / 6",null,"-",{"$f":"+BD101","v":20},null,"*","x4"," /",24,null," + C1 * x + C2",null,null,null,null,null,"(integral)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 240",200,270,248,18,32,24290]
[null,null,"x = 0 ; y = 0 ; C2 = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 260",220,290,268,18,32.5,31310]
[null,null,"x=",{"$f":"+AJ73","v":11},null,"m",";","y = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 280",240,310,288,18.5,33,39550]
[null,null,{"$f":"+H102","v":160},null,"*",{"$f":"+D104","v":11},null,"3/",6,"-",{"$f":"+N102","v":20},null,"*(",{"$f":"+D104","v":11},null,"-",{"$f":"+R102","v":1.5},null,")3/",6,"-",{"$f":"+V102","v":20},null,"*(",{"$f":"+N105","v":11},null,"-",{"$f":"+Z102","v":4},null,")3/",6,"-",{"$f":"+AD102","v":20},null,"*(",{"$f":"+Y105","v":11},null,"-",{"$f":"+AH102","v":5.5},null,")3/",6,"-",{"$f":"+AL102","v":20},null,"*(",{"$f":"+AJ105","v":11},null,"-",{"$f":"+AP102","v":7},null,")3/",6,"-",{"$f":"+AT102","v":20},null,"*(",{"$f":"+AU105","v":11},null,"-",{"$f":"+AX102","v":9.5},null,")3/",6,"-",{"$f":"+BC102","v":20},null,"*",{"$f":"+BF105","v":11},null," 4/",24,null,"+",{"$f":"+BF105","v":11},null,"*","C1","=",0,null,null,null,null,"IPBv (HE-M) 300",303,340,310,21,39,59200]
[null,null,"C1 =",null,{"$f":"-(C105*F105^3/I105-K105*(N105-Q105)^3/T105-V105*(Y105-AB105)^3/AE105-AG105*(AJ105-AM105)^3/AP105-AR105*(AU105-AX105)^3/BA105-BC105*(BF105-BI105)^3/BL105-BN105*BQ105^4/BT105)/BW105","v":-1682.916666666667},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 320/305",225,320,305,16,29,40950]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+H102","v":160},null,"*  x3  /",null,6,"-",{"$f":"+N102","v":20},null,"*(  x -",null,{"$f":"+R102","v":1.5},null,")3 / 6 -",null,{"$f":"+V102","v":20},null,"*(  x -",null,{"$f":"+Z102","v":4},null,")3 / 6 -",null,{"$f":"+AD102","v":20},null,"*(  x -",null,{"$f":"+AH102","v":5.5},null,")3 / 6 -",null,{"$f":"+AL102","v":20},null,"*(  x -",null,{"$f":"+AP102","v":7},null,")3 / 6 -",null,{"$f":"+AT102","v":20},null,"*(  x -",null,{"$f":"+AX102","v":9.5},null,")3 / 6",null,"-",{"$f":"+BN105","v":20},null,"*","x4"," /",24,null,"+",{"$f":"+E106","v":-1682.916666666667},null,null,"*","x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 320",312,359,309,21,40,68130]
[null,null,"y = (",null,{"$f":"+H107","v":160},null,"*  x3  /",null,6,"-",{"$f":"+N107","v":20},null,"*(  x -",null,{"$f":"+R107","v":1.5},null,")3 / 6 -",null,{"$f":"+V107","v":20},null,"*(  x -",null,{"$f":"+Z107","v":4},null,")3 / 6 -",null,{"$f":"+AD107","v":20},null,"*(  x -",null,{"$f":"+AH107","v":5.5},null,")3 / 6 -",null,{"$f":"+AL107","v":20},null,"*(  x -",null,{"$f":"+AP107","v":7},null,")3 / 6 -",null,{"$f":"+AT107","v":20},null,"*(  x -",null,{"$f":"+AX107","v":9.5},null,")3 / 6",null,"-",{"$f":"+BC107","v":20},null,"*","x4"," /",24,null,"+",{"$f":"+BK107","v":-1682.916666666667},null,null,"*","x ) * 108 / ( E * I )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 340",316,377,309,21,40,76770]
[null,null,"x=",{"$f":"+AJ73/2","v":5.5},null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D109<=AJ73,\"\",\"azalt.\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 360",319,395,308,21,40,84870]
[null,null,"y = (",null,{"$f":"+E108","v":160},null,"*",{"$f":"+D109","v":5.5},null,"3/",6,"-",{"$f":"IF((P110-S110)<=0,0,+K108)","v":20},null,"*(",{"$f":"+D109","v":5.5},null,"-",{"$f":"+O108","v":1.5},null,")3/",6,"-",{"$f":"IF((AA110-AD110)<=0,0,+S108)","v":20},null,"*(",{"$f":"+P110","v":5.5},null,"-",{"$f":"+W108","v":4},null,")3/",6,"-",{"$f":"IF((AL110-AO110)<=0,0,+AA108)","v":0},null,"*(",{"$f":"+AA110","v":5.5},null,"-",{"$f":"+AE108","v":5.5},null,")3/",6,"-",{"$f":"IF((AW110-AZ110)<=0,0,+AI108)","v":0},null,"*(",{"$f":"+AL110","v":5.5},null,"-",{"$f":"+AM108","v":7},null,")3/",6,"-",{"$f":"IF((BH110-BK110)<=0,0,+AQ108)","v":0},null,"*(",{"$f":"+AW110","v":5.5},null,"-",{"$f":"+AU108","v":9.5},null,")3/",6,"-",{"$f":"+AZ108","v":20},null,"*",{"$f":"+BH110","v":5.5},null,"4/",24,null,"+",null,null,null,null,null,null,null,null,"IPBv (HE-M) 400",326,432,307,21,40,104100]
[null,null,null,null,"+",{"$f":"+BH108","v":-1682.916666666667},null,null,"*",{"$f":"+BH110","v":5.5},null,")* 108 / (",null,null,{"$f":"+Z76","v":200000},null,null,"*",{"$f":"+Z75","v":92080},null,null,")",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 450",335,478,307,21,40,131500]
[null,null,"y =",null,{"$f":"-(E110*H110^3/K110-M110*(P110-S110)^3/V110-X110*(AA110-AD110)^3/AG110-AI110*(AL110-AO110)^3/AR110-AT110*(AW110-AZ110)^3/BC110-BE110*(BH110-BK110)^3/BN110-BP110*BS110^4/BV110+F111*J111)*100000000/(O111*S111)","v":31.529704695192592},null,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 500",344,524,306,21,40,161900]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"+AJ73*1000","v":11000},null,null," /",300,null,"=",{"$f":"+H113/L113","v":36.666666666666664},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 550",354,572,306,21,40,198000]
[null,null,"y=",{"$f":"+E112","v":31.529704695192592},null,null,"mm",null,{"$f":"IF(D114<M114,\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O113","v":36.666666666666664},null,null,"mm",null,{"$f":"IF(D114<M114,\"uygun.\",\"uygun değil.\")","v":"uygun."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 600",364,620,305,21,40,237400]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 650",374,668,305,21,40,281700]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 700",383,716,304,21,40,329300]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI (4 adet tekil yüklü)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 800",404,814,303,21,40,442600]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 900",424,910,302,21,40,570400]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPBv (HE-M) 1000",444,1008,302,21,40,772300]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,20,null,"KN",null,null,20,null,"KN",null,null,20,null,"KN",null,null,20,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"YENİ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,null,"KN/m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK156","v":1.1407755241105437}]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O120,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"+BD148","v":371.02977220299891},null,null,"KNm",null,"(max moment)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(U127,AT127)","v":169.85294117647058},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O120,$CG$6:$CG$120,0),0)","v":12}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E137","v":169.85294117647058},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E140","v":165.14705882352942},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,"m",null,null,1.5,null,"m",null,null,1.5,null,"m",null,null,2.5,null,"m",null,null,1.5,null,"m"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O120,$CG$6:$CG$120,0),0)","v":19}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",{"$f":"+W128+AB128+AG128+AL128+AQ128","v":8.5},null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O120,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O120,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,"MESNET TEPKİLERİ"]
[null,null,"MB = 0    (sağ mesnette moment sıfır şartından)"]
[null,null,"A","*",{"$f":"+AG130","v":8.5},null,"-",{"$f":"+Z120","v":20},null,"*",{"$f":"+AB128+AG128+AL128+AQ128","v":7},null,"-",{"$f":"+AE120","v":20},null,"*",{"$f":"+AG128+AL128+AQ128","v":5.5},null,"-",{"$f":"+AJ120","v":20},null,"*",{"$f":"+AL128+AQ128","v":4},null,"-",{"$f":"+AO120","v":20},null,"*",{"$f":"+AQ128","v":1.5},null,"-",{"$f":"+AG121","v":30},null,"*",{"$f":"+AG130","v":8.5},null,"*",{"$f":"+AG130/2","v":4.25},null,"=",0]
[null,null,"A =",null,{"$f":"(H136*K136+N136*Q136+T136*W136+Z136*AC136+AF136*AI136*AL136)/E136","v":169.85294117647058},null,"KN",null,"(sol mesnet tepkisi)"]
[null,null,"Fy = 0    (düşey denge denklemi yazılırsa)"]
[null,null,"A","+","B","-",{"$f":"+Z120","v":20},null,"-",{"$f":"+AE120","v":20},null,"-",{"$f":"+AJ120","v":20},null,"*",{"$f":"+AO120","v":20},null,"-",{"$f":"+AG121","v":30},null,"*",{"$f":"+AG130","v":8.5},null,"=",0]
[null,null,"B =",null,{"$f":"(G139+J139+M139+P139+S139*V139-E137)","v":165.14705882352942},null,"KN",null,"(sağ mesnet tepkisi)"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"Mx =",null,{"$f":"+U127","v":169.85294117647058},null," *  x  -",null,{"$f":"+Z120","v":20},null,"*(  x -",null,{"$f":"+W128","v":1.5},null,")-",{"$f":"+AE120","v":20},null,"*(  x -",null,{"$f":"+W128+AB128","v":3},null,")-",{"$f":"+AJ120","v":20},null,"*(  x -",null,{"$f":"+W128+AB128+AG128","v":4.5},null,")-",{"$f":"+AO120","v":20},null,"*(  x -",null,{"$f":"+W128+AB128+AG128+AL128","v":7},null,")-",{"$f":"+AG121","v":30},null,"*","x²"," /",2]
[null,null,"x=",{"$f":"+AG130/2","v":4.25},null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D143<=AG130,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+E142","v":169.85294117647058},null,"*",{"$f":"+D143","v":4.25},null,"-",{"$f":"IF((N144-Q144)<=0,0,+I142)","v":20},null,"*(",{"$f":"+H144","v":4.25},null,"-",{"$f":"+M142","v":1.5},null,")-",{"$f":"IF((W144-Z144)<=0,0,+P142)","v":20},null,"*(",{"$f":"+N144","v":4.25},null,"-",{"$f":"+T142","v":3},null,")-",{"$f":"IF((AF144-AI144)<=0,0,+W142)","v":0},null,"*(",{"$f":"+W144","v":4.25},null,"-",{"$f":"+AA142","v":4.5},null,")-",{"$f":"IF((AO144-AR144)<=0,0,+AD142)","v":0},null,"*(",{"$f":"+AF144","v":4.25},null,"-",{"$f":"+AH142","v":7},null,")-",{"$f":"+AK142","v":30},null,"*",{"$f":"+AO144","v":4.25},null,"²/",2,"=",{"$f":"E144*H144-K144*(N144-Q144)-T144*(W144-Z144)-AC144*(AF144-AI144)-AL144*(AO144-AR144)-AU144*AX144^2/BA144","v":370.9375},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E144","v":169.85294117647058},null,"-",{"$f":"+K144","v":20},null,"-",{"$f":"+T144","v":20},null,"-",{"$f":"+AC144","v":0},null,"-",{"$f":"+AL144","v":0},null,"-",{"$f":"+AU144","v":30},null,"*",{"$f":"+AX144","v":4.25},null,"=",{"$f":"+E145-H145-K145-N145-Q145-T145*W145","v":2.3529411764705799},null,null,"KN"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"x=",{"$f":"(E145-H145-K145-N145-Q145)/T145","v":4.3284313725490193},null,null,"m. ' deki max moment miktarı"]
[null,null,"Mmax =",null,null,{"$f":"+E142","v":169.85294117647058},null,"*",{"$f":"+D147","v":4.3284313725490193},null,"-",{"$f":"IF((O148-R148)<=0,0,+I142)","v":20},null,"*(",{"$f":"+I148","v":4.3284313725490193},null,"-",{"$f":"+M142","v":1.5},null,")-",{"$f":"IF((X148-AA148)<=0,0,+P142)","v":20},null,"*(",{"$f":"+O148","v":4.3284313725490193},null,"-",{"$f":"+T142","v":3},null,")-",{"$f":"IF((AG148-AJ148)<=0,0,+W142)","v":0},null,"*(",{"$f":"+X148","v":4.3284313725490193},null,"-",{"$f":"+AA142","v":4.5},null,")-",{"$f":"IF((AP148-AS148)<=0,0,+AD142)","v":0},null,"*(",{"$f":"+AG148","v":4.3284313725490193},null,"-",{"$f":"+AH142","v":7},null,")-",{"$f":"+AK142","v":30},null,"*",{"$f":"+AP148","v":4.3284313725490193},null,"²/",2,"=",{"$f":"F148*I148-L148*(O148-R148)-U148*(X148-AA148)-AD148*(AG148-AJ148)-AM148*(AP148-AS148)-AV148*AY148^2/BB148","v":371.02977220299891},null,null,"KNm"]
[null,null,"L / 2 =",null,{"$f":"+AG130/2","v":4.25},null,null,"m. ' deki moment miktarı"]
[null,null,"MB =",null,{"$f":"+E142","v":169.85294117647058},null,"*",{"$f":"+E149","v":4.25},null,"-",{"$f":"IF((N150-Q150)<=0,0,+I142)","v":20},null,"*(",{"$f":"+H150","v":4.25},null,"-",{"$f":"+M142","v":1.5},null,")-",{"$f":"IF((W150-Z150)<=0,0,+P142)","v":20},null,"*(",{"$f":"+N150","v":4.25},null,"-",{"$f":"+T142","v":3},null,")-",{"$f":"IF((AF150-AI150)<=0,0,+W142)","v":0},null,"*(",{"$f":"+W150","v":4.25},null,"-",{"$f":"+AA142","v":4.5},null,")-",{"$f":"IF((AO150-AR150)<=0,0,+AD142)","v":0},null,"*(",{"$f":"+AF150","v":4.25},null,"-",{"$f":"+AH142","v":7},null,")-",{"$f":"+AK142","v":30},null,"*",{"$f":"+AO150","v":4.25},null,"²/",2,"=",{"$f":"E150*H150-K150*(N150-Q150)-T150*(W150-Z150)-AC150*(AF150-AI150)-AL150*(AO150-AR150)-AU150*AX150^2/BA150","v":370.9375},null,null,"KNm"]
[null,null,"L / 4 =",null,{"$f":"+AG130/4","v":2.125},null,null,"m. ' deki moment miktarı"]
[null,null,"MA =",null,{"$f":"+E150","v":169.85294117647058},null,"*",{"$f":"+E151","v":2.125},null,"-",{"$f":"IF((N152-Q152)<=0,0,+I142)","v":20},null,"*(",{"$f":"+H152","v":2.125},null,"-",{"$f":"+Q150","v":1.5},null,")-",{"$f":"IF((W152-Z152)<=0,0,+P142)","v":0},null,"*(",{"$f":"+N152","v":2.125},null,"-",{"$f":"+Z150","v":3},null,")-",{"$f":"IF((AF152-AI152)<=0,0,+W142)","v":0},null,"*(",{"$f":"+W152","v":2.125},null,"-",{"$f":"+AI150","v":4.5},null,")-",{"$f":"IF((AO152-AR152)<=0,0,+AD142)","v":0},null,"*(",{"$f":"+AF152","v":2.125},null,"-",{"$f":"+AR150","v":7},null,")-",{"$f":"+AU150","v":30},null,"*",{"$f":"+AO152","v":2.125},null,"²/",2,"=",{"$f":"E152*H152-K152*(N152-Q152)-T152*(W152-Z152)-AC152*(AF152-AI152)-AL152*(AO152-AR152)-AU152*AX152^2/BA152","v":280.703125},null,null,"KNm"]
[null,null,"3 * L / 4 =",null,null,{"$f":"3*AG130/4","v":6.375},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,{"$f":"+E152","v":169.85294117647058},null,"*",{"$f":"+F153","v":6.375},null,"-",{"$f":"IF((N154-Q154)<=0,0,+I142)","v":20},null,"*(",{"$f":"+H154","v":6.375},null,"-",{"$f":"+Q152","v":1.5},null,")-",{"$f":"IF((W154-Z154)<=0,0,+P142)","v":20},null,"*(",{"$f":"+N154","v":6.375},null,"-",{"$f":"+Z152","v":3},null,")-",{"$f":"IF((AF154-AI154)<=0,0,+W142)","v":20},null,"*(",{"$f":"+W154","v":6.375},null,"-",{"$f":"+AI152","v":4.5},null,")-",{"$f":"IF((AO154-AR154)<=0,0,+AD142)","v":0},null,"*(",{"$f":"+AF154","v":6.375},null,"-",{"$f":"+AR152","v":7},null,")-",{"$f":"+AU152","v":30},null,"*",{"$f":"+AO154","v":6.375},null,"²/",2,"=",{"$f":"E154*H154-K154*(N154-Q154)-T154*(W154-Z154)-AC154*(AF154-AI154)-AL154*(AO154-AR154)-AU154*AX154^2/BA154","v":270.703125},null,null,"KNm"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(BD148)","v":371.02977220299891},null,null," /(",2.5,null,"*",{"$f":"+H156","v":371.02977220299891},null,null,"+",3,"*",{"$f":"ABS(BC152)","v":280.703125},null,null,"+",4,"*",{"$f":"ABS(BC150)","v":370.9375},null,null,"+",3,"*",{"$f":"ABS(BC154)","v":270.703125},null,null,")=",{"$f":"E156*H156/(L156*O156+S156*U156+Y156*AA156+AE156*AG156)","v":1.1407755241105437}]
[null,null,"SEHİM HESABI"]
[null,null,"E * I / 108 dy / dx =",null,null,null,null,null,{"$f":"+E142","v":169.85294117647058},null,"*  x²  /",null,2,"-",{"$f":"+I142","v":20},null,"*(  x -",null,{"$f":"+M142","v":1.5},null,")² / 2 -",null,{"$f":"+P142","v":20},null,"*(  x -",null,{"$f":"+T142","v":3},null,")² / 2 -",null,{"$f":"+W142","v":20},null,"*(  x -",null,{"$f":"+AA142","v":4.5},null,")² / 2 -",null,{"$f":"+AD142","v":20},null,"*(  x -",null,{"$f":"+AH142","v":7},null,")² / 2",null,"-",{"$f":"+AK142","v":30},null,"*","x3"," /",6,"+","C1",null,null,"(integral)"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+I158","v":169.85294117647058},null,"*  x3  /",null,6,"-",{"$f":"+O158","v":20},null,"*(  x -",null,{"$f":"+S158","v":1.5},null,")3 / 6 -",null,{"$f":"+W158","v":20},null,"*(  x -",null,{"$f":"+AA158","v":3},null,")3 / 6 -",null,{"$f":"+AE158","v":20},null,"*(  x -",null,{"$f":"+AI158","v":4.5},null,")3 / 6 -",null,{"$f":"+AM158","v":20},null,"*(  x -",null,{"$f":"+AQ158","v":7},null,")3 / 6",null,"-",{"$f":"+AV158","v":30},null,"*","x4"," /",24,null," + C1 * x + C2",null,null,null,null,null,"(integral)"]
[null,null,"x = 0 ; y = 0 ; C2 = 0"]
[null,null,"x=",{"$f":"+AG130","v":8.5},null,"m",";","y = 0"]
[null,null,{"$f":"+H159","v":169.85294117647058},null,"*",{"$f":"+D161","v":8.5},null,"3/",6,"-",{"$f":"+N159","v":20},null,"*(",{"$f":"+D161","v":8.5},null,"-",{"$f":"+R159","v":1.5},null,")3/",6,"-",{"$f":"+V159","v":20},null,"*(",{"$f":"+N162","v":8.5},null,"-",{"$f":"+Z159","v":3},null,")3/",6,"-",{"$f":"+AD159","v":20},null,"*(",{"$f":"+Y162","v":8.5},null,"-",{"$f":"+AH159","v":4.5},null,")3/",6,"-",{"$f":"+AL159","v":20},null,"*(",{"$f":"+AJ162","v":8.5},null,"-",{"$f":"+AP159","v":7},null,")3/",6,"-",{"$f":"+AU159","v":30},null,"*",{"$f":"+AU162","v":8.5},null," 4/",24,null,"+",{"$f":"+AU162","v":8.5},null,"*","C1","=",0]
[null,null,"C1 =",null,{"$f":"-(C162*F162^3/I162-K162*(N162-Q162)^3/T162-V162*(Y162-AB162)^3/AE162-AG162*(AJ162-AM162)^3/AP162-AR162*(AU162-AX162)^3/BA162-BC162*BF162^4/BI162)/BL162","v":-1051.4797794117644}]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+H159","v":169.85294117647058},null,"*  x3  /",null,6,"-",{"$f":"+N159","v":20},null,"*(  x -",null,{"$f":"+R159","v":1.5},null,")3 / 6 -",null,{"$f":"+V159","v":20},null,"*(  x -",null,{"$f":"+Z159","v":3},null,")3 / 6 -",null,{"$f":"+AD159","v":20},null,"*(  x -",null,{"$f":"+AH159","v":4.5},null,")3 / 6 -",null,{"$f":"+AL159","v":20},null,"*(  x -",null,{"$f":"+AP159","v":7},null,")3 / 6 ",null,"-",{"$f":"+BC162","v":30},null,"*","x4"," /",24,null,"+",{"$f":"+E163","v":-1051.4797794117644},null,null,"*","x"]
[null,null,"y = (",null,{"$f":"+H164","v":169.85294117647058},null,"*  x3  /",null,6,"-",{"$f":"+N164","v":20},null,"*(  x -",null,{"$f":"+R164","v":1.5},null,")3 / 6 -",null,{"$f":"+V164","v":20},null,"*(  x -",null,{"$f":"+Z164","v":3},null,")3 / 6 -",null,{"$f":"+AD164","v":20},null,"*(  x -",null,{"$f":"+AH164","v":4.5},null,")3 / 6 -",null,{"$f":"+AL164","v":20},null,"*(  x -",null,{"$f":"+AP164","v":7},null,")3 / 6",null,"-",{"$f":"+AU164","v":30},null,"*","x4"," /",24,null,"+",{"$f":"+BC164","v":-1051.4797794117644},null,null,"*","x ) * 108 / ( E * I )"]
[null,null,"x=",{"$f":"+AG130/2","v":4.25},null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D166<=AG130,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E165","v":169.85294117647058},null,"*",{"$f":"+D166","v":4.25},null,"3/",6,"-",{"$f":"IF((P167-S167)<=0,0,+K165)","v":20},null,"*(",{"$f":"+D166","v":4.25},null,"-",{"$f":"+O165","v":1.5},null,")3/",6,"-",{"$f":"IF((AA167-AD167)<=0,0,+S165)","v":20},null,"*(",{"$f":"+P167","v":4.25},null,"-",{"$f":"+W165","v":3},null,")3/",6,"-",{"$f":"IF((AL167-AO167)<=0,0,+AA165)","v":0},null,"*(",{"$f":"+AA167","v":4.25},null,"-",{"$f":"+AE165","v":4.5},null,")3/",6,"-",{"$f":"IF((AW167-AZ167)<=0,0,+AI165)","v":0},null,"*(",{"$f":"+AL167","v":4.25},null,"-",{"$f":"+AM165","v":7},null,")3/",6,"-",{"$f":"+AR165","v":30},null,"*",{"$f":"+AW167","v":4.25},null,"4/",24,null,"+"]
[null,null,null,"+",{"$f":"+AZ165","v":-1051.4797794117644},null,null,"*",{"$f":"+AW167","v":4.25},null,")* 108 / (",null,null,{"$f":"+Z133","v":200000},null,null,"*",{"$f":"+Z132","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"-(E167*H167^3/K167-M167*(P167-S167)^3/V167-X167*(AA167-AD167)^3/AG167-AI167*(AL167-AO167)^3/AR167-AT167*(AW167-AZ167)^3/BC167-BE167*BH167^4/BK167+E168*I168)*100000000/(N168*R168)","v":15.091742220872241},null,null,"mm"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"+AG130*1000","v":8500},null,null," /",300,null,"=",{"$f":"+H170/L170","v":28.333333333333332},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E169","v":15.091742220872241},null,null,"mm",null,{"$f":"IF(D171<M171,\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O170","v":28.333333333333332},null,null,"mm",null,{"$f":"IF(D171<M171,\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI (3 adet tekil yüklü)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,20,null,"KN",null,null,20,null,"KN",null,null,20,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,null,"KN/m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK213","v":1.1207970112079697}]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O177,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"+AU205","v":179.99999999999994},null,null,"KNm",null,"(max moment)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(U184,AO184)","v":120},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O177,$CG$6:$CG$120,0),0)","v":12}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E194","v":120},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E197","v":120},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"m","m",null,2,null,"m",null,null,2,null,"m",null,null,1,null,"m"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O177,$CG$6:$CG$120,0),0)","v":19}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",{"$f":"+W185+AB185+AG185+AL185","v":6},null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O177,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O177,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,"MESNET TEPKİLERİ"]
[null,null,"MB = 0    (sağ mesnette moment sıfır şartından)"]
[null,null,"A","*",{"$f":"+AE187","v":6},null,"-",{"$f":"+Z177","v":20},null,"*",{"$f":"+AB185+AG185+AL185","v":5},null,"-",{"$f":"+AE177","v":20},null,"*",{"$f":"+AG185+AL185","v":3},null,"-",{"$f":"+AJ177","v":20},null,"*",{"$f":"+AL185","v":1},null,"-",{"$f":"+AG178","v":30},null,"*",{"$f":"+AE187","v":6},null,"*",{"$f":"+AE187/2","v":3},null,"=",0]
[null,null,"A =",null,{"$f":"(H193*K193+N193*Q193+T193*W193+Z193*AC193*AF193)/E193","v":120},null,"KN",null,"(sol mesnet tepkisi)"]
[null,null,"Fy = 0    (düşey denge denklemi yazılırsa)"]
[null,null,"A","+","B","-",{"$f":"+Z177","v":20},null,"-",{"$f":"+AE177","v":20},null,"-",{"$f":"+AJ177","v":20},null,"-",{"$f":"+AG178","v":30},null,"*",{"$f":"+AE187","v":6},null,"=",0]
[null,null,"B =",null,{"$f":"(G196+J196+M196+P196*S196-E194)","v":120},null,"KN",null,"(sağ mesnet tepkisi)"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"Mx =",null,{"$f":"+U184","v":120},null," *  x  -",null,{"$f":"+Z177","v":20},null,"*(  x -",null,{"$f":"+W185","v":1},null,")-",{"$f":"+AE177","v":20},null,"*(  x -",null,{"$f":"+W185+AB185","v":3},null,")-",{"$f":"+AJ177","v":20},null,"*(  x -",null,{"$f":"+W185+AB185+AG185","v":5},null,")-",{"$f":"+AG178","v":30},null,"*","x²"," /",2]
[null,null,"x=",{"$f":"+AE187/2","v":3},null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D200<=AE187,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+E199","v":120},null,"*",{"$f":"+D200","v":3},null,"-",{"$f":"IF((N201-Q201)<=0,0,+I199)","v":20},null,"*(",{"$f":"+H201","v":3},null,"-",{"$f":"+M199","v":1},null,")-",{"$f":"IF((W201-Z201)<=0,0,+P199)","v":0},null,"*(",{"$f":"+N201","v":3},null,"-",{"$f":"+T199","v":3},null,")-",{"$f":"IF((AF201-AI201)<=0,0,+W199)","v":0},null,"*(",{"$f":"+W201","v":3},null,"-",{"$f":"+AA199","v":5},null,")-",{"$f":"+AD199","v":30},null,"*",{"$f":"+AF201","v":3},null,"²/",2,"=",{"$f":"E201*H201-K201*(N201-Q201)-T201*(W201-Z201)-AC201*(AF201-AI201)-AL201*AO201^2/AR201","v":185},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E201","v":120},null,"-",{"$f":"+K201","v":20},null,"-",{"$f":"+T201","v":0},null,"-",{"$f":"+AC201","v":0},null,"-",{"$f":"+AL201","v":30},null,"*",{"$f":"+AO201","v":3},null,"=",{"$f":"+E202-H202-K202-N202-Q202*T202","v":10},null,null,"KN"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"x=",{"$f":"(E202-H202-K202-N202)/Q202","v":3.3333333333333335},null,null,"m. ' deki max moment miktarı"]
[null,null,"Mmax =",null,null,{"$f":"+E199","v":120},null,"*",{"$f":"+D204","v":3.3333333333333335},null,"-",{"$f":"IF((O205-R205)<=0,0,+I199)","v":20},null,"*(",{"$f":"+I205","v":3.3333333333333335},null,"-",{"$f":"+M199","v":1},null,")-",{"$f":"IF((X205-AA205)<=0,0,+P199)","v":20},null,"*(",{"$f":"+O205","v":3.3333333333333335},null,"-",{"$f":"+T199","v":3},null,")-",{"$f":"IF((AG205-AJ205)<=0,0,+W199)","v":0},null,"*(",{"$f":"+X205","v":3.3333333333333335},null,"-",{"$f":"+AA199","v":5},null,")-",{"$f":"+AD199","v":30},null,"*",{"$f":"+AG205","v":3.3333333333333335},null,"²/",2,"=",{"$f":"F205*I205-L205*(O205-R205)-U205*(X205-AA205)-AD205*(AG205-AJ205)-AM205*AP205^2/AS205","v":179.99999999999994},null,null,"KNm"]
[null,null,"L / 2 =",null,{"$f":"+AE187/2","v":3},null,null,"m. ' deki moment miktarı"]
[null,null,"MB =",null,{"$f":"+E199","v":120},null,"*",{"$f":"+E206","v":3},null,"-",{"$f":"IF((N207-Q207)<=0,0,+I199)","v":20},null,"*(",{"$f":"+H207","v":3},null,"-",{"$f":"+M199","v":1},null,")-",{"$f":"IF((W207-Z207)<=0,0,+P199)","v":0},null,"*(",{"$f":"+N207","v":3},null,"-",{"$f":"+T199","v":3},null,")-",{"$f":"IF((AF207-AI207)<=0,0,+W199)","v":0},null,"*(",{"$f":"+W207","v":3},null,"-",{"$f":"+AA199","v":5},null,")-",{"$f":"+AD199","v":30},null,"*",{"$f":"+AF207","v":3},null,"²/",2,"=",{"$f":"E207*H207-K207*(N207-Q207)-T207*(W207-Z207)-AC207*(AF207-AI207)-AL207*AO207^2/AR207","v":185},null,null,"KNm"]
[null,null,"L / 4 =",null,{"$f":"+AE187/4","v":1.5},null,null,"m. ' deki moment miktarı"]
[null,null,"MA =",null,{"$f":"+E207","v":120},null,"*",{"$f":"+E208","v":1.5},null,"-",{"$f":"IF((N209-Q209)<=0,0,+I199)","v":20},null,"*(",{"$f":"+H209","v":1.5},null,"-",{"$f":"+Q207","v":1},null,")-",{"$f":"IF((W209-Z209)<=0,0,+P199)","v":0},null,"*(",{"$f":"+N209","v":1.5},null,"-",{"$f":"+Z207","v":3},null,")-",{"$f":"IF((AF209-AI209)<=0,0,+W199)","v":0},null,"*(",{"$f":"+W209","v":1.5},null,"-",{"$f":"+AI207","v":5},null,")-",{"$f":"+AL207","v":30},null,"*",{"$f":"+AF209","v":1.5},null,"²/",2,"=",{"$f":"E209*H209-K209*(N209-Q209)-T209*(W209-Z209)-AC209*(AF209-AI209)-AL209*AO209^2/AR209","v":136.25},null,null,"KNm"]
[null,null,"3 * L / 4 =",null,null,{"$f":"3*AE187/4","v":4.5},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,{"$f":"+E209","v":120},null,"*",{"$f":"+F210","v":4.5},null,"-",{"$f":"IF((N211-Q211)<=0,0,+I199)","v":20},null,"*(",{"$f":"+H211","v":4.5},null,"-",{"$f":"+Q209","v":1},null,")-",{"$f":"IF((W211-Z211)<=0,0,+P199)","v":20},null,"*(",{"$f":"+N211","v":4.5},null,"-",{"$f":"+Z209","v":3},null,")-",{"$f":"IF((AF211-AI211)<=0,0,+W199)","v":0},null,"*(",{"$f":"+W211","v":4.5},null,"-",{"$f":"+AI209","v":5},null,")-",{"$f":"+AL209","v":30},null,"*",{"$f":"+AF211","v":4.5},null,"²/",2,"=",{"$f":"E211*H211-K211*(N211-Q211)-T211*(W211-Z211)-AC211*(AF211-AI211)-AL211*AO211^2/AR211","v":136.25},null,null,"KNm"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AU205)","v":179.99999999999994},null,null," /(",2.5,null,"*",{"$f":"+H213","v":179.99999999999994},null,null,"+",3,"*",{"$f":"ABS(AT209)","v":136.25},null,null,"+",4,"*",{"$f":"ABS(AT207)","v":185},null,null,"+",3,"*",{"$f":"ABS(AT211)","v":136.25},null,null,")=",{"$f":"E213*H213/(L213*O213+S213*U213+Y213*AA213+AE213*AG213)","v":1.1207970112079697}]
[null,null,"SEHİM HESABI"]
[null,null,"E * I / 108 dy / dx =",null,null,null,null,null,{"$f":"+E199","v":120},null,"*  x²  /",null,2,"-",{"$f":"+I199","v":20},null,"*(  x -",null,{"$f":"+M199","v":1},null,")² / 2 -",null,{"$f":"+P199","v":20},null,"*(  x -",null,{"$f":"+T199","v":3},null,")² / 2 -",null,{"$f":"+W199","v":20},null,"*(  x -",null,{"$f":"+AA199","v":5},null,")² / 2",null,"-",{"$f":"+AD199","v":30},null,"*","x3"," /",6,"+","C1",null,null,"(integral)"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+I215","v":120},null,"*  x3  /",null,6,"-",{"$f":"+O215","v":20},null,"*(  x -",null,{"$f":"+S215","v":1},null,")3 / 6 -",null,{"$f":"+W215","v":20},null,"*(  x -",null,{"$f":"+AA215","v":3},null,")3 / 6 -",null,{"$f":"+AE215","v":20},null,"*(  x -",null,{"$f":"+AI215","v":5},null,")3 / 6",null,"-",{"$f":"+AN215","v":30},null,"*","x4"," /",24,null," + C1 * x + C2",null,null,null,null,null,"(integral)"]
[null,null,"x = 0 ; y = 0 ; C2 = 0"]
[null,null,"x=",{"$f":"+AE187","v":6},null,"m",";","y = 0"]
[null,null,{"$f":"+H216","v":120},null,"*",{"$f":"+D218","v":6},null,"3/",6,"-",{"$f":"+N216","v":20},null,"*(",{"$f":"+D218","v":6},null,"-",{"$f":"+R216","v":1},null,")3/",6,"-",{"$f":"+V216","v":20},null,"*(",{"$f":"+N219","v":6},null,"-",{"$f":"+Z216","v":3},null,")3/",6,"-",{"$f":"+AD216","v":20},null,"*(",{"$f":"+Y219","v":6},null,"-",{"$f":"+AH216","v":5},null,")3/",6,"-",{"$f":"+AM216","v":30},null,"*",{"$f":"+AJ219","v":6},null," 4/",24,null,"+",{"$f":"+AJ219","v":6},null,"*","C1","=",0]
[null,null,"C1 =",null,{"$f":"-(C219*F219^3/I219-K219*(N219-Q219)^3/T219-V219*(Y219-AB219)^3/AE219-AG219*(AJ219-AM219)^3/AP219-AR219*AU219^4/AX219)/BA219","v":-365}]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+H216","v":120},null,"*  x3  /",null,6,"-",{"$f":"+N216","v":20},null,"*(  x -",null,{"$f":"+R216","v":1},null,")3 / 6 -",null,{"$f":"+V216","v":20},null,"*(  x -",null,{"$f":"+Z216","v":3},null,")3 / 6 -",null,{"$f":"+AD216","v":20},null,"*(  x -",null,{"$f":"+AH216","v":5},null,")3 / 6",null,"-",{"$f":"+AR219","v":30},null,"*","x4"," /",24,null,"+",{"$f":"+E220","v":-365},null,null,"*","x"]
[null,null,"y = (",null,{"$f":"+H221","v":120},null,"*  x3  /",null,6,"-",{"$f":"+N221","v":20},null,"*(  x -",null,{"$f":"+R221","v":1},null,")3 / 6 -",null,{"$f":"+V221","v":20},null,"*(  x -",null,{"$f":"+Z221","v":3},null,")3 / 6 -",null,{"$f":"+AD221","v":20},null,"*(  x -",null,{"$f":"+AH221","v":5},null,")3 / 6",null,"-",{"$f":"+AM221","v":30},null,"*","x4"," /",24,null,"+",{"$f":"+AU221","v":-365},null,null,"*","x ) * 108 / ( E * I )"]
[null,null,"x=",{"$f":"+AE187/2","v":3},null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D223<=AE187,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E222","v":120},null,"*",{"$f":"+D223","v":3},null,"3/",6,"-",{"$f":"IF((P224-S224)<=0,0,+K222)","v":20},null,"*(",{"$f":"+D223","v":3},null,"-",{"$f":"+O222","v":1},null,")3/",6,"-",{"$f":"IF((AA224-AD224)<=0,0,+S222)","v":0},null,"*(",{"$f":"+P224","v":3},null,"-",{"$f":"+W222","v":3},null,")3/",6,"-",{"$f":"IF((AL224-AO224)<=0,0,+AA222)","v":0},null,"*(",{"$f":"+AA224","v":3},null,"-",{"$f":"+AE222","v":5},null,")3/",6,"-",{"$f":"+AJ222","v":30},null,"*",{"$f":"+AL224","v":3},null,"4/",24,null,"+",{"$f":"+AR222","v":-365},null,null,"*",{"$f":"+AL224","v":3},null,")* 108 / (",null,null,{"$f":"+Z190","v":200000},null,null,"*",{"$f":"+Z189","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"-(E224*H224^3/K224-M224*(P224-S224)^3/V224-X224*(AA224-AD224)^3/AG224-AI224*(AL224-AO224)^3/AR224-AT224*AW224^4/AZ224+BC224*BG224)*100000000/(BL224*BP224)","v":3.7082790327251662},null,null,"mm"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"+AE187*1000","v":6000},null,null," /",300,null,"=",{"$f":"+H226/L226","v":20},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E225","v":3.7082790327251662},null,null,"mm",null,{"$f":"IF(D227<M227,\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O226","v":20},null,null,"mm",null,{"$f":"IF(D227<M227,\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI (2 adet tekil yüklü)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,20,null,"KN",null,null,null,20,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,null,"KN/m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK269","v":1.1469453600884654}]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O233,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"+AL261","v":261.41157407407411},null,null,"KNm",null,"(max moment)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(U240,AM240)","v":137.83333333333334},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O233,$CG$6:$CG$120,0),0)","v":12}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E250","v":137.83333333333334},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E253","v":127.16666666666666},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,"m",null,null,null,2.5,null,"m",null,null,null,3.5,null,"m"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O233,$CG$6:$CG$120,0),0)","v":19}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",{"$f":"+X241+AD241+AJ241","v":7.5},null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O233,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O233,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)",null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)",null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,"MESNET TEPKİLERİ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,"MB = 0    (sağ mesnette moment sıfır şartından)"]
[null,null,"A","*",{"$f":"+AD243","v":7.5},null,"-",{"$f":"+AA233","v":20},null,"*",{"$f":"+AD241+AJ241","v":6},null,"-",{"$f":"+AG233","v":20},null,"*",{"$f":"+AJ241","v":3.5},null,"-",{"$f":"+AC234","v":30},null,"*",{"$f":"+AD243","v":7.5},null,"*",{"$f":"+AD243/2","v":3.75},null,"=",0]
[null,null,"A =",null,{"$f":"(H249*K249+N249*Q249+T249*W249*Z249)/E249","v":137.83333333333334},null,"KN",null,"(sol mesnet tepkisi)"]
[null,null,"Fy = 0    (düşey denge denklemi yazılırsa)"]
[null,null,"A","+","B","-",{"$f":"+AA233","v":20},null,"-",{"$f":"+AG233","v":20},null,"-",{"$f":"+AC234","v":30},null,"*",{"$f":"+AD243","v":7.5},null,"=",0]
[null,null,"B =",null,{"$f":"(G252+J252+M252*P252-E250)","v":127.16666666666666},null,"KN",null,"(sağ mesnet tepkisi)"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"Mx =",null,{"$f":"+U240","v":137.83333333333334},null," *  x  -",null,{"$f":"+AA233","v":20},null,"*(  x -",null,{"$f":"+X241","v":1.5},null,")-",{"$f":"+AG233","v":20},null,"*(  x -",null,{"$f":"+X241+AD241","v":4},null,")-",{"$f":"+AC234","v":30},null,"*","x²"," /",2]
[null,null,"x=",{"$f":"+AD243/2","v":3.75},null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D256<=AD243,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+E255","v":137.83333333333334},null,"*",{"$f":"+D256","v":3.75},null,"-",{"$f":"IF((N257-Q257)<=0,0,+I255)","v":20},null,"*(",{"$f":"+H257","v":3.75},null,"-",{"$f":"+M255","v":1.5},null,")-",{"$f":"IF((W257-Z257)<=0,0,+P255)","v":0},null,"*(",{"$f":"+N257","v":3.75},null,"-",{"$f":"+T255","v":4},null,")-",{"$f":"+W255","v":30},null,"*",{"$f":"+W257","v":3.75},null,"²/",2,"=",{"$f":"E257*H257-K257*(N257-Q257)-T257*(W257-Z257)-AC257*AF257^2/AI257","v":260.9375},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E257","v":137.83333333333334},null,"-",{"$f":"+K257","v":20},null,"-",{"$f":"+T257","v":0},null,"-",{"$f":"+AC257","v":30},null,"*",{"$f":"+AF257","v":3.75},null,"=",{"$f":"+E258-H258-K258-N258*Q258","v":5.3333333333333428},null,null,"KN"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"x=",{"$f":"(E258-H258-K258)/N258","v":3.927777777777778},null,null,"m. ' deki max moment miktarı"]
[null,null,"Mmax =",null,null,{"$f":"+E255","v":137.83333333333334},null,"*",{"$f":"+D260","v":3.927777777777778},null,"-",{"$f":"IF((O261-R261)<=0,0,+I255)","v":20},null,"*(",{"$f":"+I261","v":3.927777777777778},null,"-",{"$f":"+M255","v":1.5},null,")-",{"$f":"IF((X261-AA261)<=0,0,+P255)","v":0},null,"*(",{"$f":"+O261","v":3.927777777777778},null,"-",{"$f":"+T255","v":4},null,")-",{"$f":"+W255","v":30},null,"*",{"$f":"+X261","v":3.927777777777778},null,"²/",2,"=",{"$f":"F261*I261-L261*(O261-R261)-U261*(X261-AA261)-AD261*AG261^2/AJ261","v":261.41157407407411},null,null,"KNm"]
[null,null,"L / 2 =",null,{"$f":"+AD243/2","v":3.75},null,null,"m. ' deki moment miktarı"]
[null,null,"MB =",null,{"$f":"+E255","v":137.83333333333334},null,"*",{"$f":"+E262","v":3.75},null,"-",{"$f":"IF((N263-Q263)<=0,0,+I255)","v":20},null,"*(",{"$f":"+H263","v":3.75},null,"-",{"$f":"+M255","v":1.5},null,")-",{"$f":"IF((W263-Z263)<=0,0,+P255)","v":0},null,"*(",{"$f":"+N263","v":3.75},null,"-",{"$f":"+T255","v":4},null,")-",{"$f":"+W255","v":30},null,"*",{"$f":"+W263","v":3.75},null,"²/",2,"=",{"$f":"E263*H263-K263*(N263-Q263)-T263*(W263-Z263)-AC263*AF263^2/AI263","v":260.9375},null,null,"KNm"]
[null,null,"L / 4 =",null,{"$f":"+AD243/4","v":1.875},null,null,"m. ' deki moment miktarı"]
[null,null,"MA =",null,{"$f":"+E255","v":137.83333333333334},null,"*",{"$f":"+E264","v":1.875},null,"-",{"$f":"IF((N265-Q265)<=0,0,+I255)","v":20},null,"*(",{"$f":"+H265","v":1.875},null,"-",{"$f":"+M255","v":1.5},null,")-",{"$f":"IF((W265-Z265)<=0,0,+P255)","v":0},null,"*(",{"$f":"+N265","v":1.875},null,"-",{"$f":"+T255","v":4},null,")-",{"$f":"+W255","v":30},null,"*",{"$f":"+W265","v":1.875},null,"²/",2,"=",{"$f":"E265*H265-K265*(N265-Q265)-T265*(W265-Z265)-AC265*AF265^2/AI265","v":198.203125},null,null,"KNm"]
[null,null,"3 * L / 4 =",null,null,{"$f":"3*AD243/4","v":5.625},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,{"$f":"+E255","v":137.83333333333334},null,"*",{"$f":"+F266","v":5.625},null,"-",{"$f":"IF((N267-Q267)<=0,0,+I255)","v":20},null,"*(",{"$f":"+H267","v":5.625},null,"-",{"$f":"+M255","v":1.5},null,")-",{"$f":"IF((W267-Z267)<=0,0,+P255)","v":20},null,"*(",{"$f":"+N267","v":5.625},null,"-",{"$f":"+T255","v":4},null,")-",{"$f":"+W255","v":30},null,"*",{"$f":"+W267","v":5.625},null,"²/",2,"=",{"$f":"E267*H267-K267*(N267-Q267)-T267*(W267-Z267)-AC267*AF267^2/AI267","v":185.703125},null,null,"KNm"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AL261)","v":261.41157407407411},null,null," /(",2.5,null,"*",{"$f":"+H269","v":261.41157407407411},null,null,"+",3,"*",{"$f":"ABS(AK265)","v":198.203125},null,null,"+",4,"*",{"$f":"ABS(AK263)","v":260.9375},null,null,"+",3,"*",{"$f":"ABS(AK267)","v":185.703125},null,null,")=",{"$f":"E269*H269/(L269*O269+S269*U269+Y269*AA269+AE269*AG269)","v":1.1469453600884654}]
[null,null,"SEHİM HESABI"]
[null,null,"E * I / 108 dy / dx =",null,null,null,null,null,{"$f":"+E255","v":137.83333333333334},null,"*  x²  /",null,2,"-",{"$f":"+I255","v":20},null,"*(  x -",null,{"$f":"+M255","v":1.5},null,")² / 2 -",null,{"$f":"+P255","v":20},null,"*(  x -",null,{"$f":"+T255","v":4},null,")² / 2 ",null,"-",{"$f":"+W255","v":30},null,"*","x3"," /",6,"+","C1",null,null,"(integral)"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+I271","v":137.83333333333334},null,"*  x3  /",null,6,"-",{"$f":"+O271","v":20},null,"*(  x -",null,{"$f":"+S271","v":1.5},null,")3 / 6 -",null,{"$f":"+W271","v":20},null,"*(  x -",null,{"$f":"+AA271","v":4},null,")3 / 6",null,"-",{"$f":"+AF271","v":30},null,"*","x4"," /",24,null," + C1 * x + C2",null,null,null,null,null,"(integral)"]
[null,null,"x = 0 ; y = 0 ; C2 = 0"]
[null,null,"x=",{"$f":"+AD243","v":7.5},null,"m",";","y = 0"]
[null,null,{"$f":"+H272","v":137.83333333333334},null,"*",{"$f":"+D274","v":7.5},null,"3/",6,"-",{"$f":"+N272","v":20},null,"*(",{"$f":"+D274","v":7.5},null,"-",{"$f":"+R272","v":1.5},null,")3/",6,"-",{"$f":"+V272","v":20},null,"*(",{"$f":"+N275","v":7.5},null,"-",{"$f":"+Z272","v":4},null,")3/",6,"-",{"$f":"+AE272","v":30},null,"*",{"$f":"+Y275","v":7.5},null," 4/",24,null,"+",{"$f":"+Y275","v":7.5},null,"*","C1","=",0]
[null,null,"C1 =",null,{"$f":"-(C275*F275^3/I275-K275*(N275-Q275)^3/T275-V275*(Y275-AB275)^3/AE275-AG275*AJ275^4/AM275)/AP275","v":-649.7881944444448}]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+H272","v":137.83333333333334},null,"*  x3  /",null,6,"-",{"$f":"+N272","v":20},null,"*(  x -",null,{"$f":"+R272","v":1.5},null,")3 / 6 -",null,{"$f":"+V272","v":20},null,"*(  x -",null,{"$f":"+Z272","v":4},null,")3 / 6",null,"-",{"$f":"+AG275","v":30},null,"*","x4"," /",24,null,"+",{"$f":"+E276","v":-649.7881944444448},null,null,"*","x"]
[null,null,"y = (",null,{"$f":"+H277","v":137.83333333333334},null,"*  x3  /",null,6,"-",{"$f":"+N277","v":20},null,"*(  x -",null,{"$f":"+R277","v":1.5},null,")3 / 6 -",null,{"$f":"+V277","v":20},null,"*(  x -",null,{"$f":"+Z277","v":4},null,")3 / 6",null,"-",{"$f":"+AE277","v":30},null,"*","x4"," /",24,null,"+",{"$f":"+AM277","v":-649.7881944444448},null,null,"*","x ) * 108 / ( E * I )"]
[null,null,"x=",{"$f":"+AD243/2","v":3.75},null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D279<=AD243,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E278","v":137.83333333333334},null,"*",{"$f":"+D279","v":3.75},null,"3/",6,"-",{"$f":"IF((P280-S280)<=0,0,+K278)","v":20},null,"*(",{"$f":"+D279","v":3.75},null,"-",{"$f":"+O278","v":1.5},null,")3/",6,"-",{"$f":"IF((AA280-AD280)<=0,0,+S278)","v":0},null,"*(",{"$f":"+P280","v":3.75},null,"-",{"$f":"+W278","v":4},null,")3/",6,"-",{"$f":"+AB278","v":30},null,"*",{"$f":"+AA280","v":3.75},null,"4/",24,null,"+",{"$f":"+AJ278","v":-649.7881944444448},null,null,"*",{"$f":"+AA280","v":3.75},null,")* 108 / (",null,null,{"$f":"+Z246","v":200000},null,null,"*",{"$f":"+Z245","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"-(E280*H280^3/K280-M280*(P280-S280)^3/V280-X280*(AA280-AD280)^3/AG280-AI280*AL280^4/AO280+AR280*AV280)*100000000/(BA280*BE280)","v":8.2017869283729787},null,null,"mm"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"+AD243*1000","v":7500},null,null," /",300,null,"=",{"$f":"+H282/L282","v":25},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E281","v":8.2017869283729787},null,null,"mm",null,{"$f":"IF(D283<M283,\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O282","v":25},null,null,"mm",null,{"$f":"IF(D283<M283,\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI (1 adet tekil yüklü)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,null,20,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,null,"KN/m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK325","v":1.1422287390029326}]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O289,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"+AC317","v":243.43750000000003},null,null,"KNm",null,"(max moment)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(U296,AI296)","v":122.5},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O289,$CG$6:$CG$120,0),0)","v":12}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E306","v":122.5},null,"KN",null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E309","v":122.5},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.75,null,"m",null,null,null,null,3.75,null,"m"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O289,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",{"$f":"+X297+AE297","v":7.5},null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O289,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O289,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,"MESNET TEPKİLERİ"]
[null,null,"MB = 0    (sağ mesnette moment sıfır şartından)"]
[null,null,"A","*",{"$f":"+AB299","v":7.5},null,"-",{"$f":"+AB289","v":20},null,"*",{"$f":"+AE297","v":3.75},null,"-",{"$f":"+AD290","v":30},null,"*",{"$f":"+AB299","v":7.5},null,"*",{"$f":"+AB299/2","v":3.75},null,"=",0]
[null,null,"A =",null,{"$f":"(H305*K305+N305*Q305*T305)/E305","v":122.5},null,"KN",null,"(sol mesnet tepkisi)"]
[null,null,"Fy = 0    (düşey denge denklemi yazılırsa)"]
[null,null,"A","+","B","-",{"$f":"+AB289","v":20},null,"-",{"$f":"+AD290","v":30},null,"*",{"$f":"+AB299","v":7.5},null,"=",0]
[null,null,"B =",null,{"$f":"(G308+J308*M308-E306)","v":122.5},null,"KN",null,"(sağ mesnet tepkisi)"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"Mx =",null,{"$f":"+U296","v":122.5},null," *  x  -",null,{"$f":"+AB289","v":20},null,"*(  x -",null,{"$f":"+X297","v":3.75},null,")-",{"$f":"+AD290","v":30},null,"*","x²"," /",2]
[null,null,"x=",{"$f":"+AB299/2","v":3.75},null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D312<=AB299,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+E311","v":122.5},null,"*",{"$f":"+D312","v":3.75},null,"-",{"$f":"IF((N313-Q313)<=0,0,+I311)","v":0},null,"*(",{"$f":"+H313","v":3.75},null,"-",{"$f":"+M311","v":3.75},null,")-",{"$f":"+P311","v":30},null,"*",{"$f":"+N313","v":3.75},null,"²/",2,"=",{"$f":"E313*H313-K313*(N313-Q313)-T313*W313^2/Z313","v":248.4375},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E313","v":122.5},null,"-",{"$f":"+K313","v":0},null,"-",{"$f":"+T313","v":30},null,"*",{"$f":"+W313","v":3.75},null,"=",{"$f":"+E314-H314-K314*N314","v":10},null,null,"KN"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"x=",{"$f":"(E314-H314)/K314","v":4.083333333333333},null,null,"m. ' deki max moment miktarı"]
[null,null,"Mmax =",null,null,{"$f":"+E311","v":122.5},null,"*",{"$f":"+D316","v":4.083333333333333},null,"-",{"$f":"IF((O317-R317)<=0,0,+I311)","v":20},null,"*(",{"$f":"+I317","v":4.083333333333333},null,"-",{"$f":"+M311","v":3.75},null,")-",{"$f":"+P311","v":30},null,"*",{"$f":"+O317","v":4.083333333333333},null,"²/",2,"=",{"$f":"F317*I317-L317*(O317-R317)-U317*X317^2/AA317","v":243.43750000000003},null,null,"KNm"]
[null,null,"L / 2 =",null,{"$f":"+AB299/2","v":3.75},null,null,"m. ' deki moment miktarı"]
[null,null,"MB =",null,{"$f":"+E311","v":122.5},null,"*",{"$f":"+E318","v":3.75},null,"-",{"$f":"IF((N319-Q319)<=0,0,+I311)","v":0},null,"*(",{"$f":"+H319","v":3.75},null,"-",{"$f":"+M311","v":3.75},null,")-",{"$f":"+P311","v":30},null,"*",{"$f":"+N319","v":3.75},null,"²/",2,"=",{"$f":"E319*H319-K319*(N319-Q319)-T319*W319^2/Z319","v":248.4375},null,null,"KNm"]
[null,null,"L / 4 =",null,{"$f":"+AB299/4","v":1.875},null,null,"m. ' deki moment miktarı"]
[null,null,"MA =",null,{"$f":"+E311","v":122.5},null,"*",{"$f":"+E320","v":1.875},null,"-",{"$f":"IF((N321-Q321)<=0,0,+I311)","v":0},null,"*(",{"$f":"+H321","v":1.875},null,"-",{"$f":"+M311","v":3.75},null,")-",{"$f":"+P311","v":30},null,"*",{"$f":"+N321","v":1.875},null,"²/",2,"=",{"$f":"E321*H321-K321*(N321-Q321)-T321*W321^2/Z321","v":176.953125},null,null,"KNm"]
[null,null,"3 * L / 4 =",null,null,{"$f":"3*AB299/4","v":5.625},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,{"$f":"+E311","v":122.5},null,"*",{"$f":"+F322","v":5.625},null,"-",{"$f":"IF((N323-Q323)<=0,0,+I311)","v":20},null,"*(",{"$f":"+H323","v":5.625},null,"-",{"$f":"+M311","v":3.75},null,")-",{"$f":"+P311","v":30},null,"*",{"$f":"+N323","v":5.625},null,"²/",2,"=",{"$f":"E323*H323-K323*(N323-Q323)-T323*W323^2/Z323","v":176.953125},null,null,"KNm"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AC317)","v":243.43750000000003},null,null," /(",2.5,null,"*",{"$f":"+H325","v":243.43750000000003},null,null,"+",3,"*",{"$f":"ABS(AB321)","v":176.953125},null,null,"+",4,"*",{"$f":"ABS(AB319)","v":248.4375},null,null,"+",3,"*",{"$f":"ABS(AB323)","v":176.953125},null,null,")=",{"$f":"E325*H325/(L325*O325+S325*U325+Y325*AA325+AE325*AG325)","v":1.1422287390029326}]
[null,null,"SEHİM HESABI"]
[null,null,"E * I / 108 dy / dx =",null,null,null,null,null,{"$f":"+E311","v":122.5},null,"*  x²  /",null,2,"-",{"$f":"+I311","v":20},null,"*(  x -",null,{"$f":"+M311","v":3.75},null,")² / 2",null,"-",{"$f":"+P311","v":30},null,"*","x3"," /",6,"+","C1",null,null,"(integral)"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+I327","v":122.5},null,"*  x3  /",null,6,"-",{"$f":"+O327","v":20},null,"*(  x -",null,{"$f":"+S327","v":3.75},null,")3 / 6",null,"-",{"$f":"+X327","v":30},null,"*","x4"," /",24,null," + C1 * x + C2",null,null,null,null,null,"(integral)"]
[null,null,"x = 0 ; y = 0 ; C2 = 0"]
[null,null,"x=",{"$f":"+AB299","v":7.5},null,"m",";","y = 0"]
[null,null,{"$f":"+H328","v":122.5},null,"*",{"$f":"+D330","v":7.5},null,"3/",6,"-",{"$f":"+N328","v":20},null,"*(",{"$f":"+D330","v":7.5},null,"-",{"$f":"+R328","v":3.75},null,")3/",6,"-",{"$f":"+W328","v":30},null,"*",{"$f":"+N331","v":7.5},null,"4/",{"$f":"+AB328","v":24},null,"+",{"$f":"+N331","v":7.5},null,"*","C1","=",0]
[null,null,"C1 =",null,{"$f":"-(C331*F331^3/I331-K331*(N331-Q331)^3/T331-V331*Y331^4/AB331)/AE331","v":-597.65625}]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+H328","v":122.5},null,"*  x3  /",null,6,"-",{"$f":"+N328","v":20},null,"*(  x -",null,{"$f":"+R328","v":3.75},null,")3 / 6",null,"-",{"$f":"+W328","v":30},null,"*","x4"," /",24,null,"+",{"$f":"E332","v":-597.65625},null,null,"*","x"]
[null,null,"y = (",null,{"$f":"+H333","v":122.5},null,"*  x3  /",null,6,"-",{"$f":"+N333","v":20},null,"*(  x -",null,{"$f":"+R333","v":3.75},null,")3 / 6",null,"-",{"$f":"+W333","v":30},null,"*","x4"," /",24,null,"+",{"$f":"+AE333","v":-597.65625},null,null,"*","x ) * 108 / ( E * I )"]
[null,null,"x=",1,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D335<=AB299,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E334","v":122.5},null,"*",{"$f":"+D335","v":1},null,"3/",6,"-",{"$f":"IF((P336-S336)<=0,0,+K334)","v":0},null,"*(",{"$f":"+D335","v":1},null,"-",{"$f":"+O334","v":3.75},null,")3/",6,"-",{"$f":"+T334","v":30},null,"*",{"$f":"+P336","v":1},null,"4/",24,null,"+",{"$f":"+AB334","v":-597.65625},null,null,"*",{"$f":"+P336","v":1},null,")* 108 / (",null,null,{"$f":"+Z302","v":200000},null,null,"*",{"$f":"+Z301","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"-(E336*H336^3/K336-M336*(P336-S336)^3/V336-X336*AA336^4/AD336+AG336*AK336)*100000000/(AP336*AT336)","v":3.1412336193165364},null,null,"mm"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"+AB299*1000","v":7500},null,null," /",300,null,"=",{"$f":"+H338/L338","v":25},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E337","v":3.1412336193165364},null,null,"mm",null,{"$f":"IF(D339<M339,\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O338","v":25},null,null,"mm",null,{"$f":"IF(D339<M339,\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK KONSOL KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,null,"KN",null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w =",null,30,null,"KN/m"]
[]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O345,$CG$6:$CG$120,0),0)","v":600}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O345,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,"M=",{"$f":"-W363","v":183.75},null,null,"KNm",null,null,null,"x"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",1.5,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca konsol kirişte Cb = 1 alınır."]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O345,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,"A=",{"$f":"+H362","v":145},null,"KN"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O345,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)"]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O345,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[]
[null,null,null,null,null,"MESNET TEPKİLERİ"]
[null,null,null,null,null,"Fy = 0    (düşey denge denklemi yazılırsa)"]
[null,null,null,null,null,"A","-",{"$f":"+AA347","v":30},null,"*",{"$f":"+AA352","v":1.5},null,"-",{"$f":"+AF345","v":100},null,"=",0]
[null,null,null,null,null,"A =",null,{"$f":"H361*K361+N361","v":145},null,null,"KN",null,"(sol mesnet tepkisi)"]
[null,null,null,null,null,"M =",null,{"$f":"-AA347","v":-30},null,"*",{"$f":"+AA352","v":1.5},null,"*",{"$f":"+AA352/2","v":0.75},null,"-",{"$f":"+AF345","v":100},null,"*",{"$f":"+AA352","v":1.5},null,"=",{"$f":"+H363*K363*N363-Q363*T363","v":-183.75},null,null,"KNm"]
[null,null,null,null,null,"ARA KESİT TESİRLERİ"]
[null,null,null,null,null,"x=",1,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(G365<=AA352,\"\",\"azalt.\")","v":""}]
[null,null,null,null,null,"Mx =",null,{"$f":"+R351","v":183.75},null,"-",{"$f":"+V354","v":145},null,"*",{"$f":"+G365","v":1},null,"+",{"$f":"+AA347","v":30},null,"*",{"$f":"+G365","v":1},null,"² /",2,"=",{"$f":"+H366-K366*N366+Q366*T366^2/W366","v":53.75},null,null,"KNm"]
[null,null,null,null,null,"Vx =",null,{"$f":"+K366","v":145},null,"-",{"$f":"+Q366","v":30},null,"*",{"$f":"+G365","v":1},null,"=",{"$f":"+H367-K367*N367","v":115},null,null,"KN"]
[null,null,null,null,null,"SEHİM HESABI"]
[null,null,null,null,null,"v'' = P * x + w * x² / 2 "]
[null,null,null,null,null,"v' = P * x² / 2 + w * x3 / 6 + C1"]
[null,null,null,null,null,"v =  P * x3 / 6 + w * x4 / 24 + C1 * x + C2"]
[null,null,null,null,null,"sınır ve uygunluk şartları :"]
[null,null,null,null,null,"x = L ; v = 0",null,null,null,null,null,"C2","=",0]
[null,null,null,null,null,"x = L ; v' = 0",null,null,null,null,null,{"$f":"AF345","v":100},null,"*",{"$f":"+AA352","v":1.5},null,"² /",2,"+",{"$f":"+AA347","v":30},null,"*",{"$f":"+AA352","v":1.5},null,"3 /",6,"+","C1",null,null,"C1","=",{"$f":"-(L374*O374^2/R374+T374*W374^3/Z374)","v":-129.375}]
[null,null,null,null,null,"E * I / 108 * y = P * x3 / 6 + w * x4 / 24 + C1 * x + C2"]
[null,null,null,null,null,"x=",1.5,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(G376<=AA352,\"\",\"azalt.\")","v":""}]
[null,null,null,null,null,"y = (",null,{"$f":"AF345","v":100},null,"*",{"$f":"+G376","v":1.5},null,"3 /",6,"+",{"$f":"+AA347","v":30},null,"*",{"$f":"+G376","v":1.5},null,"4 /",24,null,"+",{"$f":"+AG374","v":-129.375},null,null,"*",{"$f":"+G376","v":1.5},null,")* 108 / (",null,null,{"$f":"+Y357","v":200000},null,null,"*",{"$f":"+Y356","v":92080},null,null,")"]
[null,null,null,null,null,"y =",null,{"$f":"(H377*K377^3/N377+P377*S377^4/V377+Y377*AC377)*100000000/(AH377*AL377)","v":-0.71396815269331015},null,null,"mm"]
[null,null,null,null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"+AA352*1000","v":1500},null,null," /",150,null,"=",{"$f":"+K379/O379","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,null,null,null,"y=",{"$f":"+H378","v":-0.71396815269331015},null,null,"mm",null,{"$f":"IF(ABS(G380)<ABS(P380),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+R379","v":10},null,null,"mm",null,{"$f":"IF(ABS(G380)<ABS(P380),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"YAYILI YÜKLÜ ÇELİK İKİ UCU ANKASTRE KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w =",null,30,null,"KN/m"]
[]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O386,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"M=",{"$f":"+Q402","v":62.5},null,null,"KNm",null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O386,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,"M=",{"$f":"+Q402","v":62.5},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O386,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,"A =",null,{"$f":"+Q403","v":75},null,"KN",null,null,null,null,null,null,null,null,null,null,"B =",null,{"$f":"+Q403","v":75},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",5,null,"m"]
[]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O386,$CG$6:$CG$120,0),0)","v":220}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O386,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,"MESNET TEPKİLERİ"]
[null,null,"M = w * L² / 12 =",null,null,null,null,{"$f":"+AC388","v":30},null,"*",{"$f":"+AC396","v":5},null,"²/",12,null,"=",{"$f":"+H402*K402^2/N402","v":62.5},null,null,"KNm"]
[null,null,"A = B = w * L / 2 =",null,null,null,null,null,{"$f":"+AC388","v":30},null,"*",{"$f":"+AC396","v":5},null," /",2,"=",{"$f":"+I403*L403/O403","v":75},null,null,"KN"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"x=",2.5,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D405<=AC396,\"\",\"azalt.\")","v":""}]
[null,null,"Mx = - w * ( L² - 6 * L * x + 6 * x² ) / 12 =",null,null,null,null,null,null,null,null,null,null,null,{"$f":"-AC388","v":-30},null,"*(",{"$f":"+AC396","v":5},null,"²-",6,"*",{"$f":"+AC396","v":5},null,"*",{"$f":"+D405","v":2.5},null,"+",6,"*",{"$f":"+D405","v":2.5},null,"² ) /",null,12,null,"=",{"$f":"O406*(R406^2-U406*W406*Z406+AC406*AE406^2)/AI406","v":31.25},null,null,"KNm"]
[null,null,"Vx = w * ( L / 2 - x ) =",null,null,null,null,null,null,{"$f":"+AC388","v":30},null,"*(",{"$f":"+AC396","v":5},null," /",2,"-",{"$f":"+D405","v":2.5},null,")=",{"$f":"+J407*(M407/P407-R407)","v":0},null,null,"KN"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"x=",{"$f":"+AC396/2","v":2.5},null,null,"m. ' deki max açıklık moment miktarı"]
[null,null,"Mx =",null,{"$f":"-AC388","v":-30},null,"*(",{"$f":"+AC396","v":5},null,"²-",6,"*",{"$f":"+AC396","v":5},null,"*",{"$f":"+D409","v":2.5},null,"+",6,"*",{"$f":"+D409","v":2.5},null,"² ) /",null,12,null,"=",{"$f":"E410*(H410^2-K410*M410*P410+S410*U410^2)/Y410","v":31.25},null,null,"KNm"]
[null,null,"Max =",null,{"$f":"MAX(AB410,P392)","v":62.5},null,null,"KNm"]
[null,null,"L / 2 =",null,{"$f":"+AC396/2","v":2.5},null,null,"m. ' deki moment miktarı"]
[null,null,"MB =",null,{"$f":"+E410","v":-30},null,"*(",{"$f":"+H410","v":5},null,"²-",6,"*",{"$f":"+M410","v":5},null,"*",{"$f":"+E412","v":2.5},null,"+",6,"*",{"$f":"+E412","v":2.5},null,"² ) /",null,12,null,"=",{"$f":"E413*(H413^2-K413*M413*P413+S413*U413^2)/Y413","v":31.25},null,null,"KNm"]
[null,null,"L / 4 =",null,{"$f":"+AC396/4","v":1.25},null,null,"m. ' deki moment miktarı"]
[null,null,"MA =",null,{"$f":"+E413","v":-30},null,"*(",{"$f":"+H413","v":5},null,"²-",6,"*",{"$f":"+M413","v":5},null,"*",{"$f":"+E414","v":1.25},null,"+",6,"*",{"$f":"+E414","v":1.25},null,"² ) /",null,12,null,"=",{"$f":"E415*(H415^2-K415*M415*P415+S415*U415^2)/Y415","v":7.8125},null,null,"KNm"]
[null,null,"3 * L / 4 =",null,null,{"$f":"3*AC396/4","v":3.75},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,{"$f":"+E415","v":-30},null,"*(",{"$f":"+H415","v":5},null,"²-",6,"*",{"$f":"+M415","v":5},null,"*",{"$f":"+F416","v":3.75},null,"+",6,"*",{"$f":"+F416","v":3.75},null,"² ) /",null,12,null,"=",{"$f":"E417*(H417^2-K417*M417*P417+S417*U417^2)/Y417","v":7.8125},null,null,"KNm"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(E411)","v":62.5},null,null," /(",2.5,null,"*",{"$f":"+H419","v":62.5},null,null,"+",3,"*",{"$f":"ABS(AB415)","v":7.8125},null,null,"+",4,"*",{"$f":"ABS(AB413)","v":31.25},null,null,"+",3,"*",{"$f":"ABS(AB417)","v":7.8125},null,null,")=",{"$f":"E419*H419/(L419*O419+S419*U419+Y419*AA419+AE419*AG419)","v":2.3809523809523809}]
[null,null,"SEHİM HESABI"]
[null,null,"x=",{"$f":"+AC396/2","v":2.5},null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D421<=AC396,\"\",\"azalt.\")","v":""}]
[null,null,"y = w * L4 / ( 24 * E * I ) * ( x² / L² - 2 * x3 / L3 + x4 / L4 )"]
[null,null,"y =",null,{"$f":"+AC388","v":30},null,"*",{"$f":"+AC396","v":5},null,null,"4/(",24,null,"*",{"$f":"+Z400","v":200000},null,null,null,"*",{"$f":"+Z399","v":92080},null,null,null,"*",10000,null,null,")*(",{"$f":"+D421","v":2.5},null,"²/",{"$f":"+AC396","v":5},null,"²-",2,"*",{"$f":"+D421","v":2.5},null,"3/",{"$f":"+AC396","v":5},null,"3+",{"$f":"+D421","v":2.5},null,"4/",{"$f":"+AC396","v":5},null,"4 ) * 1012"]
[null,null,"y =",null,{"$f":"E423*H423^4/(L423*O423*T423*Y423)*(AC423^2/AF423^2-AI423*AK423^3/AN423^3+AQ423^4/AT423^4)*1000000000000","v":0.26513968831450913},null,null,"mm"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"+AC396*1000","v":5000},null,null," /",300,null,"=",{"$f":"+H425/L425","v":16.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E424","v":0.26513968831450913},null,null,"mm",null,{"$f":"IF(ABS(D426)<ABS(M426),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O425","v":16.666666666666668},null,null,"mm",null,{"$f":"IF(ABS(D426)<ABS(M426),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"YAYILI YÜKLÜ ÇELİK BİR UCU ANKASTRE KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w =",null,30,null,"KN/m",null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK486","v":2.0833333333333335},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O432,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"+Y478","v":303.75},null,null,"KNm",null,"(max moment)",null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(AS438),ABS(AT438))","v":168.75},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O432,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,"M=",{"$f":"+G469","v":303.75},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U441","v":168.75},{"$f":"+AS438-AC434*AC442","v":-101.25}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x"]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O432,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,"A =",null,{"$f":"-G467","v":168.75},null,"KN",null,null,null,null,null,null,null,null,null,null,"B =",null,{"$f":"+Q468","v":101.25},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,"Uygunluk koşulları"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",9,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,"x = 0 ; v' = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v'' = 0"]
[]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O432,$CG$6:$CG$120,0),0)","v":220}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O432,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)",null,null,null,null,null,null,null,null,null,null,"x = 0 ; v = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v = 0"]
[null,null,"SEHİM HESABI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,"v''' = w * x + C1"]
[null,null,"v'' = w * x² / 2 + C1 * x + C2"]
[null,null,"v' = w * x3 / 6 + C1 * x² / 2 + C2 * x + C3"]
[null,null,"v = w * x4 / 24 + C1 * x3 / 6 + C2 * x² / 2 + C3 * x + C4"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"x = 0 ; v = 0",null,null,null,null,null,"C4 = 0"]
[null,null,"x = 0 ; v' = 0",null,null,null,null,null,"C3 = 0"]
[null,null,"x = L ; v = 0",null,null,null,null,null,{"$f":"+AC434","v":30},null,"*",{"$f":"+AC442","v":9},null,"4/",24,null,"+","C1","*",{"$f":"+AC442","v":9},null,"3 /",6,"+","C2","*",{"$f":"+T454","v":9},null,"² /",2,"=",0,null,null,"C1","*",{"$f":"+T454^3/W454","v":121.5},null,"+","C2","*",{"$f":"AA454^2/AD454","v":40.5},null,null,"+",{"$f":"I454*L454^4/O454","v":8201.25},null,null,"=",0,null,"(1.ci denklem)"]
[null,null,"x = L ; v'' = 0",null,null,null,null,null,{"$f":"+AC434","v":30},null,"*",{"$f":"+AC442","v":9},null,"² /",2,"+","C1","*",{"$f":"+L455","v":9},null,"+","C2","=",0,null,null,"C1","*",{"$f":"+S455","v":9},null,"+","C2","+",{"$f":"+I455*L455^2/O455","v":1215},null,null,"=",0,null,"(2.ci denklem)"]
[null,null,"iki adet denklem iki adet bilinmeyen çözülürse :"]
[null,null,"C1 =",null,{"$f":"+O457","v":-168.75},null,null,null,{"$f":"+AK454","v":121.5},{"$f":"+AP454","v":40.5},{"$f":"-AT454","v":-8201.25},null,{"$f":"MINVERSE(I457:J458)","v":-4.11522633744856E-3},0.16666666666666666,{"$f":"MMULT(M457:N458,K457:K458)","v":-168.75}]
[null,null,"C2 =",null,{"$f":"+O458","v":303.75},null,null,null,{"$f":"+AC455","v":9},1,{"$f":"-AH455","v":-1215},null,3.7037037037037035E-2,-0.5,303.75]
[null,null,"E * I / 108 * y = w * x4 / 24 + C1 * x3 / 6 + C2 * x² / 2 + C3 * x + C4"]
[null,null,"y = (",null,{"$f":"+AC434","v":30},null,"*","x4"," /",24,null,"+",{"$f":"+E457","v":-168.75},null,null,"*","x3"," /",6,"+",{"$f":"+E458","v":303.75},null,null,"*","x²"," /",2,") * 108 / ( E * I )"]
[null,null,"x=",5.625,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D461<=AC442,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E460","v":30},null,"*",{"$f":"+D461","v":5.625},null,"4 /",{"$f":"+J460","v":24},null,"+",{"$f":"+M460","v":-168.75},null,null,"*",{"$f":"+H462","v":5.625},null,"3 /",6,"+",{"$f":"+U460","v":303.75},null,null,"*",{"$f":"+R462","v":5.625},null,"² /",2,")* 108 / (",null,null,{"$f":"+Z446","v":200000},null,null,"*",{"$f":"+Z445","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E462*H462^4/K462+N462*R462^3/U462+W462*AA462^2/AD462)*100000000/(AH462*AL462)","v":5.7080017805720908},null,null,"mm"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"AC442*1000","v":9000},null,null," /",300,null,"=",{"$f":"+H464/L464","v":30},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E463","v":5.7080017805720908},null,null,"mm",null,{"$f":"IF(ABS(D465)<ABS(M465),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O464","v":30},null,null,"mm",null,{"$f":"IF(ABS(D465)<ABS(M465),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"MESNET TEPKİLERİ"]
[null,null,"x= 0 ; v''' =",null,null,null,{"$f":"+E457","v":-168.75},null,null,"KN",null,"(A mesnet tepkisi)"]
[null,null,"x= L ; v''' =",null,null,null,{"$f":"+AC434","v":30},null,"*",{"$f":"+AC442","v":9},null,"+",{"$f":"+E457","v":-168.75},null,null,"=",{"$f":"+G468*J468+M468","v":101.25},null,null,"KN",null,"(B mesnet tepkisi)"]
[null,null,"x= 0 ; v'' =",null,null,null,{"$f":"+E458","v":303.75},null,null,"KNm",null,"(mesnet momenti)"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"x=",1,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D471<=AC442,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+AC434","v":30},null,"*",{"$f":"+D471","v":1},null,"² /",2,"+",{"$f":"+E457","v":-168.75},null,null,"*",{"$f":"+D471","v":1},null,"+",{"$f":"+E458","v":303.75},null,null,"=",{"$f":"+E472*H472^2/K472+M472*Q472+T472","v":150},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+AC434","v":30},null,"*",{"$f":"+D471","v":1},null,"+",{"$f":"+E457","v":-168.75},null,null,"=",{"$f":"+E473*H473+K473","v":-138.75},null,null,"KN"]
[null,null,"x=",{"$f":"+AK479","v":5.625},null,null,"m.deki max açıklık moment miktarı"]
[null,null,"Mxaç =",null,null,{"$f":"+E472","v":30},null,"*",{"$f":"+D474","v":5.625},null,"² /",2,"+",{"$f":"+M472","v":-168.75},null,null,"*",{"$f":"+I475","v":5.625},null,"+",{"$f":"+T472","v":303.75},null,null,"=",{"$f":"+F475*I475^2/L475+N475*R475+U475","v":-170.859375},null,null,"KNm"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"x=",{"$f":"+AQ478","v":0},null,null,"m. ' deki max moment miktarı"]
[null,null,"Mmax =",null,null,{"$f":"+E472","v":30},null,"*",{"$f":"+D477","v":0},null,"² /",2,"+",{"$f":"+M472","v":-168.75},null,null,"*",{"$f":"+I478","v":0},null,"+",{"$f":"+T472","v":303.75},null,null,"=",{"$f":"+F478*I478^2/L478+N478*R478+U478","v":303.75},null,null,"KNm",null,null,null,null,null,null,null,null,0,null,{"$f":"ABS(P438)","v":303.75},null,{"$f":"MAX(AM478:AN479)","v":303.75},null,{"$f":"INDEX(AK478:AK479,MATCH(AO478,AM478:AM479,0),0)","v":0}]
[null,null,"L / 2 =",null,{"$f":"+AC442/2","v":4.5},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"U441/AC434","v":5.625},null,{"$f":"ABS(E472*AK479^2/K472+M472*AK479+T472)","v":170.859375}]
[null,null,"MB =",null,{"$f":"+F478","v":30},null,"*",{"$f":"+E479","v":4.5},null,"² /",2,"+",{"$f":"+N478","v":-168.75},null,null,"*",{"$f":"+H480","v":4.5},null,"+",{"$f":"+U478","v":303.75},null,null,"=",{"$f":"+E480*H480^2/K480+M480*Q480+T480","v":-151.875},null,null,"KNm"]
[null,null,"L / 4 =",null,{"$f":"+AC442/4","v":2.25},null,null,"m. ' deki moment miktarı"]
[null,null,"MA =",null,{"$f":"+E480","v":30},null,"*",{"$f":"+E481","v":2.25},null,"² /",2,"+",{"$f":"+M480","v":-168.75},null,null,"*",{"$f":"+H482","v":2.25},null,"+",{"$f":"+T480","v":303.75},null,null,"=",{"$f":"+E482*H482^2/K482+M482*Q482+T482","v":0},null,null,"KNm"]
[null,null,"3 * L / 4 =",null,null,{"$f":"3*AC442/4","v":6.75},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,{"$f":"+E482","v":30},null,"*",{"$f":"+F483","v":6.75},null,"² /",2,"+",{"$f":"+M482","v":-168.75},null,null,"*",{"$f":"+H484","v":6.75},null,"+",{"$f":"+T482","v":303.75},null,null,"=",{"$f":"+E484*H484^2/K484+M484*Q484+T484","v":-151.875},null,null,"KNm"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(Y478)","v":303.75},null,null," /(",2.5,null,"*",{"$f":"+H486","v":303.75},null,null,"+",3,"*",{"$f":"ABS(X482)","v":0},null,null,"+",4,"*",{"$f":"ABS(X480)","v":151.875},null,null,"+",3,"*",{"$f":"ABS(X484)","v":151.875},null,null,")=",{"$f":"E486*H486/(L486*O486+S486*U486+Y486*AA486+AE486*AG486)","v":2.0833333333333335}]
[]
[]
[null,"YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI (enkesiti simetrik olmayan)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,90,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w =",null,12,null,"KN/m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,"y",null,{"$f":"+J497","v":15}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,15,null,"mm",null,null,null,{"$f":"+J497","v":15},null,null,null,{"$f":"+F501/2","v":200},null,null,null,null,null,"A=",{"$f":"+AK501","v":42},null,"KN",null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+AK501","v":42},null,"KN",null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",7,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MESNET TEPKİLERİ VE AÇIKLIK MOMENTİ"]
[null,null,null,null,null,400,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A = B = w * L / 2 =",null,null,null,null,null,{"$f":"+AJ491","v":12},null,"*",{"$f":"+AH498","v":7},null," /",2,"=",{"$f":"AC501*AF501/AI501","v":42},null,null,"KN"]
[null,null,null,null,null,null,null,"x",null,null,null,null,"ağr.mrkz.",null,null,null,"x",null,null,null,null,null,"Mmax = w * L² / 8 =",null,null,null,null,null,{"$f":"+AJ491","v":12},null,"*",{"$f":"+AH498","v":7},null,"² /",8,"=",{"$f":"AC502*AF502^2/AI502","v":73.5},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ARA KESİT TESİRLERİ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+J497","v":15},null,null,null,null,null,null,"x=",2,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(X504<=AH498,\"\",\"azalt.\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mx = w * L * x / 2 - w * x² / 2 =",null,null,null,null,null,null,null,null,{"$f":"+AJ491","v":12},null,"*",{"$f":"+AH498","v":7},null,"*",{"$f":"+X504","v":2},null," /",2,"-",{"$f":"+AJ491","v":12},null,"*",{"$f":"+X504","v":2},null,"² /",2,"=",{"$f":"AF505*AI505*AL505/AO505-AQ505*AT505^2/AW505","v":60},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+F501/2","v":200},null,null,"Vx = w * L / 2 - w * x / 2 =",null,null,null,null,null,null,null,{"$f":"+AJ491","v":12},null,"*",{"$f":"+AH498","v":7},null," /",2,"-",{"$f":"+AJ491","v":12},null,"*",{"$f":"+X504","v":2},null,"=",{"$f":"+AE506*AH506/AK506-AM506*AP506","v":18},null,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+AH498/2","v":3.5},null,null,"m. ' deki max moment miktarı"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+R494","v":22},null,null,null,null,"Max =",null,{"$f":"+AJ491","v":12},null,"*",{"$f":"+AH498","v":7},null,"*",{"$f":"+X508","v":3.5},null," /",2,"-",{"$f":"+AJ491","v":12},null,"*",{"$f":"+X508","v":3.5},null,"² /",2,null,"=",{"$f":"Y509*AB509*AE509/AH509-AJ509*AM509^2/AP509","v":73.5},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+J497","v":15},null,null,null,null,null,null,null,null,null,"L / 2 =",null,{"$f":"+AH498/2","v":3.5},null,null,"m. ' deki moment miktarı"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MB = Max =",null,null,null,{"$f":"+AS509","v":73.5},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L / 4 =",null,{"$f":"+AH498/4","v":1.75},null,null,"m. ' deki moment miktarı"]
[null,null,null,null,null,null,null,null,{"$f":"+BG521","v":21.329787234042552},null,null,null,{"$f":"+L491-I513","v":68.670212765957444},null,null,null,null,null,null,null,null,null,"MA =",null,{"$f":"+Y509","v":12},null,"*",{"$f":"+AB509","v":7},null,"*",{"$f":"+Y512","v":1.75},null," /",2,"-",{"$f":"+AJ509","v":12},null,"*",{"$f":"+Y512","v":1.75},null,"² /",2,null,"=",{"$f":"Y513*AB513*AE513/AH513-AJ513*AM513^2/AP513","v":55.125},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 * L / 4 =",null,null,{"$f":"3*AH498/4","v":5.25},null,null,"m. ' deki moment miktarı"]
[null,null,null,null,null,null,null,null,null,null,"y",null,null,null,null,null,null,null,null,null,null,null,"MC =",null,{"$f":"+Y513","v":12},null,"*",{"$f":"+AB513","v":7},null,"*",{"$f":"+Z514","v":5.25},null," /",2,"-",{"$f":"+AJ513","v":12},null,"*",{"$f":"+Z514","v":5.25},null,"² /",2,null,"=",{"$f":"Y515*AB515*AE515/AH515-AJ515*AM515^2/AP515","v":55.125},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,12.5,null,"*",{"$f":"+AS509","v":73.5},null,null," /(",2.5,null,"*",{"$f":"+AB517","v":73.5},null,null,"+",3,"*",{"$f":"+AS513","v":55.125},null,null,"+",4,"*",{"$f":"+AA511","v":73.5},null,null,"+",3,"*",{"$f":"+AS515","v":55.125},null,null,")=",{"$f":"Y517*AB517/(AF517*AI517+AM517*AO517+AS517*AU517+AY517*BA517)","v":1.1363636363636365}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEHİM HESABI (açıklık ortasında)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aalan =",null,null,{"$f":"+F501-2*M493","v":370},null,"*",{"$f":"+J497","v":15},null,"+",2,"*(",{"$f":"+L491","v":90},null,"*",{"$f":"+M493","v":15},null,"+",{"$f":"+R494-M493","v":7},null,"*",{"$f":"+P497","v":15},null,")=",{"$f":"Z520*AC520+AF520*(AH520*AK520+AN520*AQ520)","v":8460},null,null,"mm²"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = (",null,{"$f":"+F501-2*M493","v":370},null,"*",{"$f":"+J497","v":15},null,"*",{"$f":"+J497/2","v":7.5},null,"+",2,"*(",{"$f":"+L491","v":90},null,"*",{"$f":"+M493","v":15},null,"*",{"$f":"+L491/2","v":45},null,"+",{"$f":"+R494-M493","v":7},null,"*",{"$f":"+P497","v":15},null,"*",{"$f":"+L491-P497/2","v":82.5},null,") ) /",null,{"$f":"+AT520","v":8460},null,null,"=",{"$f":"(Y521*AB521*AE521+AH521*(AJ521*AM521*AP521+AS521*AV521*AY521))/BC521","v":21.329787234042552},null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"+L491","v":90},null,"*",{"$f":"+F501","v":400},null,"3/",12,null,"-",{"$f":"+L491-2*P497","v":60},null,"*",{"$f":"+F501-2*M493","v":370},null,"3/",12,null,"-",{"$f":"+P497","v":15},null,"*",{"$f":"+F501-2*R494","v":356},null,"3/",12,null,"=",{"$f":"Y522*AB522^3/AE522-AH522*AK522^3/AN522-AQ522*AT522^3/AW522","v":170337480},null,null,null,"mm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y = 5 * w * L4 / ( 384 * E * Ix ) =",null,null,null,null,null,null,null,null,null,5,"*",{"$f":"+AJ491","v":12},null,"*",{"$f":"+AH498*1000","v":7000},null,null,"4/(",384,null,"*",{"$f":"+Y519","v":200000},null,null,null,"*",{"$f":"+AZ522","v":170337480},null,null,null,")=",{"$f":"AG523*AI523*AL523^4/(AP523*AS523*AX523)","v":11.012146299217296},null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"+AH498*1000","v":7000},null,null," /",300,null,"=",{"$f":"+AB524/AF524","v":23.333333333333332},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y=",{"$f":"+BC523","v":11.012146299217296},null,null,"mm",null,{"$f":"IF(X525<AG525,\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+AI524","v":23.333333333333332},null,null,"mm",null,{"$f":"IF(X525<AG525,\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI (enkesiti simetrik olmayan)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,83,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w =",null,10,null,"KN/m"]
[null,null,null,null,"mm",null,null,null,null,null,null,null,null,null,"y",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,{"$f":"+N536","v":15}]
[null,null,null,null,22]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,{"$f":"+BY561","v":202.75985663082437},null,null,null,null,{"$f":"+J532","v":15},null,null,null,null,null,15,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+AN540","v":25},null,"KN",null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+AN540","v":25},null,"KN",null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",5,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MESNET TEPKİLERİ VE AÇIKLIK MOMENTİ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,null,"A = B = w * L / 2 =",null,null,null,null,null,{"$f":"+AM530","v":10},null,"*",{"$f":"+AK537","v":5},null," /",2,"=",{"$f":"AF540*AI540/AL540","v":25},null,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mmax = w * L² / 8 =",null,null,null,null,null,{"$f":"+AM530","v":10},null,"*",{"$f":"+AK537","v":5},null,"² /",8,"=",{"$f":"AF541*AI541^2/AL541","v":31.25},null,null,"KNm"]
[null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,"ARA KESİT TESİRLERİ"]
[null,null,null,null,null,null,null,null,"ağr.mrkz.",null,null,null,null,null,null,null,null,null,null,{"$f":"+N536","v":15},null,null,null,null,null,"x=",2,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AA543<=AK537,\"\",\"azalt.\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mx = w * L * x / 2 - w * x² / 2 =",null,null,null,null,null,null,null,null,{"$f":"+AM530","v":10},null,"*",{"$f":"+AK537","v":5},null,"*",{"$f":"+AA543","v":2},null," /",2,"-",{"$f":"+AM530","v":10},null,"*",{"$f":"+AA543","v":2},null,"² /",2,"=",{"$f":"AI544*AL544*AO544/AR544-AT544*AW544^2/AZ544","v":30},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vx = w * L / 2 - w * x / 2 =",null,null,null,null,null,null,null,{"$f":"+AM530","v":10},null,"*",{"$f":"+AK537","v":5},null," /",2,"-",{"$f":"+AM530","v":10},null,"*",{"$f":"+AA543","v":2},null,"=",{"$f":"+AH545*AK545/AN545-AP545*AS545","v":5},null,null,"KN"]
[null,null,{"$f":"+X540-C536","v":197.24014336917563},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+AK537/2","v":2.5},null,null,"m. ' deki max moment miktarı"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+E533","v":22},null,null,null,"Max =",null,{"$f":"+AM530","v":10},null,"*",{"$f":"+AK537","v":5},null,"*",{"$f":"+AA547","v":2.5},null," /",2,"-",{"$f":"+AM530","v":10},null,"*",{"$f":"+AA547","v":2.5},null,"² /",2,null,"=",{"$f":"AB548*AE548*AH548/AK548-AM548*AP548^2/AS548","v":31.25},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+N536","v":15},null,null,null,null,null,null,null,null,"L / 2 =",null,{"$f":"+AK537/2","v":2.5},null,null,"m. ' deki moment miktarı"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MB = Max =",null,null,null,{"$f":"+AV548","v":31.25},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y",null,null,null,null,null,null,null,null,null,null,"L / 4 =",null,{"$f":"+AK537/4","v":1.25},null,null,"m. ' deki moment miktarı"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,91,null,"mm",null,null,null,null,null,null,null,"MA =",null,{"$f":"+AB548","v":10},null,"*",{"$f":"+AE548","v":5},null,"*",{"$f":"+AB551","v":1.25},null," /",2,"-",{"$f":"+AM548","v":10},null,"*",{"$f":"+AB551","v":1.25},null,"² /",2,null,"=",{"$f":"AB552*AE552*AH552/AK552-AM552*AP552^2/AS552","v":23.4375},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 * L / 4 =",null,null,{"$f":"3*AK537/4","v":3.75},null,null,"m. ' deki moment miktarı"]
[null,null,null,null,null,null,null,null,null,{"$f":"+BY560","v":76.740143369175627},null,null,null,null,null,null,{"$f":"+J530+P552-N536-J554","v":82.259856630824373},null,null,null,null,null,null,null,null,"MC =",null,{"$f":"+AB552","v":10},null,"*",{"$f":"+AE552","v":5},null,"*",{"$f":"+AC553","v":3.75},null," /",2,"-",{"$f":"+AM552","v":10},null,"*",{"$f":"+AC553","v":3.75},null,"² /",2,null,"=",{"$f":"AB554*AE554*AH554/AK554-AM554*AP554^2/AS554","v":23.4375},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,12.5,null,"*",{"$f":"+AV548","v":31.25},null,null," /(",2.5,null,"*",{"$f":"+AE556","v":31.25},null,null,"+",3,"*",{"$f":"+AV552","v":23.4375},null,null,"+",4,"*",{"$f":"+AD550","v":31.25},null,null,"+",3,"*",{"$f":"+AV554","v":23.4375},null,null,")=",{"$f":"AB556*AE556/(AI556*AL556+AP556*AR556+AV556*AX556+BB556*BD556)","v":1.1363636363636365}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEHİM HESABI (açıklık ortasında)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Aalan =",null,null,{"$f":"+X540","v":400},null,"*",{"$f":"+N536","v":15},null,"+",{"$f":"+J530-2*N536","v":53},null,"*",{"$f":"+J532","v":15},null,"+",{"$f":"+E533","v":22},null,"*",{"$f":"+H536","v":15},null,"+",{"$f":"+P552-2*T543","v":61},null,"*",{"$f":"+Q549","v":15},null,"+",{"$f":"+V548","v":22},null,"*",{"$f":"+T543","v":15},null,"=",{"$f":"AC559*AF559+AI559*AL559+AO559*AR559+AU559*AX559+BA559*BD559","v":8370},null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = (",null,{"$f":"+X540","v":400},null,"*",{"$f":"+N536","v":15},null,"*",{"$f":"+J530-N536/2","v":75.5},null,"+",{"$f":"+J530-2*N536","v":53},null,"*",{"$f":"+J532","v":15},null,"*",{"$f":"+H536+(J530-2*N536)/2","v":41.5},null,"+",{"$f":"+E533","v":22},null,"*",{"$f":"+H536","v":15},null,"*",{"$f":"+H536/2","v":7.5},null,"+",{"$f":"+P552-2*T543","v":61},null,"*",{"$f":"+Q549","v":15},null,"*",{"$f":"+J530+(P552-2*T543)/2","v":113.5},null,"+",{"$f":"+V548","v":22},null,"*",{"$f":"+T543","v":15},null,"*",{"$f":"+J530-N536+P552-T543/2","v":151.5},null,")/",{"$f":"+BG559","v":8370},null,null,"=",{"$f":"(AB560*AE560*AH560+AK560*AN560*AQ560+AT560*AW560*AZ560+BC560*BF560*BI560+BL560*BO560*BR560)/BU560","v":76.740143369175627},null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y = (",null,{"$f":"+AB560","v":400},null,"*",{"$f":"+AE560","v":15},null,"*",{"$f":"+X540/2","v":200},null,"+",{"$f":"+AK560","v":53},null,"*",{"$f":"+AN560","v":15},null,"*",{"$f":"+J532/2","v":7.5},null,"+",{"$f":"+AT560","v":22},null,"*",{"$f":"+AW560","v":15},null,"*",{"$f":"+E533/2","v":11},null,"+",{"$f":"+BC560","v":61},null,"*",{"$f":"+BF560","v":15},null,"*",{"$f":"+X540-Q549/2","v":392.5},null,"+",{"$f":"+BL560","v":22},null,"*",{"$f":"+BO560","v":15},null,"*",{"$f":"+X540-V548/2","v":389},null,")/",{"$f":"+BU560","v":8370},null,null,"=",{"$f":"(AB561*AE561*AH561+AK561*AN561*AQ561+AT561*AW561*AZ561+BC561*BF561*BI561+BL561*BO561*BR561)/BU561","v":202.75985663082437},null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"+N536","v":15},null,"*",{"$f":"+X540","v":400},null,"3/",12,null,"+",{"$f":"+AB562","v":15},null,"*",{"$f":"+AE562","v":400},null,"*",{"$f":"+C536-X540/2","v":2.7598566308243733},null,"²+",{"$f":"+J530-2*N536","v":53},null,"*",{"$f":"+J532","v":15},null,"3/",12,null,"+",{"$f":"+AT562","v":53},null,"*",{"$f":"+AW562","v":15},null,"*",{"$f":"+C536-J532/2","v":195.25985663082437},null,"²+"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+",{"$f":"+H536","v":15},null,"*",{"$f":"+E533","v":22},null,"3/",12,null,"+",15,null,"*",22,null,"*",{"$f":"+C536-E533/2","v":191.75985663082437},null,"²+",{"$f":"+P552-2*N536","v":61},null,"*",{"$f":"+Q549","v":15},null,"3/",12,null,"+",{"$f":"+AT563","v":61},null,"*",{"$f":"+AW563","v":15},null,"*",{"$f":"+C546-Q549/2","v":189.74014336917563},null,"²+"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+",{"$f":"+T543","v":15},null,"*",{"$f":"+V548","v":22},null,"3/",12,null,"+",15,null,"*",22,null,"*",{"$f":"+C546-V548/2","v":186.24014336917563},null,"²=",{"$f":"AB562*AE562^3/AH562+AK562*AN562*AQ562^2+AT562*AW562^3/AZ562+BC562*BF562*BI562^2+AB563*AE563^3/AH563+AK563*AN563*AQ563^2+AT563*AW563^3/AZ563+BC563*BF563*BI563^2+AB564*AE564^3/AH564+AK564*AN564*AQ564^2","v":166936977.31182796},null,null,null,null,"mm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Iy =",null,{"$f":"+AE562","v":400},null,"*",{"$f":"+AB562","v":15},null,"3/",12,null,"+",400,null,"*",15,null,"*",{"$f":"+J554-J530+N536/2","v":1.2401433691756267},null,"²+",{"$f":"+AW562","v":15},null,"*",{"$f":"+AT562","v":53},null,"3/",12,null,"+",{"$f":"+AT565","v":15},null,"*",{"$f":"+AW565","v":53},null,"*",{"$f":"+J554-H536-(J530-2*N536)/2","v":35.240143369175627},null,"²+"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+",{"$f":"+AE563","v":22},null,"*",{"$f":"+AB563","v":15},null,"3/",12,null,"+",22,null,"*",15,null,"*",{"$f":"+J554-H536/2","v":69.240143369175627},null,"²+",{"$f":"+AW563","v":15},null,"*",{"$f":"+AT563","v":61},null,"3/",12,null,"+",{"$f":"+AT566","v":15},null,"*",{"$f":"+AW566","v":61},null,"*",{"$f":"+Q554-T543-(P552-2*T543)/2","v":36.759856630824373},null,"²+"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+",{"$f":"+AE564","v":22},null,"*",{"$f":"+AB564","v":15},null,"3/",12,null,"+",22,null,"*",15,null,"*",{"$f":"+Q554-T543/2","v":74.759856630824373},null,"²=",{"$f":"AB565*AE565^3/AH565+AK565*AN565*AQ565^2+AT565*AW565^3/AZ565+BC565*BF565*BI565^2+AB566*AE566^3/AH566+AK566*AN566*AQ566^2+AT566*AW566^3/AZ566+BC566*BF566*BI566^2+AB567*AE567^3/AH567+AK567*AN567*AQ567^2","v":6254104.8118279567},null,null,null,null,"mm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ixy =",null,{"$f":"+X540","v":400},null,"*",{"$f":"+N536","v":15},null,"*",{"$f":"-(C536-X540/2)","v":-2.7598566308243733},null,"*",{"$f":"+J554-J530+N536/2","v":1.2401433691756267},null,"+",{"$f":"+J530-2*N536","v":53},null,"*",{"$f":"+J532","v":15},null,"*",{"$f":"-(C536-J532/2)","v":-195.25985663082437},null,"*",{"$f":"+J554-H536-(J530-2*N536)/2","v":35.240143369175627},null,"+",{"$f":"+E533","v":22},null,"*",{"$f":"+H536","v":15},null,"*",{"$f":"-(C536-E533/2)","v":-191.75985663082437},null,"*",{"$f":"+J554-H536/2","v":69.240143369175627},null,"+",{"$f":"+P552-2*Q549","v":61},null,"*",{"$f":"+Q549","v":15},null,"*",{"$f":"(C546-Q549/2)","v":189.74014336917563},null,"*",{"$f":"-(Q554-T543-(P552-2*T543)/2)","v":-36.759856630824373},null,"+"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+",{"$f":"+V548","v":22},null,"*",{"$f":"+T543","v":15},null,"*",{"$f":"(C546-V548/2)","v":186.24014336917563},null,"*",{"$f":"-(Q554-T543/2)","v":-74.759856630824373},null,"=",{"$f":"AB568*AE568*AH568*AK568+AN568*AQ568*AT568*AW568+AZ568*BC568*BF568*BI568+BL568*BO568*BR568*BU568+AB569*AE569*AH569*AK569","v":-20849132.688172042},null,null,null,null,"mm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"a = Iy / ( E * ( Ix * Iy - Ixy² ) ) =",null,null,null,null,null,null,null,null,{"$f":"+AT567","v":6254104.8118279567},null,null,null," /(",{"$f":"+AB558","v":200000},null,null,null,"*(",{"$f":"+AT564","v":166936977.31182796},null,null,null,"*",{"$f":"+AT567","v":6254104.8118279567},null,null,null,"-",{"$f":"+AN569","v":-20849132.688172042},null,null,null,null,"² ) ) =",null,{"$f":"AI570/(AN570*(AS570*AX570-BC570^2))","v":5.1317414433887717E-14}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"b = Ixy / ( E * ( Ix * Iy - Ixy² ) ) =",null,null,null,null,null,null,null,null,null,{"$f":"+AN569","v":-20849132.688172042},null,null,null,null," /(",{"$f":"+AN570","v":200000},null,null,null,"*(",{"$f":"+AS570","v":166936977.31182796},null,null,null,"*",{"$f":"+AX570","v":6254104.8118279567},null,null,null,"-",{"$f":"+BC570","v":-20849132.688172042},null,null,null,null,"² ) ) =",null,{"$f":"AJ571/(AP571*(AU571*AZ571-BE571^2))","v":-1.7107541605675806E-13}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y = 5 * b * w * L4 / 384 =",null,null,null,null,null,null,null,-5,"*",{"$f":"BL571","v":-1.7107541605675806E-13},null,null,"*",{"$f":"+AM530","v":10},null,"*",{"$f":"+AK537*1000","v":5000},null,null,"4/",384,null,"=",{"$f":"+AH572*AJ572*AN572*AQ572^4/AU572","v":13.922152999410649},null,null,"mm",null,"(düşey sehim)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = 5 * a * w * L4 / 384 =",null,null,null,null,null,null,null,5,"*",{"$f":"+BJ570","v":5.1317414433887717E-14},null,null,"*",{"$f":"+AN572","v":10},null,"*",{"$f":"+AQ572","v":5000},null,null,"4/",384,null,"=",{"$f":"+AH573*AJ573*AN573*AQ573^4/AU573","v":4.1762218777577891},null,null,"mm",null,"(yatay sehim)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ymax = xmax = L / 300 =",null,null,null,null,null,null,null,{"$f":"+AK537*1000","v":5000},null,null," /",300,null,"=",{"$f":"+AH574/AL574","v":16.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y=",{"$f":"+AX572","v":13.922152999410649},null,null,"mm",null,{"$f":"IF(AA575<AJ575,\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+AO574","v":16.666666666666668},null,null,"mm",null,{"$f":"IF(AA575<AJ575,\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+AX573","v":4.1762218777577891},null,null,"mm",null,{"$f":"IF(AA576<AJ576,\"<\",\">\")","v":"<"},"xmax =",null,null,{"$f":"+AJ575","v":16.666666666666668},null,null,"mm",null,{"$f":"IF(AA576<AJ576,\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI (enkesiti simetrik olmayan)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,{"$f":"+BC610","v":68.067010309278345},null,null,null,{"$f":"+M595-J581","v":181.93298969072166},null,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w =",null,25,null,"KN/m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x"]
[null,null,null,null,null,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+G588-T591","v":145.54639175257734},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,null,null,null,null,null,null,null,15,null,"mm",null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+AK591","v":37.5},null,"KN",null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+AK591","v":37.5},null,"KN",null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,200,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",3,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"ağr.mrkz.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MESNET TEPKİLERİ VE AÇIKLIK MOMENTİ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+BC611","v":54.453608247422679},null,null,"A = B = w * L / 2 =",null,null,null,null,null,{"$f":"+AI581","v":25},null,"*",{"$f":"+AG588","v":3},null," /",2,"=",{"$f":"AC591*AF591/AI591","v":37.5},null,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,12,null,"mm",null,null,null,null,null,null,null,"Mmax = w * L² / 8 =",null,null,null,null,null,{"$f":"+AI581","v":25},null,"*",{"$f":"+AG588","v":3},null,"² /",8,"=",{"$f":"AC592*AF592^2/AI592","v":28.125},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ARA KESİT TESİRLERİ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",2,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(X594<=AG588,\"\",\"azalt.\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,250,null,"mm",null,null,null,null,null,null,null,"Mx = w * L * x / 2 - w * x² / 2 =",null,null,null,null,null,null,null,null,{"$f":"+AI581","v":25},null,"*",{"$f":"+AG588","v":3},null,"*",{"$f":"+X594","v":2},null," /",2,"-",{"$f":"+AI581","v":25},null,"*",{"$f":"+X594","v":2},null,"² /",2,"=",{"$f":"AF595*AI595*AL595/AO595-AQ595*AT595^2/AW595","v":25},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vx = w * L / 2 - w * x / 2 =",null,null,null,null,null,null,null,{"$f":"+AI581","v":25},null,"*",{"$f":"+AG588","v":3},null," /",2,"-",{"$f":"+AI581","v":25},null,"*",{"$f":"+X594","v":2},null,"=",{"$f":"+AE596*AH596/AK596-AM596*AP596","v":-12.5},null,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+AG588/2","v":1.5},null,null,"m. ' deki max moment miktarı"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"+AI581","v":25},null,"*",{"$f":"+AG588","v":3},null,"*",{"$f":"+X598","v":1.5},null," /",2,"-",{"$f":"+AI581","v":25},null,"*",{"$f":"+X598","v":1.5},null,"² /",2,null,"=",{"$f":"Y599*AB599*AE599/AH599-AJ599*AM599^2/AP599","v":28.125},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L / 2 =",null,{"$f":"+AG588/2","v":1.5},null,null,"m. ' deki moment miktarı"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MB = Max =",null,null,null,{"$f":"+AS599","v":28.125},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L / 4 =",null,{"$f":"+AG588/4","v":0.75},null,null,"m. ' deki moment miktarı"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MA =",null,{"$f":"+Y599","v":25},null,"*",{"$f":"+AB599","v":3},null,"*",{"$f":"+Y602","v":0.75},null," /",2,"-",{"$f":"+AJ599","v":25},null,"*",{"$f":"+Y602","v":0.75},null,"² /",2,null,"=",{"$f":"Y603*AB603*AE603/AH603-AJ603*AM603^2/AP603","v":21.09375},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 * L / 4 =",null,null,{"$f":"3*AG588/4","v":2.25},null,null,"m. ' deki moment miktarı"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MC =",null,{"$f":"+Y603","v":25},null,"*",{"$f":"+AB603","v":3},null,"*",{"$f":"+Z604","v":2.25},null," /",2,"-",{"$f":"+AJ603","v":25},null,"*",{"$f":"+Z604","v":2.25},null,"² /",2,null,"=",{"$f":"Y605*AB605*AE605/AH605-AJ605*AM605^2/AP605","v":21.09375},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,12.5,null,"*",{"$f":"+AS599","v":28.125},null,null," /(",2.5,null,"*",{"$f":"+AB607","v":28.125},null,null,"+",3,"*",{"$f":"+AS603","v":21.09375},null,null,"+",4,"*",{"$f":"+AA601","v":28.125},null,null,"+",3,"*",{"$f":"+AS605","v":21.09375},null,null,")=",{"$f":"Y607*AB607/(AF607*AI607+AM607*AO607+AS607*AU607+AY607*BA607)","v":1.1363636363636365}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEHİM HESABI (açıklık ortasında)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = (",null,{"$f":"+G588-M592","v":188},null,"*",{"$f":"+K587","v":15},null,"*",{"$f":"+K587/2","v":7.5},null,"+",{"$f":"+M595","v":250},null,"*",{"$f":"+M592","v":12},null,"*",{"$f":"+M595/2","v":125},null,")/(",{"$f":"+G588-M592","v":188},null,"*",{"$f":"+K587","v":15},null,"+",{"$f":"+M595","v":250},null,"*",{"$f":"+M592","v":12},null,")=",{"$f":"(Y610*AB610*AE610+AH610*AK610*AN610)/(AQ610*AT610+AW610*AZ610)","v":68.067010309278345},null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y = (",null,{"$f":"+Y610","v":188},null,"*",{"$f":"+AB610","v":15},null,"*",{"$f":"(G588-M592)/2+M592","v":106},null,"+",{"$f":"+AH610","v":250},null,"*",{"$f":"+AK610","v":12},null,"*",{"$f":"+M592/2","v":6},null,")/(",{"$f":"+AQ610","v":188},null,"*",{"$f":"+AT610","v":15},null,"+",{"$f":"+AW610","v":250},null,"*",{"$f":"+AZ610","v":12},null,")=",{"$f":"(Y611*AB611*AE611+AH611*AK611*AN611)/(AQ611*AT611+AW611*AZ611)","v":54.453608247422679},null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"+K587","v":15},null,"*",{"$f":"+G588-M592","v":188},null,"3/",12,null,"+",{"$f":"+Y612","v":15},null,"*",{"$f":"+AB612","v":188},null,"*",{"$f":"+T586-(G588-M592)/2","v":51.546391752577335},null,"²+",{"$f":"+M595","v":250},null,"*",{"$f":"+M592","v":12},null,"3/",12,null,"+",{"$f":"+AQ612","v":250},null,"*",{"$f":"+AT612","v":12},null,"*",{"$f":"+T591-M592/2","v":48.453608247422679},null,"²=",{"$f":"Y612*AB612^3/AE612+AH612*AK612*AN612^2+AQ612*AT612^3/AW612+AZ612*BC612*BF612^2","v":22877922.47422681},null,null,null,"mm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Iy =",null,{"$f":"+G588-M592","v":188},null,"*",{"$f":"+K587","v":15},null,"3/",12,null,"+",{"$f":"+Y613","v":188},null,"*",{"$f":"+AB613","v":15},null,"*",{"$f":"+J581-K587/2","v":60.567010309278345},null,"²+",{"$f":"+M592","v":12},null,"*",{"$f":"+M595","v":250},null,"3/",12,null,"+",{"$f":"+AQ613","v":12},null,"*",{"$f":"+AT613","v":250},null,"*",{"$f":"+N581-M595/2","v":56.932989690721655},null,"²=",{"$f":"Y613*AB613^3/AE613+AH613*AK613*AN613^2+AQ613*AT613^3/AW613+AZ613*BC613*BF613^2","v":35746753.865979381},null,null,null,"mm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ixy =",null,{"$f":"+G588-M592","v":188},null,"*",{"$f":"+K587","v":15},null,"*",{"$f":"+J581-K587/2","v":60.567010309278345},null,"*",{"$f":"-(T586-(G588-M592)/2)","v":-51.546391752577335},null,"+",{"$f":"+M595","v":250},null,"*",{"$f":"+M592","v":12},null,"*",{"$f":"+J581-M595/2","v":-56.932989690721655},null,"*",{"$f":"+T591-M592/2","v":48.453608247422679},null,"=",{"$f":"Y614*AB614*AE614*AH614+AK614*AN614*AQ614*AT614","v":-17079896.907216497},null,null,null,"mm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"a = Iy / ( E * ( Ix * Iy - Ixy² ) ) =",null,null,null,null,null,null,null,null,{"$f":"+BI613","v":35746753.865979381},null,null,null," /(",{"$f":"+Y609","v":200000},null,null,null,"*(",{"$f":"+BI612","v":22877922.47422681},null,null,null,"*",{"$f":"+BI613","v":35746753.865979381},null,null,null,"-",{"$f":"+AW614","v":-17079896.907216497},null,null,null,null,"² ) ) =",null,{"$f":"AF615/(AK615*(AP615*AU615-AZ615^2))","v":3.3974082374619861E-13}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"b = Ixy / ( E * ( Ix * Iy - Ixy² ) ) =",null,null,null,null,null,null,null,null,null,{"$f":"+AW614","v":-17079896.907216497},null,null,null,null," /(",{"$f":"+AK615","v":200000},null,null,null,"*(",{"$f":"+AP615","v":22877922.47422681},null,null,null,"*",{"$f":"+AU615","v":35746753.865979381},null,null,null,"-",{"$f":"+AZ615","v":-17079896.907216497},null,null,null,null,"² ) ) =",null,{"$f":"AG616/(AM616*(AR616*AW616-BB616^2))","v":-1.6232909613312942E-13}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y = 5 * b * w * L4 / 384 =",null,null,null,null,null,null,null,-5,"*",{"$f":"BI616","v":-1.6232909613312942E-13},null,null,"*",{"$f":"+AI581","v":25},null,"*",{"$f":"+AG588*1000","v":3000},null,null,"4/",384,null,"=",{"$f":"+AE617*AG617*AK617*AN617^4/AR617","v":4.2801617144477477},null,null,"mm",null,"(düşey sehim)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = 5 * a * w * L4 / 384 =",null,null,null,null,null,null,null,5,"*",{"$f":"+BG615","v":3.3974082374619861E-13},null,null,"*",{"$f":"+AK617","v":25},null,"*",{"$f":"+AN617","v":3000},null,null,"4/",384,null,"=",{"$f":"+AE618*AG618*AK618*AN618^4/AR618","v":8.9580100011204724},null,null,"mm",null,"(yatay sehim)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ymax = xmax = L / 300 =",null,null,null,null,null,null,null,{"$f":"+AG588*1000","v":3000},null,null," /",300,null,"=",{"$f":"+AE619/AI619","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y=",{"$f":"+AU617","v":4.2801617144477477},null,null,"mm",null,{"$f":"IF(X620<AG620,\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+AL619","v":10},null,null,"mm",null,{"$f":"IF(X620<AG620,\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x=",{"$f":"+AU618","v":8.9580100011204724},null,null,"mm",null,{"$f":"IF(X621<AG621,\"<\",\">\")","v":"<"},"xmax =",null,null,{"$f":"+AG620","v":10},null,null,"mm",null,{"$f":"IF(X621<AG621,\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK TEK AÇIKLIKLI KONSOLLU KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,"(1.ci bölge)",null,null,null,null,null,null,null,"(2.ci bölge)",null,null,null,null,"(3.cü bölge)",null,null,null,75,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65,null,"KN",null,null,null,null,null,null,25,null,"KN/m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK677","v":1.1763270769430065},null,null,null,"(1.ci ve 2.ci bölge için)",null,null,null,null,null,null,null,null,null,null,"(3.cü bölge için Cb = 1 alınır.)"]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O627,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"ABS(AC669)","v":325.83263276901664},null,null,"KNm",null,"(max moment)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(AY641),ABS(AZ641),ABS(BA641),ABS(BB641),ABS(BC641),ABS(BD641))","v":226.51785714285714},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O627,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E647","v":223.48214285714286},null,"KN",null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E649","v":339.01785714285711},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O627,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,"m",null,null,null,null,{"$f":"+AC638-Y636","v":5.5},null,"m",null,null,null,null,1.5,null,"m",null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O627,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uygunluk koşulları"]
[null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O627,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(x = L) v2' = (x = L) v3'",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"V635","v":223.48214285714286},{"$f":"+AY641-Z629*Y636","v":140.98214285714286},{"$f":"+AZ641-AC628","v":75.982142857142861},{"$f":"+BA641-Z629*AF636","v":-226.51785714285714},{"$f":"+BB641+AJ635","v":112.49999999999997},{"$f":"+BC641-AL628*AM636","v":74.999999999999972}]
[null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( x = 0) v1 = 0",null,null,null,null,null,null,null,null,null,null,null,"( x = L) v2 = ( x = L) v3 = 0"]
[null,null,"MESNET TEPKİLERİ"]
[null,null,"A","*",{"$f":"+AC638","v":7},null,"-",{"$f":"+Z629","v":55},null,"*",{"$f":"+AC638","v":7},null,"*",{"$f":"+K646/2","v":3.5},null,"-",{"$f":"+AC628","v":65},null,"*",{"$f":"+AF636","v":5.5},null,"+",{"$f":"+AL628","v":25},null,"*",{"$f":"+AM636","v":1.5},null,"*",{"$f":"+Z646/2","v":0.75},null,"+",{"$f":"+AP627","v":75},null,"*",{"$f":"+AM636","v":1.5},null,"=",0]
[null,null,"A","=",{"$f":"(H646*K646*N646+Q646*T646-W646*Z646*AC646-AF646*AI646)/E646","v":223.48214285714286},null,null,"KN"]
[null,null,"A","+","B","-",{"$f":"+Z629","v":55},null,"*",{"$f":"+AC638","v":7},null,"-",{"$f":"+AC628","v":65},null,"-",{"$f":"+AL628","v":25},null,"*",{"$f":"+AM636","v":1.5},null,"-",{"$f":"+AP627","v":75},null,"=",0]
[null,null,"B","=",{"$f":"+G648*J648+M648+P648*S648+V648-E647","v":339.01785714285711},null,null,"KN"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"1.ci bölgede :"]
[null,null,"Mx =",null,{"$f":"+E682","v":223.48214285714286},null,"*","x","-",{"$f":"+J682","v":55},null,"*","x²"," /",2]
[null,null,"x=",1,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D653<=Y636,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+E684","v":223.48214285714286},null,"*",{"$f":"+D653","v":1},null,"-",{"$f":"+J652","v":55},null,"*",{"$f":"+D653","v":1},null,"²/",2,"=",{"$f":"+E654*H654-K654*N654^2/Q654","v":195.98214285714286},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E652","v":223.48214285714286},null,"-",{"$f":"+J652","v":55},null,"*",{"$f":"+D653","v":1},null,"=",{"$f":"+E655","v":223.48214285714286},null,"-",{"$f":"+H655*K655","v":55},null,"=",{"$f":"+N655-Q655","v":168.48214285714286},null,null,"KNm"]
[null,null,"2.ci bölgede :"]
[null,null,"Mx =",null,{"$f":"+E686","v":223.48214285714286},null,"*","x","-",{"$f":"+Z629","v":55},null,"*","x²"," /",2,"-",{"$f":"+AC628","v":65},null,"*(","x","-",{"$f":"+Y636","v":1.5},null,")"]
[null,null,"x=",3,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D658<Y636,\"artır.\",IF(D658>AC638,\"azalt.\",\"\"))","v":""}]
[null,null,"Mx =",null,{"$f":"+E657","v":223.48214285714286},null,"*",{"$f":"+D658","v":3},null,"-",{"$f":"+J657","v":55},null,"*",{"$f":"+D658","v":3},null,"²/",2,"-",{"$f":"+Q657","v":65},null,"*(",{"$f":"+D658","v":3},null,"-",{"$f":"+V657","v":1.5},null,")=",{"$f":"+E659*H659-K659*N659^2/Q659-S659*(V659-Y659)","v":325.44642857142856},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E659","v":223.48214285714286},null,"-",{"$f":"+K659","v":55},null,"*",{"$f":"+N659","v":3},null,"-",{"$f":"+S659","v":65},null,"=",{"$f":"+E660-H660*K660-N660","v":-6.5178571428571388},null,null,"KN"]
[null,null,"3.ci bölgede :"]
[null,null,"Mx =",null,{"$f":"+V635","v":223.48214285714286},null,"*","x","-",{"$f":"+Z629","v":55},null,"*",{"$f":"+AC638","v":7},null,"*(","x","-",{"$f":"+AC638","v":7},null," /",2,")-",{"$f":"+AC628","v":65},null,"*(","x","-",{"$f":"+Y636","v":1.5},null,")+",{"$f":"+AJ635","v":339.01785714285711},null,"*(","x","-",{"$f":"+AC638","v":7},null,")-",{"$f":"+AL628","v":25},null,"*(","x","-",{"$f":"+AC638","v":7},null,")²"," /",2]
[null,null,"x=",8,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D663<AC638,\"artır.\",IF(D663>(AC638+AM636),\"azalt.\",\"\"))","v":""}]
[null,null,"Mx =",null,{"$f":"+E662","v":223.48214285714286},null,"*",{"$f":"+D663","v":8},null,"-",{"$f":"+J662","v":55},null,"*",{"$f":"+AC638","v":7},null,"*(",{"$f":"+D663","v":8},null,"-",{"$f":"+R662","v":7},null," /",2,")-",{"$f":"+W662","v":65},null,"*(",{"$f":"+D663","v":8},null,"-",{"$f":"+AB662","v":1.5},null,")+",{"$f":"+AE662","v":339.01785714285711},null,"*(",{"$f":"+AB664","v":8},null,"-",{"$f":"+AJ662","v":7},null,")-",{"$f":"+AM662","v":25},null,"*(",{"$f":"+AK664","v":8},null,"-",{"$f":"+AR662","v":7},null,")²"," /",2,"=",{"$f":"E664*H664-K664*N664*(Q664-T664/W664)-Y664*(AB664-AE664)+AH664*(AK664-AN664)-AQ664*(AT664-AW664)^2/BA664","v":-40.625},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E664","v":223.48214285714286},null,"-",{"$f":"+K664","v":55},null,"*",{"$f":"+N664","v":7},null,"-",{"$f":"+Y664","v":65},null,"+",{"$f":"+AH664","v":339.01785714285711},null,"-",{"$f":"+AQ664","v":25},null,"*",{"$f":"+D663-AC638","v":1},null,"=",{"$f":"+E665-H665*K665-N665+Q665-T665*W665","v":87.499999999999972},null,null,"KN"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"1.ve 2.ci bölgede :",null,null,null,null,null,null,null,null,null,null,null,null,null,"x1=",null,{"$f":"V635/Z629","v":4.0633116883116882},null,"m",null,"M1 =",null,{"$f":"V635*S667-Z629*S667*S667/2","v":454.03880160018554},null,"KNm",null,null,{"$f":"IF(S667<Y636,S667,S668)","v":2.8814935064935066},null,{"$f":"INDEX(Y667:Y668,MATCH(AD667,S667:S668,0),0)","v":325.83263276901675}]
[null,null,"x=",{"$f":"IF(AF667<AF668,AD668,AD667)","v":2.8814935064935066},null,null,"m. ' deki max moment miktarı",null,null,null,null,null,null,null,null,null,"x2=",null,{"$f":"(V635-AC628)/Z629","v":2.8814935064935066},null,"m",null,"M2 =",null,{"$f":"V635*S668-Z629*S668*S668/2-AC628*(S668-Y636)","v":325.83263276901675},null,"KNm",null,null,{"$f":"+AC638","v":7},null,{"$f":"AP627*AM636+AL628*AM636*AM636/2","v":140.625}]
[null,null,"Mmax =",null,null,{"$f":"+E654","v":223.48214285714286},null,"*",{"$f":"+D668","v":2.8814935064935066},null,"-",{"$f":"+K654","v":55},null,"*",{"$f":"+D668","v":2.8814935064935066},null,"²/",2,"-",{"$f":"IF((W669-Z669)<0,0,AC628)","v":65},null,"*(",{"$f":"+I669","v":2.8814935064935066},null,"-",{"$f":"+Y636","v":1.5},null,")=",{"$f":"+F669*I669-L669*O669^2/R669-T669*(W669-Z669)","v":325.83263276901664},null,null,"KNm"]
[null,null,"L / 2 =",null,{"$f":"+AC638/2","v":3.5},null,null,"m. ' deki moment miktarı"]
[null,null,"MB =",null,null,{"$f":"+F669","v":223.48214285714286},null,"*",{"$f":"+E670","v":3.5},null,"-",{"$f":"+L669","v":55},null,"*",{"$f":"+E670","v":3.5},null,"²/",2,"-",{"$f":"IF((W671-Z671)<0,0,AC628)","v":65},null,"*(",{"$f":"+I671","v":3.5},null,"-",{"$f":"+Z669","v":1.5},null,")=",{"$f":"+F671*I671-L671*O671^2/R671-T671*(W671-Z671)","v":315.3125},null,null,"KNm"]
[null,null,"L / 4 =",null,{"$f":"+AC638/4","v":1.75},null,null,"m. ' deki moment miktarı"]
[null,null,"MA =",null,null,{"$f":"+F671","v":223.48214285714286},null,"*",{"$f":"+E672","v":1.75},null,"-",{"$f":"+L671","v":55},null,"*",{"$f":"+E672","v":1.75},null,"²/",2,"-",{"$f":"IF((W673-Z673)<0,0,AC628)","v":65},null,"*(",{"$f":"+I673","v":1.75},null,"-",{"$f":"+Z671","v":1.5},null,")=",{"$f":"+F673*I673-L673*O673^2/R673-T673*(W673-Z673)","v":290.625},null,null,"KNm"]
[null,null,"3 * L / 4 =",null,null,{"$f":"3*AC638/4","v":5.25},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,null,{"$f":"+F673","v":223.48214285714286},null,"*",{"$f":"+F674","v":5.25},null,"-",{"$f":"+L673","v":55},null,"*",{"$f":"+F674","v":5.25},null,"²/",2,"-",{"$f":"IF((W675-Z675)<0,0,AC628)","v":65},null,"*(",{"$f":"+I675","v":5.25},null,"-",{"$f":"+Z673","v":1.5},null,")=",{"$f":"+F675*I675-L675*O675^2/R675-T675*(W675-Z675)","v":171.5625},null,null,"KNm"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AC669)","v":325.83263276901664},null,null," /(",2.5,null,"*",{"$f":"+H677","v":325.83263276901664},null,null,"+",3,"*",{"$f":"ABS(AC673)","v":290.625},null,null,"+",4,"*",{"$f":"ABS(AC671)","v":315.3125},null,null,"+",3,"*",{"$f":"ABS(AC675)","v":171.5625},null,null,")=",{"$f":"E677*H677/(L677*O677+S677*U677+Y677*AA677+AE677*AG677)","v":1.1763270769430065}]
[null,null,"3.cü bölgede :"]
[null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca konsol kirişte Cb = 1 alınır."]
[null,null,"SEHİM HESABI"]
[null,null,"1.ci bölgede :"]
[null,null,"v1'' = ",null,{"$f":"+V635","v":223.48214285714286},null,"*","x","-",{"$f":"+Z629","v":55},null,"*","x²"," /",2]
[null,null,"v1' = ",null,{"$f":"+E682","v":223.48214285714286},null,"*","x²"," /",2,"-",{"$f":"+J682","v":55},null,"*","x3"," /",6,"+","C1"]
[null,null,"v1 = ",null,{"$f":"+E683","v":223.48214285714286},null,"*","x3"," /",6,"-",{"$f":"+L683","v":55},null,"*","x4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"2.ci bölgede :"]
[null,null,"v2'' = ",null,{"$f":"+V635","v":223.48214285714286},null,"*","x","-",{"$f":"+Z629","v":55},null,"*","x²"," /",2,"-",{"$f":"+AC628","v":65},null,"*(","x","-",{"$f":"+Y636","v":1.5},null,")"]
[null,null,"v2' = ",null,{"$f":"+E686","v":223.48214285714286},null,"*","x²"," /",2,"-",{"$f":"+J686","v":55},null,"*","x3"," /",6,"-",{"$f":"+Q686","v":65},null,"*(","x","-",{"$f":"+V686","v":1.5},null,")²"," /",2,"+","D1"]
[null,null,"v2 = ",null,{"$f":"+E687","v":223.48214285714286},null,"*","x3"," /",6,"-",{"$f":"+L687","v":55},null,"*","x4"," /",24,null,"-",{"$f":"+S687","v":65},null,"*(","x","-",{"$f":"+X687","v":1.5},null,")3"," /",6,"+","D1","*","x","+","D2"]
[null,null,"3.ci bölgede :"]
[null,null,"v3'' = ",null,{"$f":"+V635","v":223.48214285714286},null,"*","x","-",{"$f":"+Z629","v":55},null,"*",{"$f":"+AC638","v":7},null,"*(","x","-",{"$f":"+AC638","v":7},null," /",2,")-",{"$f":"+AC628","v":65},null,"*(","x","-",{"$f":"+Y636","v":1.5},null,")+",{"$f":"+AJ635","v":339.01785714285711},null,"*(","x","-",{"$f":"+AC638","v":7},null,")-",{"$f":"AL628","v":25},null,"*(","x","-",{"$f":"+AC638","v":7},null,")²"," /",2]
[null,null,"v3' = ",null,{"$f":"+E690","v":223.48214285714286},null,"*","x²"," /",2,"-",{"$f":"+J690*M690","v":385},null,"*(","x","-",{"$f":"+R690/U690","v":3.5},null,")²"," /",2,"-",{"$f":"+W690","v":65},null,"*(","x","-",{"$f":"+AB690","v":1.5},null,")²"," /",2,"+",{"$f":"+AE690","v":339.01785714285711},null,"*(","x","-",{"$f":"+AJ690","v":7},null,")²"," /",2,"-",{"$f":"+AM690","v":25},null,"*(","x","-",{"$f":"+AR690","v":7},null,")3"," /",6,"+","E1"]
[null,null,"v3 = ",null,{"$f":"+E691","v":223.48214285714286},null,"*","x3"," /",6,"-",{"$f":"+L691","v":385},null,"*(","x","-",{"$f":"+Q691","v":3.5},null,")3"," /",6,"-",{"$f":"+W691","v":65},null,"*(","x","-",{"$f":"+AB691","v":1.5},null,")3"," /",6,"+",{"$f":"+AH691","v":339.01785714285711},null,"*(","x","-",{"$f":"+AM691","v":7},null,")3"," /",6,"-",{"$f":"+AS691","v":25},null,"*(","x","-",{"$f":"+AX691","v":7},null,")4"," /",24,null,"+","E1","*","x","+","E2"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"x = 0 ; v1 = 0",null,null,null,null,null,"C2","=",0]
[null,null,"x = L ; v2 = 0",null,null,null,null,null,{"$f":"+E688","v":223.48214285714286},null,"*",{"$f":"+AC638","v":7},null,"3/",{"$f":"+J688","v":6},"-",{"$f":"+L688","v":55},null,"*",{"$f":"+L695","v":7},null,"4/",{"$f":"+Q688","v":24},null,"-",{"$f":"+T688","v":65},null,"*(",{"$f":"+T695","v":7},null,"-",{"$f":"+Y688","v":1.5},null,")3"," /",{"$f":"+AC688","v":6},"+","D1","*",{"$f":"+AC695","v":7},null,"+","D2","=",0,null,null,{"$f":"I695*L695^3/O695-Q695*T695^4/W695-Z695*(AC695-AF695)^3/AJ695","v":5471.0416666666661},null,null,"+","D1","*",{"$f":"+AN695","v":7},null,"+","D2","=",0,null,"(1.denklem)"]
[null,null,"x = L ; v3 = 0",null,null,null,null,null,{"$f":"+E692","v":223.48214285714286},null,"*",{"$f":"+AC638","v":7},null,"3/",{"$f":"+J692","v":6},"-",{"$f":"+L692","v":385},null,"*(",{"$f":"+L696","v":7},null,"-",{"$f":"+Q692","v":3.5},null,")3"," /",6,"-",{"$f":"+W692","v":65},null,"*(",{"$f":"+T696","v":7},null,"-",{"$f":"+AB692","v":1.5},null,")3"," /",{"$f":"+AF692","v":6},"+",{"$f":"+AH692","v":339.01785714285711},null,"*(",{"$f":"+AF696","v":7},null,"-",{"$f":"+AM692","v":7},null,")3"," /",6,"-",{"$f":"+AS692","v":25},null,"*(",{"$f":"+AR696","v":7},null,"-",{"$f":"+AX692","v":7},null,")4"," /",24,null,"+","E1","*",{"$f":"+BD696","v":7},null,"+","E2"]
[null,null,null,null,null,{"$f":"I696*L696^3/O696-Q696*(T696-W696)^3/AA696-AC696*(AF696-AI696)^3/AM696+AO696*(AR696-AU696)^3/AY696-BA696*(BD696-BG696)^4/BK696","v":8222.1874999999982},null,null,"+","E1","*",{"$f":"+BP696","v":7},null,"+","E2","=",0,null,"(2.denklem)"]
[null,null,"x = L ; v2' =",null,null,null,{"$f":"+E687","v":223.48214285714286},null,"*",{"$f":"+AC638","v":7},null,"² /",2,"-",{"$f":"+L687","v":55},null,"*",{"$f":"+J698","v":7},null,"3 /",{"$f":"+Q687","v":6},"-",{"$f":"+S687","v":65},null,"*(",{"$f":"+R698","v":7},null,"-",{"$f":"+X687","v":1.5},null,")²"," /",2,"+","D1","=","D1","+",{"$f":"G698*J698^2/M698-O698*R698^3/U698-W698*(Z698-AC698)^2/AG698","v":1348.0208333333335}]
[null,null,"x = L ; v3' =",null,null,null,{"$f":"+E691","v":223.48214285714286},null,"*",{"$f":"+AC638","v":7},null,"² /",{"$f":"+J691","v":2},"-",{"$f":"+L691","v":385},null,"*(",{"$f":"+J699","v":7},null,"-",{"$f":"+Q691","v":3.5},null,")²"," /",2,"-",{"$f":"+W691","v":65},null,"*(",{"$f":"+R699","v":7},null,"-",{"$f":"+AB691","v":1.5},null,")²"," /",{"$f":"+AF691","v":2},"+",{"$f":"+AH691","v":339.01785714285711},null,"*(",{"$f":"+AD699","v":7},null,"-",{"$f":"+AM691","v":7},null,")²"," /",2,"-",{"$f":"+AS691","v":25},null,"*(",{"$f":"+AP699","v":7},null,"-",{"$f":"+AX691","v":7},null,")3"," /",{"$f":"+BB691","v":6},"+","E1","=",{"$f":"G699*J699^2/M699-O699*(R699-U699)^2/Y699-AA699*(AD699-AG699)^2/AK699+AM699*(AP699-AS699)^2/AW699-AY699*(BB699-BE699)^3/BI699","v":2134.0625},null,null,"+","E1"]
[null,null,"(x = L ; v2') = ( x = L ; v3' ) = ",null,null,null,null,null,null,null,null,"D1","+",{"$f":"+AM698","v":1348.0208333333335},null,null,"=",{"$f":"+BM699","v":2134.0625},null,null,"+","E1",null,null,{"$f":"+R700-N700","v":786.04166666666652},null,null,"+","E1","-","D1","=",0,null,"(3.denklem)"]
[null,null,"x = L ; v1 =",null,null,null,{"$f":"+E684","v":223.48214285714286},null,"*",{"$f":"+Y636","v":1.5},null,"3/",{"$f":"+J684","v":6},"-",{"$f":"+L684","v":55},null,"*",{"$f":"+J701","v":1.5},null,"4/",{"$f":"+Q684","v":24},null,"+","C1","*",{"$f":"+R701","v":1.5},null,"+","C2",null,null,{"$f":"G701*J701^3/M701-O701*R701^4/U701","v":114.10714285714285},null,null,"+","C1","*",{"$f":"+Z701","v":1.5},null,"+","C2"]
[null,null,"x = L ; v2 =",null,null,null,{"$f":"+E688","v":223.48214285714286},null,"*",{"$f":"+Y636","v":1.5},null,"3/",{"$f":"+J688","v":6},"-",{"$f":"+L688","v":55},null,"*",{"$f":"+J702","v":1.5},null,"4/",{"$f":"+Q688","v":24},null,"-",{"$f":"+T688","v":65},null,"*(",{"$f":"+R702","v":1.5},null,"-",{"$f":"+Y688","v":1.5},null,")3"," /",6,"+","D1","*",{"$f":"+AA702","v":1.5},null,"+","D2",null,null,{"$f":"G702*J702^3/M702-O702*R702^4/U702-X702*(AA702-AD702)^3/AH702","v":114.10714285714285},null,null,"+","D1","*",{"$f":"+AL702","v":1.5},null,"+","D2"]
[null,null,"(x = L  ; v1 ) = ( x = L ; v2 ) =",null,null,null,null,null,null,null,null,{"$f":"+AF701","v":114.10714285714285},null,null,"+","C1","*",{"$f":"+AL701","v":1.5},null,"+","C2","=",{"$f":"+AR702","v":114.10714285714285},null,null,"+","D1","*",{"$f":"+AX702","v":1.5},null,"+","D2",null,null,"C1","*",{"$f":"+R703","v":1.5},null,"-","D1","*",{"$f":"+AC703","v":1.5},null,"-","D2","+",{"$f":"+L703-W703","v":0},"=",0,null,"(4.denklem)"]
[null,null,"x = L ; v1' =",null,null,null,{"$f":"+E683","v":223.48214285714286},null,"*",{"$f":"+Y636","v":1.5},null,"² /",2,"-",{"$f":"+L683","v":55},null,"*",{"$f":"+J704","v":1.5},null,"3 /",{"$f":"+Q683","v":6},"+","C1",null,null,{"$f":"G704*J704^2/M704-O704*R704^3/U704","v":220.47991071428572},null,null,"+","C1"]
[null,null,"x = L ; v2' =",null,null,null,{"$f":"+E687","v":223.48214285714286},null,"*",{"$f":"+Y636","v":1.5},null,"² /",2,"-",{"$f":"+L687","v":55},null,"*",{"$f":"+J705","v":1.5},null,"3 /",{"$f":"+Q687","v":6},"-",{"$f":"+S687","v":65},null,"*(",{"$f":"+R705","v":1.5},null,"-",{"$f":"+X687","v":1.5},null,")²"," /",2,"+","D1",null,null,{"$f":"G705*J705^2/M705-O705*R705^3/U705-W705*(Z705-AC705)^2/AG705","v":220.47991071428572},null,null,"+","D1"]
[null,null,"(x = L  ; v1' ) = ( x = L ; v2' ) =",null,null,null,null,null,null,null,null,{"$f":"+Z704","v":220.47991071428572},null,null,"+","C1","=",{"$f":"+AL705","v":220.47991071428572},null,null,"+","D1",null,null,"C1","-","D1","+",{"$f":"+L706-R706","v":0},"=",0,null,"(5.denklem)"]
[null,null,"beş adet denklem beş adet bilinmeyen çözülürse :"]
[null,null,"C1 =",null,{"$f":"+T708","v":-781.57738095238085},null,null,0,{"$f":"+BB695","v":7},1,0,0,{"$f":"-AV695","v":-5471.0416666666661},null,{"$f":"MINVERSE(H708:L712)","v":0.14285714285714285},0,0,0.14285714285714279,0.7857142857142857,{"$f":"MMULT(O708:S712,M708:M712)","v":-781.57738095238085}]
[null,null,"D1 =",null,{"$f":"+T709","v":-781.57738095238085},null,null,0,0,0,{"$f":"+L697","v":7},1,{"$f":"-F697","v":-8222.1874999999982},null,0.14285714285714285,0,0,0.14285714285714285,-0.21428571428571427,-781.57738095238085]
[null,null,"D2 =",null,{"$f":"+T710","v":0},null,null,0,-1,0,1,0,{"$f":"-Y700","v":-786.04166666666652},null,0,0,0,-1,1.5,0]
[null,null,"E1 =",null,-1567.6190476190473,null,null,{"$f":"+AK703","v":1.5},{"$f":"-AP703","v":-1.5},-1,0,0,{"$f":"-AU703","v":0},null,0.14285714285714285,0,1,0.14285714285714285,-0.21428571428571427,-1567.6190476190473]
[null,null,"E2 =",null,2751.1458333333339,null,null,1,-1,0,0,0,{"$f":"-AC706","v":0},null,-1,1,-7,-1,1.5,2751.1458333333339]
[null,null,"1.ci bölgede elastik eğri denklemi"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E684","v":223.48214285714286},null,"*","x3"," /",6,"-",{"$f":"+L684","v":55},null,"*","x4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"y = (",null,{"$f":"+H714","v":223.48214285714286},null,"*","x3"," /",6,"-",{"$f":"+O714","v":55},null,"*","x4"," /",24,null,"+",{"$f":"+E708","v":-781.57738095238085},null,null,"*","x",") * 108 / ( E * I )"]
[null,null,"x=",1,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D716<=Y636,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E715","v":223.48214285714286},null,"*",{"$f":"+D716","v":1},null,"3 /",6,"-",{"$f":"+L715","v":55},null,"*",{"$f":"+H717","v":1},null,"4/",{"$f":"+Q715","v":24},null,"+",{"$f":"+T715","v":-781.57738095238085},null,null,"*",{"$f":"+D716","v":1},null,")* 108 / (",null,null,{"$f":"+F642","v":200000},null,null,"*",{"$f":"+F641","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E717*H717^3/K717-M717*P717^4/S717+V717*Z717)*100000000/(AE717*AI717)","v":-4.0542029963592734},null,null,"mm"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"+AC638*1000","v":7000},null,null," /",300,null,"=",{"$f":"+H719/L719","v":23.333333333333332},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E718","v":-4.0542029963592734},null,null,"mm",null,{"$f":"IF(ABS(D720)<ABS(M720),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O719","v":23.333333333333332},null,null,"mm",null,{"$f":"IF(ABS(D720)<ABS(M720),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"2.ci bölgede elastik eğri denklemi"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E688","v":223.48214285714286},null,"*","x3"," /",6,"-",{"$f":"+L688","v":55},null,"*","x4"," /",24,null,"-",{"$f":"+T688","v":65},null,"*(","x","-",{"$f":"+Y688","v":1.5},null,")3"," /",6,"+","D1","*","x","+","D2"]
[null,null,"y = (",null,{"$f":"+H722","v":223.48214285714286},null,"*","x3"," /",6,"-",{"$f":"+O722","v":55},null,"*","x4"," /",24,null,"-",{"$f":"+W722","v":65},null,"*(","x","-",{"$f":"+AB722","v":1.5},null,")3"," /",6,"+",{"$f":"+E709","v":-781.57738095238085},null,null,"*","x","+",{"$f":"+E710","v":0},") * 108 / ( E * I )"]
[null,null,"x=",5,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D724<Y636,\"artır.\",IF(D724>AC638,\"azalt.\",\"\"))","v":""}]
[null,null,"y = (",null,{"$f":"+E723","v":223.48214285714286},null,"*",{"$f":"+D724","v":5},null,"3 /",6,"-",{"$f":"+L723","v":55},null,"*",{"$f":"+H725","v":5},null,"4/",{"$f":"+Q723","v":24},null,"-",{"$f":"+T723","v":65},null,"*(",{"$f":"+P725","v":5},null,"-",{"$f":"+Y723","v":1.5},null,")3"," /",6,"+",{"$f":"+AE723","v":-781.57738095238085},null,null,"*",{"$f":"+Y725","v":5},null,")* 108 / (",null,null,{"$f":"+AE717","v":200000},null,null,"*",{"$f":"+AI717","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E725*H725^3/K725-M725*P725^4/S725-V725*(Y725-AB725)^3/AF725+AH725*AL725)*100000000/(AQ725*AU725)","v":-6.2379439721153425},null,null,"mm"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"+AC638*1000","v":7000},null,null," /",300,null,"=",{"$f":"+H727/L727","v":23.333333333333332},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E726","v":-6.2379439721153425},null,null,"mm",null,{"$f":"IF(ABS(D728)<ABS(M728),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O727","v":23.333333333333332},null,null,"mm",null,{"$f":"IF(ABS(D728)<ABS(M728),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"3.cü bölgede elastik eğri denklemi"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E692","v":223.48214285714286},null,"*","x3"," /",6,"-",{"$f":"+L692","v":385},null,"*(","x","-",{"$f":"+Q692","v":3.5},null,")3"," /",6,"-",{"$f":"+W692","v":65},null,"*(","x","-",{"$f":"+AB692","v":1.5},null,")3"," /",6,"+",{"$f":"+AH692","v":339.01785714285711},null,"*(","x","-",{"$f":"+AM692","v":7},null,")3"," /",6,"-",{"$f":"+AS692","v":25},null,"*(","x","-",{"$f":"+AX692","v":7},null,")4"," /",24,null,"+","E1","*","x","+","E2"]
[null,null,"y = (",null,{"$f":"+H730","v":223.48214285714286},null,"*","x3"," /",6,"-",{"$f":"+O730","v":385},null,"*(","x","-",{"$f":"+T730","v":3.5},null,")3"," /",6,"-",{"$f":"+Z730","v":65},null,"*(","x","-",{"$f":"+AE730","v":1.5},null,")3"," /",6,"+",{"$f":"+AK730","v":339.01785714285711},null,"*(","x","-",{"$f":"+AP730","v":7},null,")3"," /",6,"-",{"$f":"+AV730","v":25},null,"*(","x","-",{"$f":"+BA730","v":7},null,")4"," /",24,null,"+",{"$f":"+E711","v":-1567.6190476190473},null,null,"*","x","+",{"$f":"+E712","v":2751.1458333333339},null,null,") * 108 / ( E * I )"]
[null,null,"x=",8.5,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D732<AC638,\"artır.\",IF(D732>(AC638+AM636),\"azalt.\",\"\"))","v":""}]
[null,null,"y = (",null,{"$f":"+E731","v":223.48214285714286},null,"*",{"$f":"+D732","v":8.5},null,"3 /",6,"-",{"$f":"+L731","v":385},null,"*(",{"$f":"+D732","v":8.5},null,"-",{"$f":"+Q731","v":3.5},null,")3"," /",6,"-",{"$f":"+W731","v":65},null,"*(",{"$f":"+P733","v":8.5},null,"-",{"$f":"+AB731","v":1.5},null,")3"," /",6,"+",{"$f":"+AH731","v":339.01785714285711},null,"*(",{"$f":"+AB733","v":8.5},null,"-",{"$f":"+AM731","v":7},null,")3"," /",6,"-",{"$f":"+AS731","v":25},null,"*(",{"$f":"+AN733","v":8.5},null,"-",{"$f":"+AX731","v":7},null,")4"," /",24,"+",{"$f":"+BE731","v":-1567.6190476190473},null,null,"*",{"$f":"+AZ733","v":8.5},null,"+",{"$f":"+BK731","v":2751.1458333333339},null,null,")* 108 / (",null,null,{"$f":"+AQ725","v":200000},null,null,"*",{"$f":"+AU725","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E733*H733^3/K733-M733*(P733-S733)^3/W733-Y733*(AB733-AE733)^3/AI733+AK733*(AN733-AQ733)^3/AU733-AW733*(AZ733-BC733)^4/BG733+BI733*BM733+BP733)*100000000/(BV733*BZ733)","v":4.0696669530377747},null,null,"mm"]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"+AM636*1000","v":1500},null,null," /",150,null,"=",{"$f":"+H735/L735","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E734","v":4.0696669530377747},null,null,"mm",null,{"$f":"IF(ABS(D736)<ABS(M736),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O735","v":10},null,null,"mm",null,{"$f":"IF(ABS(D736)<ABS(M736),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK TEK AÇIKLIKLI KONSOLLU KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(1.ci bölge)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(4.cü bölge)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,20,null,"KN",null,null,null,null,null,null,"(2.ci bölge)",null,null,null,null,null,null,null,"(3.cü bölge)",null,null,null,null,null,null,null,null,40,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,null,"KN/m",null,null,null,null,null,null,null,85,null,"KN",null,null,null,null,null,null,25,null,"KN/m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK797","v":1.1526499077284678},null,null,null,"(2.ci ve 3.cü bölge için)",null,null,null,null,null,null,null,null,null,null,"(1.ve 4.cü bölge için Cb = 1 alınır.)"]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O742,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"ABS(BB789)","v":376.04889634639898},null,null,"KNm",null,"(max moment)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(BA748),ABS(BB748),ABS(BC748),ABS(BD748),ABS(BE748),ABS(BF748),ABS(BG748),ABS(BH748))","v":294.35267857142856},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O742,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-W742","v":-20},{"$f":"+BA748-Z743*Z751","v":-81.25},{"$f":"BB748+AC750","v":294.35267857142856},{"$f":"+BC748-AG744*AF751","v":196.85267857142856},{"$f":"+BD748-AJ743","v":111.85267857142856},{"$f":"+BE748-AG744*AM751","v":-245.64732142857144},{"$f":"+BF748+AQ750","v":77.5},{"$f":"+BG748-AS743*AT751","v":40}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E762","v":375.60267857142856},null,"KN",null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E764","v":323.14732142857144},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O742,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.75,null,"m",null,null,null,1.5,null,"m",null,null,null,null,{"$f":"+AJ753-AF751","v":5.5},null,"m",null,null,null,null,1.5,null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O742,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uygunluk koşulları",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O742,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)",null,null,null,null,null,null,null,null,null,null,null,null,null,"(x = L) v1' = (x = L) v2'",null,null,null,null,null,null,null,null,null,null,null,null,null,"(x = L) v3' = (x = L) v4'"]
[null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( x = L) v1  = ( x = L) v2 = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,"( x = L) v3 = ( x = L) v4 = 0"]
[null,null,"MESNET TEPKİLERİ "]
[null,null,"A","*",{"$f":"+AJ753","v":7},null,"-",{"$f":"+AG744","v":65},null,"*",{"$f":"+AJ753","v":7},null,"*",{"$f":"+K761/2","v":3.5},null,"-",{"$f":"+AJ743","v":85},null,"*",{"$f":"+AM751","v":5.5},null,"+",{"$f":"+AS743","v":25},null,"*",{"$f":"+AT751","v":1.5},null,"*",{"$f":"+Z761/2","v":0.75},null,"+",{"$f":"+AW742","v":40},null,"*",{"$f":"+AT751","v":1.5},null,"-",{"$f":"+Z743","v":35},null,"*",{"$f":"+Z751","v":1.75},null,"*",{"$f":"+AO761/2+AJ753","v":7.875},null,"-",{"$f":"+W742","v":20},null,"*",{"$f":"+Z751+AJ753","v":8.75},null,"=",0]
[null,null,"A","=",{"$f":"(H761*K761*N761+Q761*T761-W761*Z761*AC761-AF761*AI761+AL761*AO761*AR761+AU761*AX761)/E761","v":375.60267857142856},null,null,"KN"]
[null,null,"A","+","B","-",{"$f":"+AG744","v":65},null,"*",{"$f":"+AJ753","v":7},null,"-",{"$f":"+AJ743","v":85},null,"-",{"$f":"+AS743","v":25},null,"*",{"$f":"+AT751","v":1.5},null,"-",{"$f":"+AW742","v":40},null,"-",{"$f":"+Z743","v":35},null,"*",{"$f":"+Z751","v":1.75},null,"-",{"$f":"+W742","v":20},null,"=",0]
[null,null,"B","=",{"$f":"+G763*J763+M763+P763*S763+V763+Y763*AB763+AE763-E762","v":323.14732142857144},null,null,"KN"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"1.ci bölgede :"]
[null,null,"Mx =",null,{"$f":"-W742","v":-20},null,"*","x","-",{"$f":"Z743","v":35},null,"*","x²"," /",2]
[null,null,"x=",1,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D768<=Z751,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+E767","v":-20},null,"*",{"$f":"+D768","v":1},null,"-",{"$f":"+J767","v":35},null,"*",{"$f":"+D768","v":1},null,"²/",2,"=",{"$f":"+E769*H769-K769*N769^2/Q769","v":-37.5},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E769","v":-20},null,"-",{"$f":"+K769","v":35},null,"*",{"$f":"+D768","v":1},null,"=",{"$f":"+E770-H770*K770","v":-55},null,null,"KNm"]
[null,null,"2.ci bölgede :"]
[null,null,"Mx =",null,{"$f":"-W742","v":-20},null,"*","x","-",{"$f":"Z743","v":35},null,"*",{"$f":"+Z751","v":1.75},null,"*(","x","-",{"$f":"+Z751/2","v":0.875},null,")+",{"$f":"+AC750","v":375.60267857142856},null,"*(","x","-",{"$f":"+Z751","v":1.75},null,")-",{"$f":"+AG744","v":65},null,"*(","x","-",{"$f":"+Z751","v":1.75},null,")²"," /",2]
[null,null,"x=",2,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D773<=Z751,\"artır.\",IF(D773>(AF751+Z751),\"azalt.\",\"\"))","v":""}]
[null,null,"Mx =",null,{"$f":"+E772","v":-20},null,"*",{"$f":"+D773","v":2},null,"-",{"$f":"+J772*M772","v":61.25},null,"*(",{"$f":"+D773","v":2},null,"-",{"$f":"+R772","v":0.875},null,")+",{"$f":"+U772","v":375.60267857142856},null,"*(",{"$f":"+D773","v":2},null,"-",{"$f":"+Z772","v":1.75},null,")-",{"$f":"+AC772","v":65},null,"*(",{"$f":"+W774","v":2},null,"-",{"$f":"+AH772","v":1.75},null,")²"," /",2,"=",{"$f":"+E774*H774-K774*(N774-Q774)+T774*(W774-Z774)-AC774*(AF774-AI774)^2/AM774","v":-17.036830357142861},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E774","v":-20},null,"-",{"$f":"+J772","v":35},null,"*",{"$f":"+M772","v":1.75},null,"+",{"$f":"+T774","v":375.60267857142856},null,"-",{"$f":"+AC774","v":65},null,"*(",{"$f":"+D773","v":2},null,"-",{"$f":"+Z751","v":1.75},null,")=",{"$f":"E775-H775*K775+N775-Q775*(T775-W775)","v":278.10267857142856},null,null,"KN"]
[null,null,"3.cü bölgede :"]
[null,null,"Mx =",null,{"$f":"-W742","v":-20},null,"*","x","-",{"$f":"+Z743","v":35},null,"*",{"$f":"+Z751","v":1.75},null,"*(","x","-",{"$f":"+Z751/2","v":0.875},null,")+",{"$f":"+AC750","v":375.60267857142856},null,"*(","x","-",{"$f":"+Z751","v":1.75},null,")-",{"$f":"+AG744","v":65},null,"*(","x","-",{"$f":"+Z751","v":1.75},null,")²"," /",2,"-",{"$f":"+AJ743","v":85},null,"*(","x","-",{"$f":"+Z751+AF751","v":3.25},null,")"]
[null,null,"x=",4.5,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D778<=(Z751+AF751),\"artır.\",IF(D778>(AF751+Z751+AM751),\"azalt.\",\"\"))","v":""}]
[null,null,"Mx =",null,{"$f":"+E777","v":-20},null,"*",{"$f":"+D778","v":4.5},null,"-",{"$f":"+J777*M777","v":61.25},null,"*(",{"$f":"+D778","v":4.5},null,"-",{"$f":"+R777","v":0.875},null,")+",{"$f":"+U777","v":375.60267857142856},null,"*(",{"$f":"+N779","v":4.5},null,"-",{"$f":"+Z777","v":1.75},null,")-",{"$f":"+AC777","v":65},null,"*(",{"$f":"+W779","v":4.5},null,"-",{"$f":"+AH777","v":1.75},null,")²"," /",2,"-",{"$f":"+AN777","v":85},null,"*(",{"$f":"+AF779","v":4.5},null,"-",{"$f":"+AS777","v":3.25},null,")=",{"$f":"E779*H779-K779*(N779-Q779)+T779*(W779-Z779)-AC779*(AF779-AI779)^2/AM779-AO779*(AR779-AU779)","v":368.84486607142844},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E779","v":-20},null,"-",{"$f":"+J777","v":35},null,"*",{"$f":"+M777","v":1.75},null,"+",{"$f":"+T779","v":375.60267857142856},null,"-",{"$f":"+AC779","v":65},null,"*(",{"$f":"+AF779","v":4.5},null,"-",{"$f":"+AI779","v":1.75},null,")-",{"$f":"+AO779","v":85},null,"=",{"$f":"+E780-H780*K780+N780-Q780*(T780-W780)-Z780","v":30.602678571428555},null,null,"KN"]
[null,null,"4.cü bölgede :"]
[null,null,"Mx =",null,{"$f":"-W742","v":-20},null,"*","x","-",{"$f":"+Z743","v":35},null,"*",{"$f":"+Z751","v":1.75},null,"*(","x","-",{"$f":"+Z751/2","v":0.875},null,")+",{"$f":"+AC750","v":375.60267857142856},null,"*(","x","-",{"$f":"+Z751","v":1.75},null,")-",{"$f":"+AG744","v":65},null,"*",{"$f":"+AJ753","v":7},null,"*(","x","-",{"$f":"Z751+AJ753/2","v":5.25},null,")-",{"$f":"+AJ743","v":85},null,"*(","x","-",{"$f":"+Z751+AF751","v":3.25},null,")+",{"$f":"+AQ750","v":323.14732142857144},null,"*(","x","-",{"$f":"+Z751+AJ753","v":8.75},null,")-",{"$f":"+AS743","v":25},null,"*(","x","-",{"$f":"+Z751+AJ753","v":8.75},null,")²"," /",2]
[null,null,"x=",9.25,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D783<=(Z751+AF751+AM751),\"artır.\",IF(D783>(AF751+Z751+AM751+AT751),\"azalt.\",\"\"))","v":""}]
[null,null,"Mx =",null,{"$f":"+E782","v":-20},null,"*",{"$f":"+D783","v":9.25},null,"-",{"$f":"+J782*M782","v":61.25},null,"*(",{"$f":"+D783","v":9.25},null,"-",{"$f":"+R782","v":0.875},null,")+",{"$f":"+U782","v":375.60267857142856},null,"*(",{"$f":"+N784","v":9.25},null,"-",{"$f":"+Z782","v":1.75},null,")-",{"$f":"+AC782*AF782","v":455},null,"*(",{"$f":"+W784","v":9.25},null,"-",{"$f":"+AK782","v":5.25},null,")-",{"$f":"+AN782","v":85},null,"*(",{"$f":"+AF784","v":9.25},null,"-",{"$f":"+AS782","v":3.25},null,")+",{"$f":"+AV782","v":323.14732142857144},null,"*(",{"$f":"+AO784","v":9.25},null,"-",{"$f":"+BA782","v":8.75},null,")-",{"$f":"+BD782","v":25},null,"*(",{"$f":"+AX784","v":9.25},null,"-",{"$f":"+BI782","v":8.75},null,")²"," /",2,"=",{"$f":"E784*H784-K784*(N784-Q784)+T784*(W784-Z784)-AC784*(AF784-AI784)-AL784*(AO784-AR784)+AU784*(AX784-BA784)-BD784*(BG784-BJ784)^2/BN784","v":-52.500000000000057},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E784","v":-20},null,"-",{"$f":"+J782","v":35},null,"*",{"$f":"+M782","v":1.75},null,"+",{"$f":"+T784","v":375.60267857142856},null,"-",{"$f":"+AC784","v":455},null,"-",{"$f":"+AL784","v":85},null,"+",{"$f":"+AU784","v":323.14732142857144},null,"-",{"$f":"+BD784","v":25},null,"*(",{"$f":"+BG784","v":9.25},null,"-",{"$f":"+BJ784","v":8.75},null,")=",{"$f":"+E785-H785*K785+N785-Q785-T785+W785-Z785*(AC785-AF785)","v":65},null,null,"KN"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"2.ve 3.cü bölgede :",null,null,null,null,null,null,null,null,null,null,null,null,null,"x1=",null,{"$f":"(-W742-Z743*Z751+AC750)/AG744","v":4.5285027472527473},null,"m",null,"M1 =",null,{"$f":"AC750*S787-W742*(Z751+S787)-Z743*Z751*(Z751/2+S787)-AG744*S787*S787/2","v":577.89470678595956},null,"KNm",null,null,{"$f":"IF(S787<AF751,S787,S788)","v":3.2208104395604393},null,{"$f":"INDEX(Y787:Y788,MATCH(AD787,S787:S788,0),0)","v":376.04889634639903}]
[null,null,"x=",{"$f":"IF(AF787<AF788,AD788+Z751,AD787+Z751)","v":4.9708104395604398},null,null,"m. ' deki max moment miktarı",null,null,null,null,null,null,null,null,null,"x2=",null,{"$f":"(-W742-Z743*Z751-AJ743+AC750)/AG744","v":3.2208104395604393},null,"m",null,"M2 =",null,{"$f":"AC750*S788-W742*(Z751+S788)-Z743*Z751*(Z751/2+S788)-AG744*S788*S788/2-AJ743*(S788-AF751)","v":376.04889634639903},null,"KNm",null,null,{"$f":"+AJ753","v":7},null,{"$f":"AW742*AT751+AS743*AT751*AT751/2","v":88.125}]
[null,null,"Mmax =",null,null,{"$f":"+E769","v":-20},null,"*",{"$f":"+D788","v":4.9708104395604398},null,"-",{"$f":"+Z743","v":35},null,"*",{"$f":"+Z751","v":1.75},null,"*(",{"$f":"+I789","v":4.9708104395604398},null,"-",{"$f":"+Z751/2","v":0.875},null,")+",{"$f":"+AC750","v":375.60267857142856},null,"*(",{"$f":"+R789","v":4.9708104395604398},null,"-",{"$f":"+Z751","v":1.75},null,")-",{"$f":"+AG744","v":65},null,"*(",{"$f":"+D788","v":4.9708104395604398},null,"-",{"$f":"+Z751","v":1.75},null,")²"," /",2,"-",{"$f":"IF((AV789-AY789)<0,0,AJ743)","v":85},null,"*(",{"$f":"+AJ789","v":4.9708104395604398},null,"-",{"$f":"+Z751+AF751","v":3.25},null,")=",{"$f":"F789*I789-L789*O789*(R789-U789)+X789*(AA789-AD789)-AG789*(AJ789-AM789)^2/AQ789-AS789*(AV789-AY789)","v":376.04889634639898},null,null,"KNm"]
[null,null,"L / 2 =",null,{"$f":"+AJ753/2+Z751","v":5.25},null,null,"m. ' deki moment miktarı"]
[null,null,"MB =",null,{"$f":"+F789","v":-20},null,"*",{"$f":"+E790","v":5.25},null,"-",{"$f":"+L789","v":35},null,"*",{"$f":"+O789","v":1.75},null,"*(",{"$f":"+E790","v":5.25},null,"-",{"$f":"+U789","v":0.875},null,")+",{"$f":"+X789","v":375.60267857142856},null,"*(",{"$f":"+Q791","v":5.25},null,"-",{"$f":"+AD789","v":1.75},null,")-",{"$f":"+AG789","v":65},null,"*(",{"$f":"+Z791","v":5.25},null,"-",{"$f":"+AM789","v":1.75},null,")²"," /",2,"-",{"$f":"IF((AU791-AX791)<0,0,AJ743)","v":85},null,"*(",{"$f":"+AI791","v":5.25},null,"-",{"$f":"+AY789","v":3.25},null,")=",{"$f":"E791*H791-K791*N791*(Q791-T791)+W791*(Z791-AC791)-AF791*(AI791-AL791)^2/AP791-AR791*(AU791-AX791)","v":373.515625},null,null,"KNm"]
[null,null,"L / 4 =",null,{"$f":"+AJ753/4+Z751","v":3.5},null,null,"m. ' deki moment miktarı"]
[null,null,"MA =",null,{"$f":"+E791","v":-20},null,"*",{"$f":"+E792","v":3.5},null,"-",{"$f":"+K791","v":35},null,"*",{"$f":"+N791","v":1.75},null,"*(",{"$f":"+E792","v":3.5},null,"-",{"$f":"+T791","v":0.875},null,")+",{"$f":"+W791","v":375.60267857142856},null,"*(",{"$f":"+Q793","v":3.5},null,"-",{"$f":"+AC791","v":1.75},null,")-",{"$f":"+AF791","v":65},null,"*(",{"$f":"+Z793","v":3.5},null,"-",{"$f":"+AL791","v":1.75},null,")²"," /",2,"-",{"$f":"IF((AU793-AX793)<0,0,AJ743)","v":85},null,"*(",{"$f":"+AI793","v":3.5},null,"-",{"$f":"+AX791","v":3.25},null,")=",{"$f":"E793*H793-K793*N793*(Q793-T793)+W793*(Z793-AC793)-AF793*(AI793-AL793)^2/AP793-AR793*(AU793-AX793)","v":305.7421875},null,null,"KNm"]
[null,null,"3 * L / 4 =",null,null,{"$f":"3*AJ753/4+Z751","v":7},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,{"$f":"+E793","v":-20},null,"*",{"$f":"+F794","v":7},null,"-",{"$f":"+K793","v":35},null,"*",{"$f":"+N793","v":1.75},null,"*(",{"$f":"+H795","v":7},null,"-",{"$f":"+T793","v":0.875},null,")+",{"$f":"+W793","v":375.60267857142856},null,"*(",{"$f":"+Q795","v":7},null,"-",{"$f":"+AC793","v":1.75},null,")-",{"$f":"+AF793","v":65},null,"*(",{"$f":"+Z795","v":7},null,"-",{"$f":"+AL793","v":1.75},null,")²"," /",2,"-",{"$f":"IF((AU795-AX795)<0,0,AJ743)","v":85},null,"*(",{"$f":"+AI795","v":7},null,"-",{"$f":"+AX793","v":3.25},null,")=",{"$f":"E795*H795-K795*N795*(Q795-T795)+W795*(Z795-AC795)-AF795*(AI795-AL795)^2/AP795-AR795*(AU795-AX795)","v":242.2265625},null,null,"KNm"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(BB789)","v":376.04889634639898},null,null," /(",2.5,null,"*",{"$f":"+H797","v":376.04889634639898},null,null,"+",3,"*",{"$f":"ABS(BA793)","v":305.7421875},null,null,"+",4,"*",{"$f":"ABS(BA791)","v":373.515625},null,null,"+",3,"*",{"$f":"ABS(BA795)","v":242.2265625},null,null,")=",{"$f":"E797*H797/(L797*O797+S797*U797+Y797*AA797+AE797*AG797)","v":1.1526499077284678}]
[null,null,"1.ci bölgede :"]
[null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca konsol kirişte Cb = 1 alınır."]
[null,null,"4.cü bölgede :"]
[null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca konsol kirişte Cb = 1 alınır."]
[null,null,"SEHİM HESABI"]
[null,null,"1.ci bölgede :"]
[null,null,"v1'' = ",null,{"$f":"-W742","v":-20},null,"*","x","-",{"$f":"Z743","v":35},null,"*","x²"," /",2]
[null,null,"v1' = ",null,{"$f":"+E804","v":-20},null,"*","x²"," /",2,"-",{"$f":"+J804","v":35},null,"*","x3"," /",6,"+","C1"]
[null,null,"v1 = ",null,{"$f":"+E805","v":-20},null,"*","x3"," /",6,"-",{"$f":"+L805","v":35},null,"*","x4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"2.ci bölgede :"]
[null,null,"v2'' = ",null,{"$f":"-W742","v":-20},null,"*","x","-",{"$f":"+Z743","v":35},null,"*",{"$f":"+Z751","v":1.75},null,"*(","x","-",{"$f":"+Z751/2","v":0.875},null,")+",{"$f":"+AC750","v":375.60267857142856},null,"*(","x","-",{"$f":"+Z751","v":1.75},null,")-",{"$f":"+AG744","v":65},null,"*(","x","-",{"$f":"+Z751","v":1.75},null,")²"," /",2]
[null,null,"v2' = ",null,{"$f":"+E808","v":-20},null,"*","x²"," /",2,"-",{"$f":"+J808*M808","v":61.25},null,"*(","x","-",{"$f":"+R808","v":0.875},null,")²"," /",2,"+",{"$f":"+U808","v":375.60267857142856},null,"*(","x","-",{"$f":"+Z808","v":1.75},null,")²"," /",2,"-",{"$f":"+AC808","v":65},null,"*(","x","-",{"$f":"+AH808","v":1.75},null,")3"," /",6,"+","D1"]
[null,null,"v2 = ",null,{"$f":"+E809","v":-20},null,"*","x3"," /",6,"-",{"$f":"+L809","v":61.25},null,"*(","x","-",{"$f":"+Q809","v":0.875},null,")3"," /",6,"+",{"$f":"+W809","v":375.60267857142856},null,"*(","x","-",{"$f":"+AB809","v":1.75},null,")3"," /",6,"-",{"$f":"+AH809","v":65},null,"*(","x","-",{"$f":"+AM809","v":1.75},null,")4"," /",24,null,"+","D1","*","x","+","D2"]
[null,null,"3.cü bölgede :"]
[null,null,"v3'' = ",null,{"$f":"-W742","v":-20},null,"*","x","-",{"$f":"+Z743","v":35},null,"*",{"$f":"+Z751","v":1.75},null,"*(","x","-",{"$f":"+Z751/2","v":0.875},null,")+",{"$f":"+AC750","v":375.60267857142856},null,"*(","x","-",{"$f":"+Z751","v":1.75},null,")-",{"$f":"+AG744","v":65},null,"*(","x","-",{"$f":"+Z751","v":1.75},null,")²"," /",2,"-",{"$f":"+AJ743","v":85},null,"*(","x","-",{"$f":"+AF751+Z751","v":3.25},null,")"]
[null,null,"v3' = ",null,{"$f":"+E812","v":-20},null,"*","x²"," /",2,"-",{"$f":"+J812*M812","v":61.25},null,"*(","x","-",{"$f":"+R812","v":0.875},null,")²"," /",2,"+",{"$f":"+U812","v":375.60267857142856},null,"*(","x","-",{"$f":"+Z812","v":1.75},null,")²"," /",2,"-",{"$f":"+AC812","v":65},null,"*(","x","-",{"$f":"+AH812","v":1.75},null,")3"," /",6,"-",{"$f":"+AN812","v":85},null,"*(","x","-",{"$f":"+AS812","v":3.25},null,")²"," /",2,"+","E1"]
[null,null,"v3 = ",null,{"$f":"+E813","v":-20},null,"*","x3"," /",6,"-",{"$f":"+L813","v":61.25},null,"*(","x","-",{"$f":"+Q813","v":0.875},null,")3"," /",6,"+",{"$f":"+W813","v":375.60267857142856},null,"*(","x","-",{"$f":"+AB813","v":1.75},null,")3"," /",6,"-",{"$f":"+AH813","v":65},null,"*(","x","-",{"$f":"+AM813","v":1.75},null,")4"," /",24,null,"-",{"$f":"+AS813","v":85},null,"*(","x","-",{"$f":"+AX813","v":3.25},null,")3"," /",6,"+","E1","*","x","+","E2"]
[null,null,"4.cü bölgede :"]
[null,null,"v4'' = ",null,{"$f":"-W742","v":-20},null,"*","x","-",{"$f":"Z743","v":35},null,"*",{"$f":"+Z751","v":1.75},null,"*(","x","-",{"$f":"+Z751/2","v":0.875},null,")+",{"$f":"+AC750","v":375.60267857142856},null,"*(","x","-",{"$f":"+Z751","v":1.75},null,")-",{"$f":"+AG744","v":65},null,"*",{"$f":"+AJ753","v":7},null,"*(","x","-",{"$f":"+Z751+AJ753/2","v":5.25},null,")-",{"$f":"+AJ743","v":85},null,"*(","x","-",{"$f":"+Z751+AF751","v":3.25},null,")+",{"$f":"+AQ750","v":323.14732142857144},null,"*(","x","-",{"$f":"+Z751+AJ753","v":8.75},null,")-",{"$f":"AS743","v":25},null,"*(","x","-",{"$f":"+Z751+AJ753","v":8.75},null,")²"," /",2]
[null,null,"v4' = ",null,{"$f":"+E816","v":-20},null,"*","x²"," /",2,"-",{"$f":"+J816*M816","v":61.25},null,"*(","x","-",{"$f":"+R816","v":0.875},null,")²"," /",2,"+",{"$f":"+U816","v":375.60267857142856},null,"*(","x","-",{"$f":"+Z816","v":1.75},null,")²"," /",2,"-",{"$f":"+AC816*AF816","v":455},null,"*(","x","-",{"$f":"+AK816","v":5.25},null,")²"," /",2,"-",{"$f":"+AN816","v":85},null,"*(","x","-",{"$f":"+AS816","v":3.25},null,")²"," /",2,"+",{"$f":"+AV816","v":323.14732142857144},null,"*(","x","-",{"$f":"+BA816","v":8.75},null,")²"," /",2,"-",{"$f":"+BD816","v":25},null,"*(","x","-",{"$f":"+BI816","v":8.75},null,")3"," /",6,"+","F1"]
[null,null,"v4 = ",null,{"$f":"+E817","v":-20},null,"*","x3"," /",6,"-",{"$f":"+L817","v":61.25},null,"*(","x","-",{"$f":"+Q817","v":0.875},null,")3"," /",6,"+",{"$f":"+W817","v":375.60267857142856},null,"*(","x","-",{"$f":"+AB817","v":1.75},null,")3"," /",6,"-",{"$f":"+AH817","v":455},null,"*(","x","-",{"$f":"+AM817","v":5.25},null,")3"," /",6,"-",{"$f":"+AS817","v":85},null,"*(","x","-",{"$f":"+AX817","v":3.25},null,")3"," /",6,"+",{"$f":"+BD817","v":323.14732142857144},null,"*(","x","-",{"$f":"+BI817","v":8.75},null,")3"," /",6,"-",{"$f":"+BO817","v":25},null,"*(","x","-",{"$f":"+BT817","v":8.75},null,")4"," /",24,null,"+"]
[null,null,null,null,"+","F1","*","x","+","F2"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"x = L ; v1 = 0",null,null,null,null,null,{"$f":"+E806","v":-20},null,"*",{"$f":"+Z751","v":1.75},null,"3/",6,"-",{"$f":"+L806","v":35},null,"*",{"$f":"+L821","v":1.75},null,"4/",24,null,"+","C1","*",{"$f":"+T821","v":1.75},null,"+","C2","=",0,null,null,"C1","*",{"$f":"+AB821","v":1.75},null,"+","C2","+",{"$f":"I821*L821^3/O821-Q821*T821^4/W821","v":-31.542154947916664},null,null,"=",0,null,"(1.denklem)"]
[null,null,"x = L ; v2 = 0",null,null,null,null,null,{"$f":"+E810","v":-20},null,"*",{"$f":"+Z751","v":1.75},null,"3/",6,"-",{"$f":"+L810","v":61.25},null,"*(",{"$f":"+L822","v":1.75},null,"-",{"$f":"+Q810","v":0.875},null,")3"," /",6,"+",{"$f":"+W810","v":375.60267857142856},null,"*(",{"$f":"+T822","v":1.75},null,"-",{"$f":"+AB810","v":1.75},null,")3"," /",6,"-",{"$f":"+AH810","v":65},null,"*(",{"$f":"+AF822","v":1.75},null,"-",{"$f":"+AM810","v":1.75},null,")4"," /",24,null,"+","D1","*",{"$f":"+AR822","v":1.75},null,"+","D2","=",0,null,null,"D1","*",{"$f":"+BD822","v":1.75},null,"+","D2","+",{"$f":"I822*L822^3/O822-Q822*(T822-W822)^3/AA822+AC822*(AF822-AI822)^3/AM822-AO822*(AR822-AU822)^4/AY822","v":-24.703369140625},null,null,"=",0,null,"(2.denklem)"]
[null,null,"x = L ; v3 = 0",null,null,null,null,null,{"$f":"+E814","v":-20},null,"*",{"$f":"+Z751+AJ753","v":8.75},null,"3/",6,"-",{"$f":"+L814","v":61.25},null,"*(",{"$f":"+L823","v":8.75},null,"-",{"$f":"+Q814","v":0.875},null,")3"," /",6,"+",{"$f":"+W814","v":375.60267857142856},null,"*(",{"$f":"+T823","v":8.75},null,"-",{"$f":"+AB814","v":1.75},null,")3"," /",6,"-",{"$f":"+AH814","v":65},null,"*(",{"$f":"+AF823","v":8.75},null,"-",{"$f":"+AM814","v":1.75},null,")4"," /",24,null,"-",{"$f":"+AT814","v":85},null,"*(",{"$f":"+AR823","v":8.75},null,"-",{"$f":"+AY814","v":3.25},null,")3"," /",6,"+","E1","*",{"$f":"+BE823","v":8.75},null,"+","E2","=",0]
[null,null,null,null,null,null,null,null,"E1","*",{"$f":"+BP823","v":8.75},null,"+","E2","+",{"$f":"I823*L823^3/O823-Q823*(T823-W823)^3/AA823+AC823*(AF823-AI823)^3/AM823-AO823*(AR823-AU823)^4/AY823-BB823*(BE823-BH823)^3/BL823","v":5393.7178548177089},null,null,"=",0,null,"(3.denklem)"]
[null,null,"x = L ; v4 = 0",null,null,null,null,null,{"$f":"+E818","v":-20},null,"*",{"$f":"+Z751+AJ753","v":8.75},null,"3/",6,"-",{"$f":"+L818","v":61.25},null,"*(",{"$f":"+L825","v":8.75},null,"-",{"$f":"+Q818","v":0.875},null,")3"," /",6,"+",{"$f":"+W818","v":375.60267857142856},null,"*(",{"$f":"+T825","v":8.75},null,"-",{"$f":"+AB818","v":1.75},null,")3"," /",6,"-",{"$f":"+AH818","v":455},null,"*(",{"$f":"+AF825","v":8.75},null,"-",{"$f":"+AM818","v":5.25},null,")3"," /",6,"-",{"$f":"+AS818","v":85},null,"*(",{"$f":"+AR825","v":8.75},null,"-",{"$f":"+AX818","v":3.25},null,")3"," /",6,"+",{"$f":"+BD818","v":323.14732142857144},null,"*(",{"$f":"+BD825","v":8.75},null,"-",{"$f":"+BI818","v":8.75},null,")3"," /",6,"-"]
[null,null,null,null,null,null,"-",{"$f":"+BO818","v":25},null,"*(",{"$f":"+BP825","v":8.75},null,"-",{"$f":"+BT818","v":8.75},null,")4"," /",24,null,"+","F1","*",{"$f":"+K826","v":8.75},null,"+","F2","=",0,null,null,"F1","*",{"$f":"+W826","v":8.75},null,"+","F2","+",{"$f":"I825*L825^3/O825-Q825*(T825-W825)^3/AA825+AC825*(AF825-AI825)^3/AM825-AO825*(AR825-AU825)^3/AY825-BA825*(BD825-BG825)^3/BK825+BM825*(BP825-BS825)^3/BW825-H826*(K826-N826)^4/R826","v":8645.0720214843768},null,null,"=",0,null,"(4.denklem)"]
[null,null,"(x = L) v1' =",null,null,null,{"$f":"+E805","v":-20},null,"*",{"$f":"+Z751","v":1.75},null,"²/",2,"-",{"$f":"+L805","v":35},null,"*",{"$f":"+J827","v":1.75},null,"3/",6,"+","C1",null,null,{"$f":"G827*J827^2/M827-O827*R827^3/U827","v":-61.888020833333329},null,null,"+","C1"]
[null,null,"(x = L) v2' =",null,null,null,{"$f":"+E809","v":-20},null,"*",{"$f":"+Z751","v":1.75},null,"²/",2,"-",{"$f":"+L809","v":61.25},null,"*(",{"$f":"+J828","v":1.75},null,"-",{"$f":"+Q809","v":0.875},null,")²"," /",2,"+",{"$f":"+W809","v":375.60267857142856},null,"*(",{"$f":"+R828","v":1.75},null,"-",{"$f":"+AB809","v":1.75},null,")²"," /",2,"-",{"$f":"+AH809","v":65},null,"*(",{"$f":"+AD828","v":1.75},null,"-",{"$f":"+AM809","v":1.75},null,")3"," /",6,"+","D1",null,null,{"$f":"G828*J828^2/M828-O828*(R828-U828)^2/Y828+AA828*(AD828-AG828)^2/AK828-AM828*(AP828-AS828)^3/AW828","v":-54.072265625},null,null,"+","D1"]
[null,null,"(x = L) v1' = (x = L) v2' =",null,null,null,null,null,null,null,{"$f":"+Z827","v":-61.888020833333329},null,null,"+","C1","=",{"$f":"+BB828","v":-54.072265625},null,null,"+","D1",null,null,"C1","-","D1","+",{"$f":"+K829-Q829","v":-7.8157552083333286},null,null,"=",0,null,"(5.denklem)"]
[null,null,"(x = L) v3' =",null,null,null,{"$f":"+E813","v":-20},null,"*",{"$f":"+Z751+AJ753","v":8.75},null,"²/",2,"-",{"$f":"+L813","v":61.25},null,"*(",{"$f":"+J830","v":8.75},null,"-",{"$f":"+Q813","v":0.875},null,")²"," /",2,"+",{"$f":"+W813","v":375.60267857142856},null,"*(",{"$f":"+R830","v":8.75},null,"-",{"$f":"+AB813","v":1.75},null,")²"," /",2,"-",{"$f":"+AH813","v":65},null,"*(",{"$f":"+AD830","v":8.75},null,"-",{"$f":"+AM813","v":1.75},null,")3"," /",6,"-",{"$f":"+AS813","v":85},null,"*(",{"$f":"+AP830","v":8.75},null,"-",{"$f":"+AX813","v":3.25},null,")²"," /",2,"+","E1",null,null,{"$f":"G830*J830^2/M830-O830*(R830-U830)^2/Y830+AA830*(AD830-AG830)^2/AK830-AM830*(AP830-AS830)^3/AW830-AY830*(BB830-BE830)^2/BI830","v":1535.9537760416665},null,null,"+","E1"]
[null,null,"(x = L) v4' =",null,null,null,{"$f":"+E817","v":-20},null,"*",{"$f":"+Z751+AJ753","v":8.75},null,"²/",2,"-",{"$f":"+L817","v":61.25},null,"*(",{"$f":"+J831","v":8.75},null,"-",{"$f":"+Q817","v":0.875},null,")²"," /",2,"+",{"$f":"+W817","v":375.60267857142856},null,"*(",{"$f":"+R831","v":8.75},null,"-",{"$f":"+AB817","v":1.75},null,")²"," /",2,"-",{"$f":"+AH817","v":455},null,"*(",{"$f":"+AD831","v":8.75},null,"-",{"$f":"+AM817","v":5.25},null,")²"," /",2,"-",{"$f":"+AS817","v":85},null,"*(",{"$f":"+AP831","v":8.75},null,"-",{"$f":"+AX817","v":3.25},null,")²"," /",2,"+",{"$f":"+BD817","v":323.14732142857144},null,"*(",{"$f":"+BB831","v":8.75},null,"-",{"$f":"+BI817","v":8.75},null,")²"," /",2,"-"]
[null,null,null,null,null,null,"-",{"$f":"+BO817","v":25},null,"*(",{"$f":"+BN831","v":8.75},null,"-",{"$f":"+BT817","v":8.75},null,")3"," /",6,"+","F1",null,null,{"$f":"G831*J831^2/M831-O831*(R831-U831)^2/Y831+AA831*(AD831-AG831)^2/AK831-AM831*(AP831-AS831)^2/AW831-AY831*(BB831-BE831)^2/BI831+BK831*(BN831-BQ831)^2/BU831-H832*(K832-N832)^3/R832","v":2464.912109375},null,null,"+","F1"]
[null,null,"(x = L) v3' = (x = L) v4' =",null,null,null,null,null,null,null,{"$f":"+BN830","v":1535.9537760416665},null,null,"+","E1","=",{"$f":"+W832","v":2464.912109375},null,null,"+","F1",null,null,"E1","-","F1","+",{"$f":"+K833-Q833","v":-928.95833333333348},null,null,"=",0,null,"(6.denklem)"]
[null,null,"(x = L) v2' =",null,null,null,{"$f":"+E809","v":-20},null,"*",{"$f":"+Z751+AF751","v":3.25},null,"²/",2,"-",{"$f":"+L809","v":61.25},null,"*(",{"$f":"+J834","v":3.25},null,"-",{"$f":"+Q809","v":0.875},null,")²"," /",2,"+",{"$f":"+W809","v":375.60267857142856},null,"*(",{"$f":"+R834","v":3.25},null,"-",{"$f":"+AB809","v":1.75},null,")²"," /",2,"-",{"$f":"+AH809","v":65},null,"*(",{"$f":"+AD834","v":3.25},null,"-",{"$f":"+AM809","v":1.75},null,")3"," /",6,"+","D1",null,null,{"$f":"G834*J834^2/M834-O834*(R834-U834)^2/Y834+AA834*(AD834-AG834)^2/AK834-AM834*(AP834-AS834)^3/AW834","v":107.62137276785711},null,null,"+","D1"]
[null,null,"(x = L) v3' =",null,null,null,{"$f":"+E813","v":-20},null,"*",{"$f":"+Z751+AF751","v":3.25},null,"²/",2,"-",{"$f":"+L813","v":61.25},null,"*(",{"$f":"+J835","v":3.25},null,"-",{"$f":"+Q813","v":0.875},null,")²"," /",2,"+",{"$f":"+W813","v":375.60267857142856},null,"*(",{"$f":"+R835","v":3.25},null,"-",{"$f":"+AB813","v":1.75},null,")²"," /",2,"-",{"$f":"+AH813","v":65},null,"*(",{"$f":"+AD835","v":3.25},null,"-",{"$f":"+AM813","v":1.75},null,")3"," /",6,"-",{"$f":"+AS813","v":85},null,"*(",{"$f":"+AP835","v":3.25},null,"-",{"$f":"+AX813","v":3.25},null,")²"," /",2,"+","E1",null,null,{"$f":"G835*J835^2/M835-O835*(R835-U835)^2/Y835+AA835*(AD835-AG835)^2/AK835-AM835*(AP835-AS835)^3/AW835-AY835*(BB835-BE835)^2/BI835","v":107.62137276785711},null,null,"+","E1"]
[null,null,"(x = L) v2' = (x = L) v3' =",null,null,null,null,null,null,null,{"$f":"+BB834","v":107.62137276785711},null,null,"+","D1","=",{"$f":"+BN835","v":107.62137276785711},null,null,"+","E1",null,null,"D1","-","E1","+",{"$f":"+K836-Q836","v":0},"=",0,null,"(7.denklem)"]
[null,null,"(x = L) v2 =",null,null,null,{"$f":"+E810","v":-20},null,"*",{"$f":"+Z751+AF751","v":3.25},null,"3/",6,"-",{"$f":"+L810","v":61.25},null,"*(",{"$f":"+J837","v":3.25},null,"-",{"$f":"+Q810","v":0.875},null,")3"," /",6,"+",{"$f":"+W810","v":375.60267857142856},null,"*(",{"$f":"+R837","v":3.25},null,"-",{"$f":"+AB810","v":1.75},null,")3"," /",6,"-",{"$f":"+AH810","v":65},null,"*(",{"$f":"+AD837","v":3.25},null,"-",{"$f":"+AM810","v":1.75},null,")4"," /",24,null,"+","D1","*",{"$f":"+AP837","v":3.25},null,"+","D2",null,null,"D1","*",{"$f":"+BB837","v":3.25},null,"+","D2","+",{"$f":"G837*J837^3/M837-O837*(R837-U837)^3/Y837+AA837*(AD837-AG837)^3/AK837-AM837*(AP837-AS837)^4/AW837","v":-53.617292131696445}]
[null,null,"(x = L) v3 =",null,null,null,{"$f":"+E814","v":-20},null,"*",{"$f":"+Z751+AF751","v":3.25},null,"3/",6,"-",{"$f":"+L814","v":61.25},null,"*(",{"$f":"+J838","v":3.25},null,"-",{"$f":"+Q814","v":0.875},null,")3"," /",6,"+",{"$f":"+W814","v":375.60267857142856},null,"*(",{"$f":"+R838","v":3.25},null,"-",{"$f":"+AB814","v":1.75},null,")3"," /",6,"-",{"$f":"+AH814","v":65},null,"*(",{"$f":"+AD838","v":3.25},null,"-",{"$f":"+AM814","v":1.75},null,")4"," /",24,null,"-",{"$f":"+AT814","v":85},null,"*(",{"$f":"+AP838","v":3.25},null,"-",{"$f":"+AY814","v":3.25},null,")3"," /",6,"+","E1","*",{"$f":"+BC838","v":3.25},null,"+","E2",null,null,"E1","*",{"$f":"+BN838","v":3.25},null,"+","E2","+",{"$f":"G838*J838^3/M838-O838*(R838-U838)^3/Y838+AA838*(AD838-AG838)^3/AK838-AM838*(AP838-AS838)^4/AW838-AZ838*(BC838-BF838)^3/BJ838","v":-53.617292131696445}]
[null,null,"(x = L) v2 = (x = L) v3 =",null,null,null,null,null,null,"D1","*",{"$f":"+BJ837","v":3.25},null,"+","D2","+",{"$f":"+BO837","v":-53.617292131696445},null,null,"=","E1","*",{"$f":"+BV838","v":3.25},null,"+","E2","+",{"$f":"+CA838","v":-53.617292131696445},null,null,null,null,"D1","*",{"$f":"+L839","v":3.25},null,"+","D2","-","E1","*",{"$f":"+W839","v":3.25},null,"-","E2","+",{"$f":"+Q839-AB839","v":0},"=",0,null,"(8.denklem)"]
[null,null,"sekiz adet denklem sekiz adet bilinmeyen çözülürse :"]
[null,null,"C1 =",null,{"$f":"+AA841","v":-766.24441964285734},null,null,null,{"$f":"+AL821","v":1.75},1,0,0,0,0,0,0,{"$f":"-AQ821","v":31.542154947916664},null,{"$f":"MINVERSE(I841:P848)","v":0},-0.14285714285714282,0.14285714285714288,0,1,0,0.7857142857142857,0.14285714285714282,{"$f":"MMULT(S841:Z848,Q841:Q848)","v":-766.24441964285734}]
[null,null,"C2 =",null,{"$f":"+AA842","v":1372.4698893229172},null,null,null,0,0,{"$f":"+BN822","v":1.75},1,0,0,0,0,{"$f":"-BS822","v":24.703369140625},null,1,0.24999999999999994,-0.25000000000000006,0,-1.75,0,-1.375,-0.24999999999999994,1372.4698893229172]
[null,null,"D1 =",null,-774.06017485119071,null,null,null,0,0,0,0,{"$f":"+K824","v":8.75},1,0,0,{"$f":"-P824","v":-5393.7178548177089},null,0,-0.14285714285714282,0.14285714285714288,0,0,0,0.7857142857142857,0.14285714285714282,-774.06017485119071]
[null,null,"D2 =",null,1379.3086751302087,null,null,null,0,0,0,0,0,0,{"$f":"+AG826","v":8.75},1,{"$f":"-AL826","v":-8645.0720214843768},null,0,1.25,-0.25000000000000006,0,0,0,-1.3749999999999998,-0.25000000000000006,1379.3086751302087]
[null,null,"E1 =",null,-774.06017485119048,null,null,null,1,0,-1,0,0,0,0,0,{"$f":"-AB829","v":7.8157552083333286},null,0,-0.14285714285714285,0.14285714285714285,0,0,0,-0.21428571428571427,0.14285714285714285,-774.06017485119048]
[null,null,"E2 =",null,1379.3086751302083,null,null,null,0,0,0,0,1,0,-1,0,{"$f":"-AB833","v":928.95833333333348},null,0,1.25,-0.24999999999999994,0,0,0,1.875,-1.25,1379.3086751302083]
[null,null,"F1 =",null,-1703.0185081845239,null,null,null,0,0,1,0,-1,0,0,0,{"$f":"-AB836","v":0},null,0,-0.14285714285714285,0.14285714285714285,0,0,-1,-0.21428571428571427,0.14285714285714285,-1703.0185081845239]
[null,null,"F2 =",null,6256.3399251302089,null,null,null,0,0,{"$f":"+AI839","v":3.25},1,{"$f":"-AP839","v":-3.25},-1,0,0,{"$f":"-AU839","v":0},null,0,1.25,-1.25,1,0,8.75,1.875,-1.25,6256.3399251302089]
[null,null,"1.ci bölgede elastik eğri denklemi"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E806","v":-20},null,"*","x3"," /",6,"-",{"$f":"+L806","v":35},null,"*","x4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"y = (",null,{"$f":"+H850","v":-20},null,"*","x3"," /",6,"-",{"$f":"+O850","v":35},null,"*","x4"," /",24,null,"+",{"$f":"+E841","v":-766.24441964285734},null,null,"*","x","+",{"$f":"+E842","v":1372.4698893229172},null,null,") * 108 / ( E * I )"]
[null,null,"x=",0,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D852<=Z751,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E851","v":-20},null,"*",{"$f":"+D852","v":0},null,"3/",6,"-",{"$f":"+L851","v":35},null,"*",{"$f":"+H853","v":0},null,"4/",24,null,"+",{"$f":"+T851","v":-766.24441964285734},null,null,"*",{"$f":"+P853","v":0},null,"+",{"$f":"+Z851","v":1372.4698893229172},null,null,")* 108 / (",null,null,{"$f":"+F757","v":200000},null,null,"*",{"$f":"+F756","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E853*H853^3/K853-M853*P853^4/S853+V853*Z853+AC853)*100000000/(AI853*AM853)","v":7.4525949680870829},null,null,"mm"]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"+Z751*1000","v":1750},null,null," /",150,null,"=",{"$f":"+H855/L855","v":11.666666666666666},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E854","v":7.4525949680870829},null,null,"mm",null,{"$f":"IF(ABS(D856)<ABS(M856),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O855","v":11.666666666666666},null,null,"mm",null,{"$f":"IF(ABS(D856)<ABS(M856),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"2.ci bölgede elastik eğri denklemi"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E810","v":-20},null,"*","x3"," /",6,"-",{"$f":"+L810","v":61.25},null,"*(","x","-",{"$f":"+Q810","v":0.875},null,")3"," /",6,"+",{"$f":"+W810","v":375.60267857142856},null,"*(","x","-",{"$f":"+AB810","v":1.75},null,")3"," /",6,"-",{"$f":"+AH810","v":65},null,"*(","x","-",{"$f":"+AM810","v":1.75},null,")4"," /",24,null,"+","D1","*","x","+","D2"]
[null,null,"y = (",null,{"$f":"+H858","v":-20},null,"*","x3"," /",6,"-",{"$f":"+O858","v":61.25},null,"*(","x","-",{"$f":"+T858","v":0.875},null,")3"," /",6,"+",{"$f":"+Z858","v":375.60267857142856},null,"*(","x","-",{"$f":"+AE858","v":1.75},null,")3"," /",6,"-",{"$f":"+AK858","v":65},null,"*(","x","-",{"$f":"+AP858","v":1.75},null,")4"," /",24,null,"+",{"$f":"+E843","v":-774.06017485119071},null,null,"*","x","+",{"$f":"+E844","v":1379.3086751302087},null,null,") * 108 / ( E * I )"]
[null,null,"x=",2,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D860<=Z751,\"artır.\",IF(D860>(AF751+Z751),\"azalt.\",\"\"))","v":""}]
[null,null,"y = (",null,{"$f":"+E859","v":-20},null,"*",{"$f":"+D860","v":2},null,"3/",6,"-",{"$f":"+O858","v":61.25},null,"*(",{"$f":"+H861","v":2},null,"-",{"$f":"+T858","v":0.875},null,")3"," /",6,"+",{"$f":"+Z858","v":375.60267857142856},null,"*(",{"$f":"+P861","v":2},null,"-",{"$f":"+AE858","v":1.75},null,")3"," /",6,"-",{"$f":"+AK858","v":65},null,"*(",{"$f":"+AB861","v":2},null,"-",{"$f":"+AP858","v":1.75},null,")4"," /",24,null,"+",{"$f":"+E843","v":-774.06017485119071},null,null,"*",{"$f":"+AN861","v":2},null,"+",{"$f":"+E844","v":1379.3086751302087},null,null,")* 108 / (",null,null,{"$f":"+AI853","v":200000},null,null,"*",{"$f":"+AM853","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E861*H861^3/K861-M861*(P861-S861)^3/W861+Y861*(AB861-AE861)^3/AI861-AK861*(AN861-AQ861)^4/AU861+AX861*BB861+BE861)*100000000/(BK861*BO861)","v":-1.1351308688089237},null,null,"mm"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"+AJ753*1000","v":7000},null,null," /",300,null,"=",{"$f":"+H863/L863","v":23.333333333333332},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E862","v":-1.1351308688089237},null,null,"mm",null,{"$f":"IF(ABS(D864)<ABS(M864),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O863","v":23.333333333333332},null,null,"mm",null,{"$f":"IF(ABS(D864)<ABS(M864),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"3.cü bölgede elastik eğri denklemi"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E814","v":-20},null,"*","x3"," /",6,"-",{"$f":"+L814","v":61.25},null,"*(","x","-",{"$f":"+Q814","v":0.875},null,")3"," /",6,"+",{"$f":"+W814","v":375.60267857142856},null,"*(","x","-",{"$f":"+AB814","v":1.75},null,")3"," /",6,"-",{"$f":"+AH814","v":65},null,"*(","x","-",{"$f":"+AM814","v":1.75},null,")4"," /",24,null,"-",{"$f":"+AT814","v":85},null,"*(","x","-",{"$f":"+AY814","v":3.25},null,")3"," /",6,"+","E1","*","x","+","E2"]
[null,null,"y = (",null,{"$f":"+H866","v":-20},null,"*","x3"," /",6,"-",{"$f":"+O866","v":61.25},null,"*(","x","-",{"$f":"+T866","v":0.875},null,")3"," /",6,"+",{"$f":"+Z866","v":375.60267857142856},null,"*(","x","-",{"$f":"+AE866","v":1.75},null,")3"," /",6,"-",{"$f":"+AK866","v":65},null,"*(","x","-",{"$f":"+AP866","v":1.75},null,")4"," /",24,null,"-",{"$f":"+AW866","v":85},null,"*(","x","-",{"$f":"+BB866","v":3.25},null,")3"," /",6,"+",{"$f":"+E845","v":-774.06017485119048},null,null,"*","x","+",{"$f":"+E846","v":1379.3086751302083},null,null,") * 108 / ( E * I )"]
[null,null,"x=",4.5,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D868<=(Z751+AF751),\"artır.\",IF(D868>(AF751+Z751+AM751),\"azalt.\",\"\"))","v":""}]
[null,null,"y = (",null,{"$f":"+E867","v":-20},null,"*",{"$f":"+D868","v":4.5},null,"3/",6,"-",{"$f":"+O866","v":61.25},null,"*(",{"$f":"+H869","v":4.5},null,"-",{"$f":"+T866","v":0.875},null,")3"," /",6,"+",{"$f":"+Z866","v":375.60267857142856},null,"*(",{"$f":"+P869","v":4.5},null,"-",{"$f":"+AE866","v":1.75},null,")3"," /",6,"-",{"$f":"+AK866","v":65},null,"*(",{"$f":"+AB869","v":4.5},null,"-",{"$f":"+AP866","v":1.75},null,")4"," /",24,"-",{"$f":"+AW866","v":85},null,"*(",{"$f":"+AN869","v":4.5},null,"-",{"$f":"+BB866","v":3.25},null,")3"," /",6,"+",{"$f":"+BE867","v":-774.06017485119048},null,null,"*",{"$f":"+AZ869","v":4.5},null,"+",{"$f":"+E846","v":1379.3086751302083},null,null,")* 108 / (",null,null,{"$f":"+BK861","v":200000},null,null,"*",{"$f":"+BO861","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E869*H869^3/K869-M869*(P869-S869)^3/W869+Y869*(AB869-AE869)^3/AI869-AK869*(AN869-AQ869)^4/AU869-AW869*(AZ869-BC869)^3/BG869+BI869*BM869+BP869)*100000000/(BV869*BZ869)","v":-9.6364719857546568},null,null,"mm"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"+AJ753*1000","v":7000},null,null," /",300,null,"=",{"$f":"+H871/L871","v":23.333333333333332},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E870","v":-9.6364719857546568},null,null,"mm",null,{"$f":"IF(ABS(D872)<ABS(M872),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O871","v":23.333333333333332},null,null,"mm",null,{"$f":"IF(ABS(D872)<ABS(M872),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"4.cü bölgede elastik eğri denklemi"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E818","v":-20},null,"*","x3"," /",6,"-",{"$f":"+L818","v":61.25},null,"*(","x","-",{"$f":"+Q818","v":0.875},null,")3"," /",6,"+",{"$f":"+W818","v":375.60267857142856},null,"*(","x","-",{"$f":"+AB818","v":1.75},null,")3"," /",6,"-",{"$f":"+AH818","v":455},null,"*(","x","-",{"$f":"+AM818","v":5.25},null,")3"," /",6,"-",{"$f":"+AS818","v":85},null,"*(","x","-",{"$f":"+AX818","v":3.25},null,")3"," /",6,"+",{"$f":"+BD818","v":323.14732142857144},null,"*(","x","-",{"$f":"+BI818","v":8.75},null,")3"," /",6,"-",{"$f":"+BO818","v":25},null,"*(","x","-",{"$f":"+BT818","v":8.75},null,")4"," /",24,null,"+"]
[null,null,null,null,null,null,"+","F1","*","x","+","F2"]
[null,null,"y = (",null,{"$f":"+H874","v":-20},null,"*","x3"," /",6,"-",{"$f":"+O874","v":61.25},null,"*(","x","-",{"$f":"+T874","v":0.875},null,")3"," /",6,"+",{"$f":"+Z874","v":375.60267857142856},null,"*(","x","-",{"$f":"+AE874","v":1.75},null,")3"," /",6,"-",{"$f":"+AK874","v":455},null,"*(","x","-",{"$f":"+AP874","v":5.25},null,")3"," /",6,"-",{"$f":"+AV874","v":85},null,"*(","x","-",{"$f":"+BA874","v":3.25},null,")3"," /",6,"+",{"$f":"+BG874","v":323.14732142857144},null,"*(","x","-",{"$f":"+BL874","v":8.75},null,")3"," /",6,"-",{"$f":"+BR874","v":25},null,"*(","x","-",{"$f":"+BW874","v":8.75},null,")4"," /",24,null,"+"]
[null,null,null,null,"+",{"$f":"+E847","v":-1703.0185081845239},null,null,"*","x","+",{"$f":"+E848","v":6256.3399251302089},null,null,") * 108 / ( E * I )"]
[null,null,"x=",10.25,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D878<=(Z751+AF751+AM751),\"artır.\",IF(D878>(AF751+Z751+AM751+AT751),\"azalt.\",\"\"))","v":""}]
[null,null,"y = (",null,{"$f":"+E876","v":-20},null,"*",{"$f":"+D878","v":10.25},null,"3/",6,"-",{"$f":"+L876","v":61.25},null,"*(",{"$f":"+H879","v":10.25},null,"-",{"$f":"+Q876","v":0.875},null,")3"," /",6,"+",{"$f":"+W876","v":375.60267857142856},null,"*(",{"$f":"+P879","v":10.25},null,"-",{"$f":"+AB876","v":1.75},null,")3"," /",6,"-",{"$f":"+AH876","v":455},null,"*(",{"$f":"+AB879","v":10.25},null,"-",{"$f":"+AM876","v":5.25},null,")3"," /",6,"-",{"$f":"+AS876","v":85},null,"*(",{"$f":"+AB879","v":10.25},null,"-",{"$f":"+AX876","v":3.25},null,")3"," /",6,"-",{"$f":"+BD876","v":323.14732142857144},null,"*(",{"$f":"+AN879","v":10.25},null,"-",{"$f":"+BI876","v":8.75},null,")3"," /",6]
[null,null,null,null,"-",{"$f":"+BO876","v":25},null,"*(",{"$f":"+BL879","v":10.25},null,"-",{"$f":"+BT876","v":8.75},null,")4"," /",24,null,"+",{"$f":"+F877","v":-1703.0185081845239},null,null,"*",{"$f":"+I880","v":10.25},null,"+",{"$f":"+L877","v":6256.3399251302089},null,null,")* 108 / (",null,null,{"$f":"+BV869","v":200000},null,null,"*",{"$f":"+BZ869","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E879*H879^3/K879-M879*(P879-S879)^3/W879+Y879*(AB879-AE879)^3/AI879-AK879*(AN879-AQ879)^3/AU879-AW879*(AZ879-BC879)^3/BG879-BI879*(BL879-BO879)^3/BS879-F880*(I880-L880)^4/P880+S880*W880+Z880)*100000000/(AF880*AJ880)","v":3.9013865805743704},null,null,"mm"]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"+AT751*1000","v":1500},null,null," /",150,null,"=",{"$f":"+H882/L882","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E881","v":3.9013865805743704},null,null,"mm",null,{"$f":"IF(ABS(D883)<ABS(M883),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O882","v":10},null,null,"mm",null,{"$f":"IF(ABS(D883)<ABS(M883),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK TEK AÇIKLIKLI ANKASTRE KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,null,"KN"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK920","v":2.388570349959549}]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O889,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ma =",null,{"$f":"E933","v":-286.84204101562494},null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mb =",null,{"$f":"+E940","v":-356.51733398437494},null,"KNm",null,null,"Max =",null,{"$f":"ABS(AL912)","v":356.517333984375},null,null,"KNm",null,"(max moment)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(BL895),ABS(BM895),ABS(BN895))","v":252.22503662109375},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O889,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AB898","v":145.27496337890625},{"$f":"+BL895-AJ889","v":-4.72503662109375},{"$f":"+BM895-AR891*AR899","v":-252.22503662109375}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x"]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O889,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E934","v":145.27496337890625},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E937","v":252.22503662109375},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.5,null,"m",null,null,null,null,null,null,null,null,null,{"$f":"+AN901-AF899","v":4.5},null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O889,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",8,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O889,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)",null,null,null,null,null,null,null,null,null,null,null,null,null,"x = 0 ; v' = 0",null,null,null,null,null,null,null,null,null,null,"Uygunluk koşulları",null,null,null,null,null,null,null,null,null,null,null,"x = L ; v' = 0",null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[]
[null,null,"ARA KESİT TESİRLERİ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = 0 ; v = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v = 0"]
[null,null,"x=",5,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D907<=AN901,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+W893","v":-286.84204101562494},null,null,"+",{"$f":"+AB898","v":145.27496337890625},null,null,"*",{"$f":"+D907","v":5},null,"-",{"$f":"IF((S908-V908)<0,0,AJ889)","v":150},null,"*(",{"$f":"+D907","v":5},null,"-",{"$f":"+AF899","v":3.5},null,")-",{"$f":"IF((AB908-AE908)<0,0,AR891)","v":55},null,"*(",{"$f":"+S908","v":5},null,"-",{"$f":"+AF899","v":3.5},null,")²"," /",2,"=",{"$f":"+E908+I908*M908-P908*(S908-V908)-Y908*(AB908-AE908)^2/AI908","v":152.65777587890631},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+I908","v":145.27496337890625},null,"-",{"$f":"+P908","v":150},null,"-",{"$f":"+Y908","v":55},null,"*(",{"$f":"+D907","v":5},null,"-",{"$f":"+AF899","v":3.5},null,")=",{"$f":"+E909-H909-K909*(N909-Q909)","v":-87.22503662109375},null,null,"KNm"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"x=",{"$f":"+BA911","v":8},null,null,"m. ' deki max moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,{"$f":"ABS(+W893)","v":286.84204101562494},null,{"$f":"MAX(AW911,AW912,AW913,AW914)","v":356.51733398437494},null,{"$f":"INDEX(AU911:AU914,MATCH(AY911,AW911:AW914,0),0)","v":8}]
[null,null,"Mmax =",null,null,{"$f":"+W893","v":-286.84204101562494},null,null,"+",{"$f":"+AB898","v":145.27496337890625},null,null,"*",{"$f":"+D911","v":8},null,"-",{"$f":"IF((T912-W912)<0,0,AJ889)","v":150},null,"*(",{"$f":"+D911","v":8},null,"-",{"$f":"+AF899","v":3.5},null,")-",{"$f":"IF((AC912-AF912)<0,0,AR891)","v":55},null,"*(",{"$f":"+T912","v":8},null,"-",{"$f":"+AF899","v":3.5},null,")²"," /",2,"=",{"$f":"+F912+J912*N912-Q912*(T912-W912)-Z912*(AC912-AF912)^2/AJ912","v":-356.517333984375},null,null,"KNm",null,null,null,null,null,{"$f":"+AF899","v":3.5},null,{"$f":"ABS(W893+AB898*AF899)","v":221.62033081054693}]
[null,null,"L / 2 =",null,{"$f":"+AN901/2","v":4},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AB898-AJ889+AR891*AF899)/AR891","v":3.4140902432528408},null,{"$f":"ABS(W893+AB898*AU913-IF((AU913-P922)<0,0,K922)*(AU913-P922)-IF((AU913-X922)<0,0,S922)*(AU913-X922)^2/AB922)","v":209.13979404521262}]
[null,null,"MB =",null,null,{"$f":"+F912","v":-286.84204101562494},null,null,"+",{"$f":"+J912","v":145.27496337890625},null,null,"*",{"$f":"+E913","v":4},null,"-",{"$f":"IF((T914-W914)<0,0,AJ889)","v":150},null,"*(",{"$f":"+E913","v":4},null,"-",{"$f":"+W912","v":3.5},null,")-",{"$f":"IF((AC914-AF914)<0,0,AR891)","v":55},null,"*(",{"$f":"+T914","v":4},null,"-",{"$f":"+AF912","v":3.5},null,")²"," /",2,"=",{"$f":"+F914+J914*N914-Q914*(T914-W914)-Z914*(AC914-AF914)^2/AJ914","v":212.38281250000006},null,null,"KNm",null,null,null,null,null,{"$f":"+AN901","v":8},null,{"$f":"ABS(BD893)","v":356.51733398437494}]
[null,null,"L / 4 =",null,{"$f":"+AN901/4","v":2},null,null,"m. ' deki moment miktarı"]
[null,null,"MA =",null,null,{"$f":"+F914","v":-286.84204101562494},null,null,"+",{"$f":"+J914","v":145.27496337890625},null,null,"*",{"$f":"+E915","v":2},null,"-",{"$f":"IF((T916-W916)<0,0,AJ889)","v":0},null,"*(",{"$f":"+E915","v":2},null,"-",{"$f":"+W914","v":3.5},null,")-",{"$f":"IF((AC916-AF916)<0,0,AR891)","v":0},null,"*(",{"$f":"+T916","v":2},null,"-",{"$f":"+AF914","v":3.5},null,")²"," /",2,"=",{"$f":"+F916+J916*N916-Q916*(T916-W916)-Z916*(AC916-AF916)^2/AJ916","v":3.7078857421875568},null,null,"KNm"]
[null,null,"3 * L / 4 =",null,null,{"$f":"+AN901*3/4","v":6},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,null,{"$f":"+F916","v":-286.84204101562494},null,null,"+",{"$f":"+J916","v":145.27496337890625},null,null,"*",{"$f":"+F917","v":6},null,"-",{"$f":"IF((T918-W918)<0,0,AJ889)","v":150},null,"*(",{"$f":"+F917","v":6},null,"-",{"$f":"+W916","v":3.5},null,")-",{"$f":"IF((AC918-AF918)<0,0,AR891)","v":55},null,"*(",{"$f":"+T918","v":6},null,"-",{"$f":"+AF916","v":3.5},null,")²"," /",2,"=",{"$f":"+F918+J918*N918-Q918*(T918-W918)-Z918*(AC918-AF918)^2/AJ918","v":37.9327392578125},null,null,"KNm"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AL912)","v":356.517333984375},null,null," /(",2.5,null,"*",{"$f":"+H920","v":356.517333984375},null,null,"+",3,"*",{"$f":"ABS(AL916)","v":3.7078857421875568},null,null,"+",4,"*",{"$f":"ABS(AL914)","v":212.38281250000006},null,null,"+",3,"*",{"$f":"ABS(AL918)","v":37.9327392578125},null,null,")=",{"$f":"E920*H920/(L920*O920+S920*U920+Y920*AA920+AE920*AG920)","v":2.388570349959549}]
[null,null,"SEHİM HESABI"]
[null,null,"v'' =",null,"Ma +",null,"A","*","x","-",{"$f":"+AJ889","v":150},null,"*(","x","-",{"$f":"+AF899","v":3.5},null,")-",{"$f":"+AR891","v":55},null,"*(","x","-",{"$f":"+AF899","v":3.5},null,")²"," /",2]
[null,null,"v' =",null,"Ma  *",null,"x","+","A","*","x²"," /",2,"-",{"$f":"+K922","v":150},null,"*(","x","-",{"$f":"+P922","v":3.5},null,")²"," /",2,"-",{"$f":"+S922","v":55},null,"*(","x","-",{"$f":"+X922","v":3.5},null,")3"," /",6,"+","C1"]
[null,null,"v =",null,"Ma  *",null,"x²"," /",2,"+","A","*","x3"," /",6,"-",{"$f":"+O923","v":150},null,"*(","x","-",{"$f":"+T923","v":3.5},null,")3"," /",6,"-",{"$f":"+Z923","v":55},null,"*(","x","-",{"$f":"+AE923","v":3.5},null,")4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"x = 0 ; v = 0",null,null,null,null,null,"C2 = 0"]
[null,null,"x = 0 ; v' = 0",null,null,null,null,null,"C1 = 0"]
[null,null,"x = L ; v = 0",null,null,null,null,null,"Ma  *",null,{"$f":"+AN901","v":8},null,"² /",2,"+","A","*",{"$f":"+K928","v":8},null,"3 /",6,"-",{"$f":"IF((Z928-AC928)<0,0,Q924)","v":150},null,"*(",{"$f":"+R928","v":8},null,"-",{"$f":"+V924","v":3.5},null,")3"," /",6,"-",{"$f":"IF((AL928-AO928)<0,0,AB924)","v":55},null,"*(",{"$f":"+Z928","v":8},null,"-",{"$f":"+AG924","v":3.5},null,")4"," /",24,null,"=",0]
[null,null,null,null,null,null,null,null,"Ma  *",null,{"$f":"K928^2/N928","v":32},null,"+","A","*",{"$f":"+R928^3/U928","v":85.333333333333329},null,"+",{"$f":"-W928*(Z928-AC928)^3/AG928-AI928*(AL928-AO928)^4/AS928","v":-3217.8515625},null,null,"=",0,null,"(1. denklem)"]
[null,null,"x = L ; v' = 0",null,null,null,null,null,"Ma  *",null,{"$f":"+AN901","v":8},null,"+","A","*",{"$f":"+AN901","v":8},null,"² /",2,"-",{"$f":"IF((X930-AA930)<0,0,O923)","v":150},null,"*(",{"$f":"+P930","v":8},null,"-",{"$f":"+T923","v":3.5},null,")²"," /",2,"-",{"$f":"IF((AJ930-AM930)<0,0,Z923)","v":55},null,"*(",{"$f":"+X930","v":8},null,"-",{"$f":"+AE923","v":3.5},null,")3"," /",6,"=",0]
[null,null,null,null,null,null,null,null,"Ma  *",null,{"$f":"+K930","v":8},null,"+","A","*",{"$f":"+P930^2/S930","v":32},null,"+",{"$f":"-U930*(X930-AA930)^2/AE930-AG930*(AJ930-AM930)^3/AQ930","v":-2354.0625},null,null,"=",0,null,"(2. denklem)"]
[null,null,"iki adet denklem iki adet bilinmeyen çözülürse :"]
[null,null,"Ma =",null,{"$f":"+N933","v":-286.84204101562494},null,null,null,{"$f":"+K929","v":32},{"$f":"+P929","v":85.333333333333329},{"$f":"-S929","v":3217.8515625},{"$f":"MINVERSE(I933:J934)","v":9.3749999999999986E-2},-0.24999999999999994,{"$f":"MMULT(L933:M934,K933:K934)","v":-286.84204101562494}]
[null,null,"A =",null,{"$f":"+N934","v":145.27496337890625},null,null,null,{"$f":"+K931","v":8},{"$f":"+P931","v":32},{"$f":"-S931","v":2354.0625},-2.3437499999999997E-2,9.3749999999999986E-2,145.27496337890625]
[null,null,"düşey denge denkleminden"]
[null,null,"B","+","A","-",{"$f":"+AJ889","v":150},null,"-",{"$f":"+AR891","v":55},null,"*",{"$f":"+AR899","v":4.5},null,"=",0]
[null,null,"B","=",{"$f":"+G936+J936*M936-E934","v":252.22503662109375},null,null,"KN"]
[null,null,"sağ konsola göre moment alınırsa"]
[null,null,"Ma +",null,{"$f":"+AB898","v":145.27496337890625},null,"*",{"$f":"+AN901","v":8},null,"-",{"$f":"+AJ889","v":150},null,"*",{"$f":"+AR899","v":4.5},null,"-",{"$f":"+AR891","v":55},null,"*",{"$f":"+AR899","v":4.5},null,"*",{"$f":"+T939/2","v":2.25},null,"-","Mb = 0"]
[null,null,"Mb =",null,{"$f":"+E939*H939-K939*N939-Q939*T939*W939+E933","v":-356.51733398437494},null,null,"KN"]
[null,null,"E * I / 108 * y =",null,null,null,null,"Ma  *",null,"x²"," /",2,"+","A","*","x3"," /",6,"-",{"$f":"+Q924","v":150},null,"*(","x","-",{"$f":"+V924","v":3.5},null,")3"," /",6,"-",{"$f":"+AB924","v":55},null,"*(","x","-",{"$f":"+AG924","v":3.5},null,")4"," /",24]
[null,null,"x=",4,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D942<=AN901,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E933","v":-286.84204101562494},null,null,"*",{"$f":"+D942","v":4},null,"² /",2,"+",{"$f":"+E934","v":145.27496337890625},null,null,"*",{"$f":"+D942","v":4},null,"3 /",6,"-",{"$f":"IF((Z943-AC943)<0,0,Q924)","v":150},null,"*(",{"$f":"+R943","v":4},null,"-",{"$f":"+V924","v":3.5},null,")3"," /",6,"-",{"$f":"IF((AL943-AO943)<0,0,AB924)","v":55},null,"*(",{"$f":"+Z943","v":4},null,"-",{"$f":"+AG924","v":3.5},null,")4"," /",24,null,")* 108 / (",null,null,{"$f":"+F904","v":200000},null,null,"*",{"$f":"+F903","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E943*I943^2/L943+N943*R943^3/U943-W943*(Z943-AC943)^3/AG943-AI943*(AL943-AO943)^4/AS943)*100000000/(AX943*BB943)","v":-4.0638843826925832},null,null,"mm"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"AN901*1000","v":8000},null,null," /",300,null,"=",{"$f":"+H945/L945","v":26.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E944","v":-4.0638843826925832},null,null,"mm",null,{"$f":"IF(ABS(D946)<ABS(M946),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O945","v":26.666666666666668},null,null,"mm",null,{"$f":"IF(ABS(D946)<ABS(M946),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK TEK AÇIKLIKLI BASİT KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,null,"KN"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK988","v":1.216582766266489}]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O952,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"ABS(AH980)","v":539.08963290127849},null,null,"KNm",null,"(max moment)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(BK958),ABS(BL958),ABS(BM958))","v":243.515625},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O952,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AB961","v":153.984375},{"$f":"+BK958-AJ952","v":3.984375},{"$f":"+BL958-AR954*AR962","v":-243.515625}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x"]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O952,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E971","v":153.984375},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E973","v":243.515625},null,"KN",null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.5,null,"m",null,null,null,null,null,null,null,null,null,{"$f":"+AN964-AF962","v":4.5},null,"m",null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O952,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",8,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[]
[null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O952,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)"]
[null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[]
[null,null,"MESNET TEPKİLERİ ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( x = 0) v = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( x = L) v = 0"]
[null,null,"A","*",{"$f":"+AN964","v":8},null,"-",{"$f":"+AJ952","v":150},null,"*",{"$f":"+AR962","v":4.5},null,"-",{"$f":"+AR954","v":55},null,"*",{"$f":"+AR962","v":4.5},null,"*",{"$f":"+Q970/2","v":2.25},null,"=",0]
[null,null,"A =",null,{"$f":"(H970*K970+N970*Q970*T970)/E970","v":153.984375},null,null,"KN"]
[null,null,"A","*","B","-",{"$f":"+AJ952","v":150},null,"-",{"$f":"+AR954","v":55},null,"*",{"$f":"+AR962","v":4.5},null,"=",0]
[null,null,"B =",null,{"$f":"+G972+J972*M972-E971","v":243.515625},null,null,"KN"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"x=",3,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D975<=AN964,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+AB961","v":153.984375},null,null,"*",{"$f":"+D975","v":3},null,"-",{"$f":"IF((O976-R976)<0,0,AJ952)","v":0},null,"*(",{"$f":"+D975","v":3},null,"-",{"$f":"+AF962","v":3.5},null,")-",{"$f":"IF((X976-AA976)<0,0,AR954)","v":0},null,"*(",{"$f":"+O976","v":3},null,"-",{"$f":"+AF962","v":3.5},null,")²"," /",2,"=",{"$f":"E976*I976-L976*(O976-R976)-U976*(X976-AA976)^2/AE976","v":461.953125},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E976","v":153.984375},null,null,"-",{"$f":"+L976","v":0},null,"-",{"$f":"+U976","v":0},null,"*(",{"$f":"+D975","v":3},null,"-",{"$f":"+AF962","v":3.5},null,")=",{"$f":"+E977-I977-L977*(O977-R977)","v":153.984375},null,null,"KNm"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"x=",{"$f":"+BB979","v":3.5724431818181817},null,null,"m. ' deki max moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AF962","v":3.5},null,{"$f":"+AB961*AF962","v":538.9453125},null,{"$f":"MAX(AX979:AX980)","v":539.08963290127849},null,{"$f":"INDEX(AV979:AV980,MATCH(AZ979,AX979:AX980,0),0)","v":3.5724431818181817}]
[null,null,"Mmax =",null,null,{"$f":"+AB961","v":153.984375},null,null,"*",{"$f":"+D979","v":3.5724431818181817},null,"-",{"$f":"IF((P980-S980)<0,0,AJ952)","v":150},null,"*(",{"$f":"+D979","v":3.5724431818181817},null,"-",{"$f":"+AF962","v":3.5},null,")-",{"$f":"IF((Y980-AB980)<0,0,AR954)","v":55},null,"*(",{"$f":"+P980","v":3.5724431818181817},null,"-",{"$f":"+AF962","v":3.5},null,")²"," /",2,"=",{"$f":"F980*J980-M980*(P980-S980)-V980*(Y980-AB980)^2/AF980","v":539.08963290127849},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,{"$f":"(AB961-AJ952+AR954*AF962)/AR954","v":3.5724431818181817},null,{"$f":"E990*AV980-IF((AV980-P990)<0,0,K990)*(AV980-P990)-IF((AV980-X990)<0,0,S990)*(AV980-X990)^2/AB990","v":539.08963290127849}]
[null,null,"L / 2 =",null,{"$f":"+AN964/2","v":4},null,null,"m. ' deki moment miktarı"]
[null,null,"MB =",null,{"$f":"+F980","v":153.984375},null,null,"*",{"$f":"+E981","v":4},null,"-",{"$f":"IF((O982-R982)<0,0,AJ952)","v":150},null,"*(",{"$f":"+E981","v":4},null,"-",{"$f":"+S980","v":3.5},null,")-",{"$f":"IF((X982-AA982)<0,0,AR954)","v":55},null,"*(",{"$f":"+O982","v":4},null,"-",{"$f":"+AB980","v":3.5},null,")²"," /",2,"=",{"$f":"E982*I982-L982*(O982-R982)-U982*(X982-AA982)^2/AE982","v":534.0625},null,null,"KNm"]
[null,null,"L / 4 =",null,{"$f":"+AN964/4","v":2},null,null,"m. ' deki moment miktarı"]
[null,null,"MA =",null,{"$f":"+E982","v":153.984375},null,null,"*",{"$f":"+E983","v":2},null,"-",{"$f":"IF((O984-R984)<0,0,AJ952)","v":0},null,"*(",{"$f":"+E983","v":2},null,"-",{"$f":"+R982","v":3.5},null,")-",{"$f":"IF((X984-AA984)<0,0,AR954)","v":0},null,"*(",{"$f":"+O984","v":2},null,"-",{"$f":"+AA982","v":3.5},null,")²"," /",2,"=",{"$f":"E984*I984-L984*(O984-R984)-U984*(X984-AA984)^2/AE984","v":307.96875},null,null,"KNm"]
[null,null,"3 * L / 4 =",null,null,{"$f":"+AN964*3/4","v":6},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,{"$f":"+E984","v":153.984375},null,null,"*",{"$f":"+F985","v":6},null,"-",{"$f":"IF((O986-R986)<0,0,AJ952)","v":150},null,"*(",{"$f":"+F985","v":6},null,"-",{"$f":"+R984","v":3.5},null,")-",{"$f":"IF((X986-AA986)<0,0,AR954)","v":55},null,"*(",{"$f":"+O986","v":6},null,"-",{"$f":"+AA984","v":3.5},null,")²"," /",2,"=",{"$f":"E986*I986-L986*(O986-R986)-U986*(X986-AA986)^2/AE986","v":377.03125},null,null,"KNm"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AH980)","v":539.08963290127849},null,null," /(",2.5,null,"*",{"$f":"+H988","v":539.08963290127849},null,null,"+",3,"*",{"$f":"ABS(AG984)","v":307.96875},null,null,"+",4,"*",{"$f":"ABS(AG982)","v":534.0625},null,null,"+",3,"*",{"$f":"ABS(AG986)","v":377.03125},null,null,")=",{"$f":"E988*H988/(L988*O988+S988*U988+Y988*AA988+AE988*AG988)","v":1.216582766266489}]
[null,null,"SEHİM HESABI"]
[null,null,"v'' =",null,{"$f":"+AB961","v":153.984375},null,null,"*","x","-",{"$f":"+AJ952","v":150},null,"*(","x","-",{"$f":"+AF962","v":3.5},null,")-",{"$f":"+AR954","v":55},null,"*(","x","-",{"$f":"+AF962","v":3.5},null,")²"," /",2]
[null,null,"v' =",null,{"$f":"+E990","v":153.984375},null,null,"*","x²"," /",2,"-",{"$f":"+K990","v":150},null,"*(","x","-",{"$f":"+P990","v":3.5},null,")²"," /",2,"-",{"$f":"+S990","v":55},null,"*(","x","-",{"$f":"+X990","v":3.5},null,")3"," /",6,"+","C1"]
[null,null,"v =",null,{"$f":"+E991","v":153.984375},null,null,"*","x3"," /",6,"-",{"$f":"+M991","v":150},null,"*(","x","-",{"$f":"+R991","v":3.5},null,")3"," /",6,"-",{"$f":"+X991","v":55},null,"*(","x","-",{"$f":"+AC991","v":3.5},null,")4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"x = 0 ; v = 0",null,null,null,null,null,"C2 = 0"]
[null,null,"x = L ; v = 0",null,null,null,null,null,{"$f":"+E992","v":153.984375},null,null,"*",{"$f":"+AN964","v":8},null,"3 /",6,"-",{"$f":"+M992","v":150},null,"*(",{"$f":"+AN964","v":8},null,"-",{"$f":"+R992","v":3.5},null,")3"," /",6,"-",{"$f":"+X992","v":55},null,"*(",{"$f":"+U995","v":8},null,"-",{"$f":"+AC992","v":3.5},null,")4"," /",24,null,"+","C1","*",{"$f":"+AN964","v":8},null,"=",0,null,null,"C1 =",null,{"$f":"-(I995*M995^3/P995-R995*(U995-X995)^3/AB995-AD995*(AG995-AJ995)^4/AN995)/AS995","v":-1240.2685546875}]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E992","v":153.984375},null,null,"*","x3"," /",6,"-",{"$f":"+M992","v":150},null,"*(","x","-",{"$f":"+R992","v":3.5},null,")3"," /",6,"-",{"$f":"+X992","v":55},null,"*(","x","-",{"$f":"+AC992","v":3.5},null,")4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"y = (",null,{"$f":"+H996","v":153.984375},null,null,"*","x3"," /",6,"-",{"$f":"+P996","v":150},null,"*(","x","-",{"$f":"+U996","v":3.5},null,")3"," /",6,"-",{"$f":"+AA996","v":55},null,"*(","x","-",{"$f":"+AF996","v":3.5},null,")4"," /",24,null,"+",{"$f":"+BA995","v":-1240.2685546875},null,null,"*","x",") * 108 / ( E * I )"]
[null,null,"x=",4,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D998<=AN964,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E997","v":153.984375},null,null,"*",{"$f":"+D998","v":4},null,"3 /",6,"-",{"$f":"IF((Q999-T999)<0,0,AJ952)","v":150},null,"*(",{"$f":"+I999","v":4},null,"-",{"$f":"+R997","v":3.5},null,")3"," /",6,"-",{"$f":"IF((AC999-AF999)<0,0,AR954)","v":55},null,"*(",{"$f":"+Q999","v":4},null,"-",{"$f":"+AC997","v":3.5},null,")4"," /",24,null,"+",{"$f":"+AJ997","v":-1240.2685546875},null,null,"*",{"$f":"+AC999","v":4},null,")* 108 / (",null,null,{"$f":"+F967","v":200000},null,null,"*",{"$f":"+F966","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E999*I999^3/L999-N999*(Q999-T999)^3/X999-Z999*(AC999-AF999)^4/AJ999+AM999*AQ999)*100000000/(AV999*AZ999)","v":-18.037806515620478},null,null,"mm"]
[null,null,"y=",{"$f":"+E1000","v":-18.037806515620478},null,null,"mm",null,{"$f":"IF(ABS(D1002)<ABS(M1002),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O1001","v":26.666666666666668},null,null,"mm",null,{"$f":"IF(ABS(D1002)<ABS(M1002),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(BL1014),ABS(BM1014),ABS(BN1014))","v":212.12196350097653},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O1008,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AB1017","v":212.12196350097653},{"$f":"+BL1014-AJ1008","v":62.121963500976534},{"$f":"+BM1014-AR1010*AR1018","v":-185.37803649902347}]
[]
[]
[null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = 0 ; v = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v = 0"]
[null,null,"Mx =",null,{"$f":"+W1012","v":-465.10070800781239},null,null,"+",{"$f":"+AB1017","v":212.12196350097653},null,null,"*",{"$f":"+D1027","v":5},null,"-",{"$f":"IF((S1028-V1028)<0,0,AJ1008)","v":150},null,"*(",{"$f":"+D1027","v":5},null,"-",{"$f":"+AF1018","v":3.5},null,")-",{"$f":"IF((AB1028-AE1028)<0,0,AR1010)","v":55},null,"*(",{"$f":"+S1028","v":5},null,"-",{"$f":"+AF1018","v":3.5},null,")²"," /",2,"=",{"$f":"+E1028+I1028*M1028-P1028*(S1028-V1028)-Y1028*(AB1028-AE1028)^2/AI1028","v":308.6341094970702},null,null,"KNm"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"MB =",null,null,{"$f":"+F1032","v":-465.10070800781239},null,null,"+",{"$f":"+J1032","v":212.12196350097653},null,null,"*",{"$f":"+E1033","v":4},null,"-",{"$f":"IF((T1034-W1034)<0,0,AJ1008)","v":150},null,"*(",{"$f":"+E1033","v":4},null,"-",{"$f":"+W1032","v":3.5},null,")-",{"$f":"IF((AC1034-AF1034)<0,0,AR1010)","v":55},null,"*(",{"$f":"+T1034","v":4},null,"-",{"$f":"+AF1032","v":3.5},null,")²"," /",2,"=",{"$f":"+F1034+J1034*N1034-Q1034*(T1034-W1034)-Z1034*(AC1034-AF1034)^2/AJ1034","v":301.51214599609375},null,null,"KNm"]
[null,null,"3 * L / 4 =",null,null,{"$f":"+AN1020*3/4","v":6},null,null,"m. ' deki moment miktarı"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AL1032)","v":465.10070800781239},null,null," /(",2.5,null,"*",{"$f":"+H1040","v":465.10070800781239},null,null,"+",3,"*",{"$f":"ABS(AL1036)","v":40.856781005859318},null,null,"+",4,"*",{"$f":"ABS(AL1034)","v":301.51214599609375},null,null,"+",3,"*",{"$f":"ABS(AL1038)","v":260.75607299804676},null,null,")=",{"$f":"E1040*H1040/(L1040*O1040+S1040*U1040+Y1040*AA1040+AE1040*AG1040)","v":1.7759316159320446}]
[null,null,"v =",null,"Ma  *",null,"x²"," /",2,"+","A","*","x3"," /",6,"-",{"$f":"+O1043","v":150},null,"*(","x","-",{"$f":"+T1043","v":3.5},null,")3"," /",6,"-",{"$f":"+Z1043","v":55},null,"*(","x","-",{"$f":"+AE1043","v":3.5},null,")4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"x = 0 ; v = 0",null,null,null,null,null,"C2 = 0"]
[null,null,null,null,null,null,null,null,"Ma  *",null,{"$f":"K1048^2/N1048","v":32},null,"+","A","*",{"$f":"+R1048^3/U1048","v":85.333333333333329},null,"-",{"$f":"W1048*(Z1048-AC1048)^3/AG1048+AI1048*(AL1048-AO1048)^4/AS1048","v":3217.8515625},null,null,"=",0,null,"(1. denklem)"]
[null,null,"Ma =",null,{"$f":"+N1053","v":-465.10070800781239},null,null,null,{"$f":"+K1049","v":32},{"$f":"+P1049","v":85.333333333333329},{"$f":"S1049","v":3217.8515625},{"$f":"MINVERSE(I1053:J1054)","v":4.6875E-2},-0.49999999999999989,{"$f":"MMULT(L1053:M1054,K1053:K1054)","v":-465.10070800781239}]
[null,null,"düşey denge denkleminden"]
[null,null,"B","+","A","-",{"$f":"+AJ1008","v":150},null,"-",{"$f":"+AR1010","v":55},null,"*",{"$f":"+AR1018","v":4.5},null,"=",0]
[null,null,"x=",4,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D1059<=AN1020,\"\",\"azalt.\")","v":""}]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"AN1020*1000","v":8000},null,null," /",300,null,"=",{"$f":"+H1062/L1062","v":26.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(1.ci bölge)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK1098","v":2.4717597126999631}]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O1068,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AB1077","v":80.141601562500028},{"$f":"+BL1074-AG1069*AG1078","v":35.141601562500028},{"$f":"+BM1074-AR1070*AS1078","v":-114.85839843749997}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O1068,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+H1149","v":80.141601562500028},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+R1150","v":114.85839843750003},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,"m",null,null,null,null,null,null,null,null,null,{"$f":"+AN1080-AG1078","v":5},null,"m"]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O1068,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",8,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( x = L ; v1' ) = ( z = 0 ; v2')"]
[null,null,"x=",{"$f":"+BK1089","v":8},null,null,"m. ' deki max moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AB1077/AG1069","v":5.3427734375000018},null,{"$f":"ABS(W1072+AB1077*BE1089-AG1069*BE1089*BE1089/2)","v":92.585303783416833},null,{"$f":"MAX(BG1089,BG1090,BG1091,BG1092)","v":147.87109375000006},null,{"$f":"INDEX(BE1089:BE1092,MATCH(BI1089,BG1089:BG1092,0),0)","v":8}]
[null,null,"MB =",null,null,{"$f":"+F1090","v":-121.50390625000003},null,null,"+",{"$f":"+J1090","v":80.141601562500028},null,null,"*",{"$f":"+E1091","v":4},null,"-",{"$f":"IF(T1092>AG1078,0,AG1069)","v":0},null,"*",{"$f":"+E1091","v":4},null,"² /",2,"-",{"$f":"IF(AE1092<AG1078,0,AG1069)","v":15},null,"*",{"$f":"+AG1078","v":3},null,"*(",{"$f":"+E1091","v":4},null,"-",{"$f":"+AG1078/2","v":1.5},null,")-",{"$f":"IF(E1091<AG1078,0,AR1070)","v":30},null,"*(",{"$f":"+E1091","v":4},null,"-",{"$f":"+AG1078","v":3},null,")²"," /",2,"=",{"$f":"+F1092+J1092*N1092-Q1092*T1092^2/W1092-Y1092*AB1092*(AE1092-AH1092)-AK1092*(AN1092-AQ1092)^2/AU1092","v":71.562500000000085},null,null,"KNm",null,null,null,null,{"$f":"+AN1080","v":8},null,{"$f":"ABS(BD1072)","v":147.87109375000006}]
[null,null,"MA =",null,null,{"$f":"+F1092","v":-121.50390625000003},null,null,"+",{"$f":"+J1092","v":80.141601562500028},null,null,"*",{"$f":"+E1093","v":2},null,"-",{"$f":"IF(T1094>AG1078,0,AG1069)","v":15},null,"*",{"$f":"+E1093","v":2},null,"² /",2,"-",{"$f":"IF(AE1094<AG1078,0,AG1069)","v":0},null,"*",{"$f":"+AG1078","v":3},null,"*(",{"$f":"+E1093","v":2},null,"-",{"$f":"+AG1078/2","v":1.5},null,")-",{"$f":"IF(E1093<AG1078,0,AR1070)","v":0},null,"*(",{"$f":"+E1093","v":2},null,"-",{"$f":"+AG1078","v":3},null,")²"," /",2,"=",{"$f":"+F1094+J1094*N1094-Q1094*T1094^2/W1094-Y1094*AB1094*(AE1094-AH1094)-AK1094*(AN1094-AQ1094)^2/AU1094","v":8.7792968750000284},null,null,"KNm"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AW1090)","v":147.87109374999977},null,null," /(",2.5,null,"*",{"$f":"+H1098","v":147.87109374999977},null,null,"+",3,"*",{"$f":"ABS(AW1094)","v":8.7792968750000284},null,null,"+",4,"*",{"$f":"ABS(AW1092)","v":71.562500000000085},null,null,"+",3,"*",{"$f":"ABS(AW1096)","v":21.845703125000114},null,null,")=",{"$f":"E1098*H1098/(L1098*O1098+S1098*U1098+Y1098*AA1098+AE1098*AG1098)","v":2.4717597126999631}]
[null,null,"SEHİM HESABI"]
[null,null,"v1' =",null,{"$f":"+E1102","v":15},null,"*","x3"," /",6,"+","C1","*","x²"," /",2,"+","C2","*","x","+","C3"]
[null,null,"v1 =",null,{"$f":"+E1103","v":15},null,"*","x4"," /",24,null,"+","C1","*","x3"," /",6,"+","C2","*","x²"," /",2,"+","C3","*","x","+","C4"]
[null,null,"v2' =",null,{"$f":"+E1107","v":30},null,"*","z3"," /",6,"+","D1","*","z²"," /",2,"+","D2","*","z","+","D3"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"z = 0 ; v2'' =",null,null,null,"D2"]
[null,null,"z = L ; v2' = 0",null,null,null,null,null,{"$f":"+E1108","v":30},null,"*",{"$f":"+AS1078","v":5},null,"3 /",6,"+","D1","*",{"$f":"+L1117","v":5},null,"² /",2,"+","D2","*",{"$f":"+S1117","v":5},null,"+","D3",null,null,"D1","*",{"$f":"+S1117^2/V1117","v":12.5},null,"+","D2","*",{"$f":"+Z1117","v":5},null,"+","D3","+",{"$f":"+I1117*L1117^3/O1117","v":625},null,null,"=",0,null,"(3.ci denklem)"]
[null,null,"z = 0 ; v2 =",null,null,null,"D4"]
[null,null,"( x = L ; v1 ) = ( z = 0 ; v2 ) =",null,null,null,null,null,null,null,null,"C1","*",{"$f":"+AG1118","v":4.5},null,"+","C2","*",{"$f":"+AL1118","v":4.5},null,"-","D4","+",{"$f":"+AO1118","v":50.625},null,null,"=",0,null,"(4.ci denklem)"]
[null,null,"( x = L ; v1''' ) = ( z = 0 ; v2''') =",null,null,null,null,null,null,null,null,"C1","-","D1","+",{"$f":"+R1121-R1122","v":45},null,"=",0,null,"(5.ci denklem)"]
[null,null,"( x = L ; v1' ) = ( z = 0 ; v2') =",null,null,null,null,null,null,null,null,"C1","*",{"$f":"+AD1124","v":4.5},null,"+","C2","*",{"$f":"+AI1124","v":3},null,"-","D3","+",{"$f":"AL1124","v":67.5},null,null,"=",0,null,"(6.ci denklem)"]
[null,null,"C2 =",null,{"$f":"+W1129","v":121.50390625000003},null,null,null,0,0,{"$f":"+AP1116","v":20.833333333333332},{"$f":"+AU1116","v":12.5},{"$f":"+AZ1116","v":5},1,{"$f":"-BE1116","v":-781.25},null,-7.8125000000000111E-2,9.3749999999999931E-2,-0.24999999999999994,9.375E-2,-1.171875,0.21875,121.50390625000003]
[null,null,"D3 =",null,71.37451171875,null,null,null,1,0,-1,0,0,0,{"$f":"-P1123","v":-45},null,0.556640625,0.17578124999999997,-0.32812499999999994,0.17578124999999997,-0.43945312500000011,-0.44921875000000006,71.37451171875]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E1104","v":15},null,"*","x4"," /",24,null,"+","C1","*","x3"," /",6,"+","C2","*","x²"," /",2,"+","C3","*","x","+","C4"]
[null,null,"y =",null,{"$f":"(E1137*H1137^4/K1137+N1137*R1137^3/U1137+W1137*AA1137^2/AD1137)*100000000/(AH1137*AL1137)","v":1.2855960637149759},null,null,"mm"]
[null,null,"2.ci bölgede :"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E1109","v":30},null,"*","z4"," /",24,null,"+","D1","*","z3"," /",6,"+","D2","*","z²"," /",2,"+","D3","*","z","+","D4"]
[null,null,"y = (",null,{"$f":"+H1142","v":30},null,"*",{"$f":"+D1143","v":2},null,"4 /",24,null,"+",{"$f":"+E1130","v":-35.141601562499979},null,null,"*",{"$f":"+H1144","v":2},null,"3 /",6,"+",{"$f":"+E1131","v":-51.420898437500043},null,null,"*",{"$f":"+R1144","v":2},null,"² /",2,"+",{"$f":"+E1132","v":71.37451171875},null,null,"*",{"$f":"+AA1144","v":2},null,"+",{"$f":"+E1133","v":236.75537109375006},null,null,")* 108 / (",null,null,{"$f":"+AH1137","v":200000},null,null,"*",{"$f":"+AL1137","v":92080},null,null,")"]
[null,null,"MESNET TEPKİLERİ"]
[null,null,"(x = 0 ; v1'') =",null,null,null,null,{"$f":"+E1129","v":121.50390625000003},null,null,"KNm",null,"(Ma mesnet tepkisi)"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"2.ci bölgede  z =",null,null,null,null,3,null,"m. 'de ki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(H1157<=AS1078,\"\",\"azalt.\")","v":""}]
[null,null,"Mx = ",null,{"$f":"+E1107","v":30},null,"*",{"$f":"+H1157","v":3},null,"² /",2,"+",{"$f":"+E1130","v":-35.141601562499979},null,null,"*",{"$f":"+H1158","v":3},null,"+",{"$f":"+E1131","v":-51.420898437500043},null,null,"=",{"$f":"E1158*H1158^2/K1158+M1158*Q1158+T1158","v":-21.845703124999986},null,null,"KNm"]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK TEK AÇIKLIKLI ANKASTRE KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK1195","v":1.8870219506675727}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(BL1170),ABS(BM1170),ABS(BN1170))","v":107.86743164062494},null,null,"KN",null,"(max kesme kuvveti)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,"m",null,null,null,null,null,null,null,null,null,{"$f":"+AN1176-AG1174","v":5},null,"m"]
[null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O1164,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,"(kiriş atalet momenti)",null,null,null,null,null,null,null,null,null,null,null,null,null,"x = 0 ; v1' = 0",null,null,null,null,null,null,null,null,null,null,"Uygunluk koşulları",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = 0 ; v1 = 0",null,null,null,null,null,null,null,null,null,"( x = L ; v1 ) = ( z = 0 ; v2 )",null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v2 = 0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( x = L ; v1' ) = ( z = 0 ; v2')"]
[]
[null,null,"Mmax =",null,null,{"$f":"+W1168","v":-195.43945312499989},null,null,"+",{"$f":"+AB1173","v":107.86743164062494},null,null,"*",{"$f":"+D1186","v":0},null,"-",{"$f":"IF(T1187>AG1174,0,AG1165)","v":15},null,"*",{"$f":"+D1186","v":0},null,"² /",2,"-",{"$f":"IF(AE1187<AG1174,0,AG1165)","v":0},null,"*",{"$f":"+AG1174","v":3},null,"*(",{"$f":"+D1186","v":0},null,"-",{"$f":"+AG1174/2","v":1.5},null,")-",{"$f":"IF(D1186<AG1174,0,AR1166)","v":0},null,"*(",{"$f":"+D1186","v":0},null,"-",{"$f":"+AG1174","v":3},null,")²"," /",2,"=",{"$f":"+F1187+J1187*N1187-Q1187*T1187^2/W1187-Y1187*AB1187*(AE1187-AH1187)-AK1187*(AN1187-AQ1187)^2/AU1187","v":-195.43945312499989},null,null,"KNm",null,null,null,null,{"$f":"(AB1173-AG1165*AG1174+AR1166*AG1174)/AR1166","v":5.0955810546874982},null,{"$f":"ABS(W1168+AB1173*BE1187-AG1165*AG1174*(BE1187-AG1174/2)-AR1166*(BE1187-AG1174)^2/2)","v":126.53474114835248}]
[null,null,"L / 4 =",null,{"$f":"+AN1176/4","v":2},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,null,{"$f":"+F1191","v":-195.43945312499989},null,null,"+",{"$f":"+J1191","v":107.86743164062494},null,null,"*",{"$f":"+F1192","v":6},null,"-",{"$f":"IF(T1193>AG1174,0,AG1165)","v":0},null,"*",{"$f":"+F1192","v":6},null,"² /",2,"-",{"$f":"IF(AE1193<AG1174,0,AG1165)","v":15},null,"*",{"$f":"+AG1174","v":3},null,"*(",{"$f":"+F1192","v":6},null,"-",{"$f":"+AG1174/2","v":1.5},null,")-",{"$f":"IF(F1192<AG1174,0,AR1166)","v":30},null,"*(",{"$f":"+F1192","v":6},null,"-",{"$f":"+AG1174","v":3},null,")²"," /",2,"=",{"$f":"+F1193+J1193*N1193-Q1193*T1193^2/W1193-Y1193*AB1193*(AE1193-AH1193)-AK1193*(AN1193-AQ1193)^2/AU1193","v":114.26513671874977},null,null,"KNm"]
[null,null,"SEHİM HESABI"]
[null,null,"v1'' =",null,{"$f":"+E1198","v":15},null,"*","x²"," /",2,"+","C1","*","x","+","C2"]
[null,null,"2.ci bölgede :"]
[null,null,"v2''' =",null,{"$f":"+AR1166","v":30},null,"*","z","+","D1"]
[null,null,"v2 =",null,{"$f":"+E1205","v":30},null,"*","z4"," /",24,null,"+","D1","*","z3"," /",6,"+","D2","*","z²"," /",2,"+","D3","*","z","+","D4"]
[null,null,"x = 0 ; v1 = 0",null,null,null,null,null,"C4 = 0"]
[null,null,"( x = L ; v1'' ) = ( z = 0 ; v2'' ) =",null,null,null,null,null,null,null,null,"C1","*",{"$f":"+Q1210","v":3},null,"+","C2","-","D2","+",{"$f":"+G1210*J1210^2/M1210","v":67.5},null,null,"=",0,null,"(1.ci denklem)"]
[null,null,"x = L ; v1 =",null,null,null,{"$f":"+E1201","v":15},null,"*",{"$f":"+AG1174","v":3},null,"4 /",24,null,"+","C1","*",{"$f":"+J1215","v":3},null,"3 /",6,"+","C2","*",{"$f":"+R1215","v":3},null,"² /",2,null,null,"C1","*",{"$f":"+R1215^3/U1215","v":4.5},null,"+","C2","*",{"$f":"+Y1215^2/AB1215","v":4.5},null,"+",{"$f":"+G1215*J1215^4/M1215","v":50.625}]
[null,null,"( x = L ; v1 ) = ( z = 0 ; v2 ) =",null,null,null,null,null,null,null,null,"C1","*",{"$f":"+AG1215","v":4.5},null,"+","C2","*",{"$f":"+AL1215","v":4.5},null,"-","D4","+",{"$f":"+AO1215","v":50.625},null,null,"=",0,null,"(4.ci denklem)"]
[null,null,"x = L ; v1' =",null,null,null,{"$f":"+E1200","v":15},null,"*",{"$f":"+AG1174","v":3},null,"3 /",6,"+","C1","*",{"$f":"+J1221","v":3},null,"² /",2,"+","C2","*",{"$f":"+Q1221","v":3},null,null,null,"C1","*",{"$f":"+Q1221^2/T1221","v":4.5},null,"+","C2","*",{"$f":"+X1221","v":3},null,"+",{"$f":"+G1221*J1221^3/M1221","v":67.5}]
[null,null,"z = 0 ; v2' =",null,null,null,"D3"]
[null,null,"altı adet denklem altı adet bilinmeyen çözülürse :"]
[null,null,"D1 =",null,-62.867431640625,null,null,null,0,0,{"$f":"+AA1214","v":5},1,0,0,{"$f":"-AF1214","v":-375},null,0.11425781249999992,-5.8593749999999948E-3,0.1875,-5.8593749999999844E-3,-0.18457031249999994,-2.9296875E-2,-62.867431640625]
[null,null,"1.ci bölgede :"]
[null,null,"x=",3,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D1233<=AG1174,\"\",\"azalt.\")","v":""}]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"AN1176*1000","v":8000},null,null," /",300,null,"=",{"$f":"+H1236/L1236","v":26.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"2.ci bölgede :"]
[null,null,"y =",null,{"$f":"(E1241*H1241^4/K1241+N1241*R1241^3/U1241+W1241*AA1241^2/AD1241+AF1241*AJ1241+AM1241)*100000000/(AS1241*AW1241)","v":3.2383796963662705},null,null,"mm"]
[null,null,"MESNET TEPKİLERİ"]
[null,null,"(z = L ; v2''') =",null,null,null,null,{"$f":"+E1203","v":30},null,"*",{"$f":"+AS1174","v":5},null,"+",{"$f":"+E1227","v":-62.867431640625},null,null,"=",{"$f":"+H1247*K1247+N1247","v":87.132568359375},null,null,"KN",null,"(B mesnet tepkisi)"]
[null,null,"(x = 0 ; v1'') =",null,null,null,null,{"$f":"+E1226","v":195.43945312499989},null,null,"KNm",null,"(Ma mesnet tepkisi)"]
[null,null,"M = ",null,{"$f":"+E1199","v":15},null,"*",{"$f":"+H1250","v":3},null,"² /",2,"+",{"$f":"+E1225","v":-107.86743164062494},null,null,"*",{"$f":"+H1251","v":3},null,"+",{"$f":"+E1226","v":195.43945312499989},null,null,"=",{"$f":"E1251*H1251^2/K1251+M1251*Q1251+T1251","v":-60.662841796874943},null,null,"KNm"]
[null,null,"Mx = ",null,{"$f":"+E1204","v":30},null,"*",{"$f":"+H1253","v":3},null,"² /",2,"+",{"$f":"+E1227","v":-62.867431640625},null,null,"*",{"$f":"+H1254","v":3},null,"+",{"$f":"+E1228","v":-60.662841796874972},null,null,"=",{"$f":"E1254*H1254^2/K1254+M1254*Q1254+T1254","v":-114.26513671874997},null,null,"KNm"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"+R1297","v":18.75},null,null,"KNm",null,"(max moment)"]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O1260,$CG$6:$CG$120,0),0)","v":12}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E1279","v":18.75},null,"KN",null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E1281","v":18.75},null,"KN",null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O1260,$CG$6:$CG$120,0),0)","v":220}]
[]
[null,null,"A","=",{"$f":"H1278*K1278/N1278*P1278/E1278","v":18.75},null,null,"KN"]
[null,null,"SEHİM HESABI"]
[null,null,"v =",null,{"$f":"+E1284","v":18.75},null,"*","x3"," /",6,"-",{"$f":"+L1284","v":2.7777777777777777},null,"*","x5"," /",20,null,"+","C1","*","x","+","C2"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"( x = L / 2 ) v'  = 0",null,null,null,null,null,null,{"$f":"+E1284","v":18.75},null,"*",{"$f":"+AD1271/2","v":1.5},null,"² /",2,"-",{"$f":"+L1284","v":2.7777777777777777},null,"*",{"$f":"+M1288","v":1.5},null,"4/",4,"+","C1","=",0,null,null,"C1","=",{"$f":"-(J1288*M1288^2/P1288-R1288*U1288^4/X1288)","v":-17.578125}]
[null,null,"y = (",null,{"$f":"+H1289","v":18.75},null,"*",{"$f":"+D1290","v":1.5},null,"3/",6,"-",{"$f":"+O1289","v":2.7777777777777777},null,"*",{"$f":"+H1291","v":1.5},null,"5/",20,null,"+",{"$f":"+AG1288","v":-17.578125},null,null,"*",{"$f":"+P1291","v":1.5},null,")* 108 / (",null,null,{"$f":"+F1275","v":200000},null,null,"*",{"$f":"+F1274","v":92080},null,null,")"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"Mmax =",null,null,{"$f":"+E1283","v":18.75},null,"*",{"$f":"+D1296","v":1.5},null,"-",{"$f":"+Y1283","v":2.7777777777777777},null,"*",{"$f":"+D1296","v":1.5},null,"3 =",{"$f":"+F1297*I1297-L1297*O1297^3","v":18.75},null,null,"KNm"]
[null,null,"L / 4 =",null,{"$f":"+AD1271/4","v":0.75},null,null,"m. ' deki moment miktarı"]
[null,null,"3 * L / 4 =",null,null,{"$f":"+AD1271*3/4","v":2.25},null,null,"m. ' deki moment miktarı"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"Vx = ",null,{"$f":"+W1270","v":18.75},null,"-",{"$f":"+AD1262","v":25},null,"*",{"$f":"+D1307","v":0.8},null,"² /",{"$f":"+AD1271","v":3},null,"=",{"$f":"+E1309-H1309*K1309^2/N1309","v":13.416666666666664},null,null,"KN"]
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK TEK AÇIKLIKLI BASİT KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK1351","v":1.2262861049393265}]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O1315,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AB1324","v":115.3125},{"$f":"+BK1321-AH1315","v":-34.6875},{"$f":"+BL1321-AR1317*AS1325","v":-199.6875}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.5,null,"m",null,null,null,1.5,null,"m",null,null,null,null,null,{"$f":"+AN1327-AE1325-AK1325","v":3},null,"m",null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(O1315,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",8,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[]
[null,null,"A =",null,{"$f":"(H1333*K1333+N1333*Q1333*T1333)/E1333","v":115.3125},null,null,"KN"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"Vx =",null,{"$f":"+E1339","v":115.3125},null,null,"-",{"$f":"+L1339","v":150},null,"-",{"$f":"+U1339","v":55},null,"*(",{"$f":"+D1338","v":6},null,"-",{"$f":"+AE1325+AK1325","v":5},null,")=",{"$f":"+E1340-I1340-L1340*(O1340-R1340)","v":-89.6875},null,null,"KNm"]
[null,null,"Mmax =",null,null,{"$f":"+AB1324","v":115.3125},null,null,"*",{"$f":"+D1342","v":3.5},null,"-",{"$f":"IF((P1343-S1343)<0,0,AH1315)","v":150},null,"*(",{"$f":"+D1342","v":3.5},null,"-",{"$f":"+AE1325","v":3.5},null,")-",{"$f":"IF((Y1343-AB1343)<0,0,AR1317)","v":0},null,"*(",{"$f":"+P1343","v":3.5},null,"-",{"$f":"+AE1325+AK1325","v":5},null,")²"," /",2,"=",{"$f":"F1343*J1343-M1343*(P1343-S1343)-V1343*(Y1343-AB1343)^2/AF1343","v":403.59375},null,null,"KNm",null,null,null,null,null,null,null,null,null,{"$f":"+AE1325+AK1325","v":5},null,{"$f":"AB1324*AU1343-AH1315*AK1325","v":351.5625}]
[null,null,"L / 4 =",null,{"$f":"+AN1327/4","v":2},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,{"$f":"+E1347","v":115.3125},null,null,"*",{"$f":"+F1348","v":6},null,"-",{"$f":"IF((O1349-R1349)<0,0,AH1315)","v":150},null,"*(",{"$f":"+F1348","v":6},null,"-",{"$f":"+R1347","v":3.5},null,")-",{"$f":"IF((X1349-AA1349)<0,0,AR1317)","v":55},null,"*(",{"$f":"+O1349","v":6},null,"-",{"$f":"+AA1347","v":5},null,")²"," /",2,"=",{"$f":"E1349*I1349-L1349*(O1349-R1349)-U1349*(X1349-AA1349)^2/AE1349","v":289.375},null,null,"KNm"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,"SEHİM HESABI"]
[null,null,"v =",null,{"$f":"+E1354","v":115.3125},null,null,"*","x3"," /",6,"-",{"$f":"+M1354","v":150},null,"*(","x","-",{"$f":"+R1354","v":3.5},null,")3"," /",6,"-",{"$f":"+X1354","v":55},null,"*(","x","-",{"$f":"+AC1354","v":5},null,")4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E1355","v":115.3125},null,null,"*","x3"," /",6,"-",{"$f":"+M1355","v":150},null,"*(","x","-",{"$f":"+R1355","v":3.5},null,")3"," /",6,"-",{"$f":"+X1355","v":55},null,"*(","x","-",{"$f":"+AC1355","v":5},null,")4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"x=",4,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D1361<=AN1327,\"\",\"azalt.\")","v":""}]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"AN1327*1000","v":8000},null,null," /",300,null,"=",{"$f":"+H1364/L1364","v":26.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(1.ci bölge)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,null,"KN",null,null,null,null,null,null,null,null,"(2.ci bölge)",null,null,null,95,null,"KN"]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O1371,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ma =",null,{"$f":"+E1415","v":-728.525390625},null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(BG1376),ABS(BH1376),ABS(BI1376),ABS(BJ1376),ABS(BK1376),ABS(BL1376),ABS(BM1376))","v":449.893798828125},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AB1380","v":449.893798828125},{"$f":"+BG1376-AE1372*AF1381","v":187.393798828125},{"$f":"+BH1376-AJ1371","v":37.393798828125},{"$f":"+BI1376-AE1372*AN1381","v":-300.106201171875},{"$f":"+BJ1376+AS1380","v":177.5},{"$f":"+BK1376-AV1373*AV1381","v":95},{"$f":"+BL1376-AY1371","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O1371,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E1413","v":449.893798828125},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E1414","v":477.606201171875},null,"KN"]
[]
[null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,"A","+","B","-",{"$f":"+AJ1371","v":150},null,"-",{"$f":"+AY1371","v":95},null,"-",{"$f":"+AE1372","v":75},null,"*",{"$f":"+AJ1383","v":8},null,"-",{"$f":"+AV1373","v":55},null,"*",{"$f":"+AV1381","v":1.5},null,"=",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v2 = 0"]
[null,null,"Ma +",null,"A","*",{"$f":"+AJ1383","v":8},null,"-",{"$f":"+AJ1371","v":150},null,"*",{"$f":"+AN1381","v":4.5},null,"-",{"$f":"+AE1372","v":75},null,"*",{"$f":"+AJ1383","v":8},null,"*",{"$f":"+S1391/2","v":4},null,"+",{"$f":"+AV1373","v":55},null,"*",{"$f":"+AV1381","v":1.5},null,"*",{"$f":"+AB1391/2","v":0.75},null,"+",{"$f":"+AY1371","v":95},null,"*",{"$f":"+AV1381","v":1.5},null,"=",0]
[null,null,"Ma +",null,"A","*",{"$f":"+G1391","v":8},null,"+",{"$f":"-J1391*M1391-P1391*S1391*V1391+Y1391*AB1391*AE1391+AH1391*AK1391","v":-2870.625},null,null,"=",0,null,"(2.ci denklem)",null,null,null,null,"(kayıcı mesnette moment sıfır şartından)"]
[null,null,"v1' =",null,"Ma *",null,"x","+","A","*","x²"," /",2,"-",{"$f":"+K1394","v":75},null,"*","x3"," /",6,"-",{"$f":"+R1394","v":150},null,"*(","x","-",{"$f":"+W1394","v":3.5},null,")²"," /",2,"+","C1"]
[null,null,"v2'' =",null,"Ma +",null,"A","*","x","-",{"$f":"+AE1372","v":75},null,"*",{"$f":"+AJ1383","v":8},null,"*(","x","-",{"$f":"+AJ1383/2","v":4},null,")-",{"$f":"+AJ1371","v":150},null,"*(","x","-",{"$f":"+AF1381","v":3.5},null,")+","B","*(","x","-",{"$f":"+AJ1383","v":8},null,")-",{"$f":"+AV1373","v":55},null,"*(","x","-",{"$f":"+AJ1383","v":8},null,")²"," /",2]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"x = L ; v1 = 0",null,null,null,null,null,"Ma *",null,{"$f":"+AJ1383","v":8},null,"² /",2,"+","A","*",{"$f":"+K1404","v":8},null,"3 /",6,"-",{"$f":"+Q1396","v":75},null,"*",{"$f":"+R1404","v":8},null,"4 /",24,null,"-",{"$f":"+Y1396","v":150},null,"*(",{"$f":"+Z1404","v":8},null,"-",{"$f":"+AD1396","v":3.5},null,")3"," /",6,"=",0]
[null,null,null,null,null,null,null,null,"Ma *",null,{"$f":"+K1406^2/N1406","v":32},null,"+","A","*",{"$f":"+R1406^3/U1406","v":85.333333333333329},null,"+","D2","+",{"$f":"-W1406*(Z1406-AC1406)^3/AG1406-AI1406*(AL1406-AO1406)^3/AS1406-BF1406*(BI1406-BL1406)^4/BP1406+BS1406*BW1406","v":-21478.125},null,null,"=",0,null,"(4.cü denklem)"]
[null,null,null,null,null,null,null,"Ma *",null,{"$f":"+J1409","v":8},null,"+","A","*",{"$f":"+O1409^2/R1409","v":32},null,"+","D1","-",{"$f":"T1409*(W1409-Z1409)^2/AD1409+AF1409*(AI1409-AL1409)^2/AP1409+BC1409*(BF1409-BI1409)^3/BM1409","v":6318.75}]
[null,null,"A =",null,{"$f":"+S1413","v":449.893798828125},null,null,null,1,1,0,0,{"$f":"G1390","v":927.5},null,{"$f":"MINVERSE(I1413:L1416)","v":0},0.1875,-5.859375E-3,0,{"$f":"MMULT(O1413:R1416,M1413:M1416)","v":449.893798828125}]
[null,null,"B =",null,{"$f":"+S1414","v":477.606201171875},null,null,null,{"$f":"+G1392","v":8},0,1,0,{"$f":"-J1392","v":2870.625},null,1,-0.1875,5.859375E-3,0,477.606201171875]
[null,null,"D2 =",null,6400,null,null,null,{"$f":"+P1407","v":85.333333333333329},0,{"$f":"+K1407","v":32},1,{"$f":"-U1407","v":21478.125},null,0,0,-1,1,6400]
[null,null,"y = (",null,"Ma *",null,"x²"," /",2,"+","A","*","x3"," /",6,"-",{"$f":"+T1418","v":75},null,"*","x4"," /",24,null,"-",{"$f":"+AB1418","v":150},null,"*(","x","-",{"$f":"+AG1418","v":3.5},null,")3"," /",6,") * 108 / ( E * I )"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"AJ1383*1000","v":8000},null,null," /",300,null,"=",{"$f":"+H1423/L1423","v":26.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"2.ci bölgede :"]
[null,null,"y = (",null,{"$f":"+E1415","v":-728.525390625},null,null,"*",{"$f":"+D1428","v":9.5},null,"² /",2,"+",{"$f":"+E1413","v":449.893798828125},null,null,"*",{"$f":"+I1429","v":9.5},null,"3 /",6,"-",{"$f":"+Q1427","v":600},null,"*(",{"$f":"+D1428","v":9.5},null,"-",{"$f":"+V1427","v":4},null,")3"," /",6,"-",{"$f":"+AB1427","v":150},null,"*(",{"$f":"+Z1429","v":9.5},null,"-",{"$f":"+AG1427","v":3.5},null,")3"," /",6,"+",{"$f":"+E1414","v":477.606201171875},null,null,"*(",{"$f":"+AL1429","v":9.5},null,"-",{"$f":"+AQ1427","v":8},null,")3"," /",6,"-",{"$f":"+AW1427","v":55},null,"*(",{"$f":"+AY1429","v":9.5},null,"-",{"$f":"+BB1427","v":8},null,")4"," /",24,null,"+",{"$f":"+BI1427","v":-1600},null,null,"*",{"$f":"+BK1429","v":9.5},null,"+"]
[null,null,null,"+",{"$f":"+BO1427","v":6400},null,null,")* 108 / (",null,null,{"$f":"+AT1421","v":200000},null,null,"*",{"$f":"+AX1421","v":92080},null,null,")"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"1.ci bölgede :"]
[null,null,"2.ci bölgede :"]
[null,null,"Mx =",null,{"$f":"+E1415","v":-728.525390625},null,null,"+",{"$f":"+E1413","v":449.893798828125},null,null,"*",{"$f":"+D1440","v":9},null,"-",{"$f":"+K1398*N1398","v":600},null,"*(",{"$f":"+D1440","v":9},null,"-",{"$f":"+S1398","v":4},null,")-",{"$f":"IF((AB1441-AE1441)<0,0,V1398)","v":150},null,"*(",{"$f":"+S1441","v":9},null,"-",{"$f":"+AA1398","v":3.5},null,")+",{"$f":"+E1414","v":477.606201171875},null,null,"*(",{"$f":"+AB1441","v":9},null,"-",{"$f":"+AH1398","v":8},null,")-",{"$f":"+AK1398","v":55},null,"*(",{"$f":"+AL1441","v":9},null,"-",{"$f":"+AP1398","v":8},null,")²"," /",2,"=",{"$f":"E1441+I1441*M1441-P1441*(S1441-V1441)-Y1441*(AB1441-AE1441)+AH1441*(AL1441-AO1441)-AR1441*(AU1441-AX1441)^2/BB1441","v":-54.375},null,null,"KNm"]
[null,null,"1.ci bölgede :"]
[null,null,"Mmax =",null,null,{"$f":"+E1437","v":-728.525390625},null,null,"+",{"$f":"+I1437","v":449.893798828125},null,null,"*",{"$f":"+D1445","v":0},null,"-",{"$f":"+P1437","v":75},null,"*",{"$f":"+D1445","v":0},null,"² /",2,"-",{"$f":"IF((AB1446-AE1446)<0,0,R1394)","v":0},null,"*(",{"$f":"+T1446","v":0},null,"-",{"$f":"+AD1437","v":3.5},null,")=",{"$f":"F1446+J1446*N1446-Q1446*T1446^2/W1446-Y1446*(AB1446-AE1446)","v":-728.525390625},null,null,"KNm",null,null,null,0,null,{"$f":"ABS(+W1375)","v":728.525390625},null,{"$f":"MAX(AQ1446,AQ1447,AQ1448,AQ1449)","v":728.525390625},null,{"$f":"INDEX(AO1446:AO1449,MATCH(AS1446,AQ1446:AQ1449,0),0)","v":0}]
[null,null,"MA =",null,{"$f":"+E1448","v":-728.525390625},null,null,"+",{"$f":"+I1448","v":449.893798828125},null,null,"*",{"$f":"+E1449","v":2},null,"-",{"$f":"+P1448","v":75},null,"*",{"$f":"+E1449","v":2},null,"² /",2,"-",{"$f":"IF((AA1450-AD1450)<0,0,R1394)","v":0},null,"*(",{"$f":"+S1450","v":2},null,"-",{"$f":"+AD1448","v":3.5},null,")=",{"$f":"E1450+I1450*M1450-P1450*S1450^2/V1450-X1450*(AA1450-AD1450)","v":21.26220703125},null,null,"KNm"]
[null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"w =",null,75,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AH1463","v":500},null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-U1476","v":309.375},null,null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A =",null,{"$f":"+F1461","v":150},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,null,"A","-",{"$f":"+M1462","v":75},null,"*",{"$f":"+N1469","v":1.5},null,"-",{"$f":"+F1461","v":150},null,"=",0]
[null,null,null,"ARA KESİT TESİRLERİ"]
[null,null,null,"M = - P * x - w * x ² / 2 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca konsol kirişte Cb = 1 alınır."]
[null,null,null,"Mx =",null,{"$f":"-F1461","v":-150},null,"*",{"$f":"+E1479","v":1},null,"-",{"$f":"+M1462","v":75},null,"*",{"$f":"+E1479","v":1},null,"² /",2,"=",{"$f":"+F1480*I1480-L1480*O1480^2/R1480","v":-187.5},null,null,"KNm"]
[null,null,null,"Io = b * h3 / 12 "]
[null,null,null,"( E * Io * x / L ) * v'' = - w * x² / 2 - P * x"]
[null,null,null,"E * Io * v' = - w * L * x² / 4 - P * L * x + C1 =",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-M1462","v":-75},null,"*",{"$f":"+N1469","v":1.5},null,"*","x²"," /",4,"-",{"$f":"+F1461","v":150},null,"*",{"$f":"+N1469","v":1.5},null,"*","x","+","C1","=",{"$f":"+Q1489*T1489/Y1489","v":-28.125},null,"*","x²","-",{"$f":"+AA1489*AD1489","v":225},null,null,"*","x","+","C1"]
[null,null,null,"x = L ; v = 0",null,null,null,null,null,{"$f":"+AV1490","v":-9.375},null,"*",{"$f":"+N1469","v":1.5},null,"3-",{"$f":"+BA1490","v":112.5},null,"*",{"$f":"+M1493","v":1.5},null,"²+",{"$f":"+AD1492","v":400.78125},null,null,"*",{"$f":"+S1493","v":1.5},null,"+","C2","=",0,null,null,"C2","=",{"$f":"-(J1493*M1493^3-P1493*S1493^2+V1493*Z1493)","v":-316.40625}]
[null,null,null,"E * Io / 108 * y =",null,null,null,null,{"$f":"+AV1490","v":-9.375},null,"*","x3","-",{"$f":"+BA1490","v":112.5},null,"*","x²","+","C1","*","x","+","C2"]
[null,null,null,"x=",0,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,null,{"$f":"IF(E1496<=N1469,\"\",\"azalt.\")","v":""},null,null,null,"(konsol ucu sehim için  x = 0  giriniz.)"]
[null,null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"N1469*1000","v":1500},null,null," /",150,null,"=",{"$f":"+I1499/M1499","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,"TEKİL YÜKLÜ ÇELİK KONSOL KİRİŞ SEHİM HESABI (değişken kesit)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,null,"KN",null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kiriş ucu enkesiti",null,null,null,null,null,null,null,"kiriş mesnet enkesiti"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BD1508<BL1509,\"\",\"artır.\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Io =",null,{"$f":"BA1512*BD1508^3/12","v":450000000},null,null,null,null,"mm4",null,null,{"$f":"+BA1512","v":200},null,"mm"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(moment diyagramı)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT1509","v":225},null,"KNm",null,null,null,null,null,null,null,"konsol kiriş 3 boyut çizimi"]
[null,null,null,"SEHİM HESABI"]
[null,null,null,"Ix =",null,{"$f":"+BA1512/1000","v":0.2},null,"*(",{"$f":"+G1525","v":0.3},null,"*(",1,"+",{"$f":"+L1525","v":0.66666666666666663},null,"*","x"," /",{"$f":"+Q1525","v":1.5},null,") )3  /",null,12,null,null,null,null,null,null,null,null,"(kesme kuvveti diyagramı)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+BL1509","v":500},null,"mm"]
[null,null,null,"E * Ix = E * Io * (",null,null,null,null,1,"+",{"$f":"+N1526","v":0.66666666666666663},null,"*","x"," /",{"$f":"+S1526","v":1.5},null,")3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+BA1512","v":200},null,"mm"]
[null,null,null,"1.ci integral hesabı"]
[null,null,null,{"$f":"V1532","v":-150},null,"ʃ","(","u","-",1,")/",{"$f":"+U1534","v":0.44444444444444442},null," /","u3","*",1," /",{"$f":"+AC1534","v":0.44444444444444442},null,"*","du","=",{"$f":"+D1535","v":-150},null,"ʃ","(","u","-",1,")/(",{"$f":"+L1535*S1535","v":0.19753086419753085},null,"*","u3",")*","du","=",{"$f":"+X1535","v":-150},null,"ʃ",1," /(",{"$f":"+AF1535","v":0.19753086419753085},null,null,"*","u²",")-",1," /(",{"$f":"+AR1535","v":0.19753086419753085},null,null,"*","u3",")* ","du","=",{"$f":"+AM1535","v":-150},null," /",{"$f":"+AR1535","v":0.19753086419753085},null,null,"ʃ","(",1," /","u²","-",1," /","u3",")*","du"]
[null,null,null,"2.ci integral hesabı"]
[null,null,null,{"$f":"+D1539","v":75},null," /",{"$f":"+G1539","v":0.19753086419753085},null,null,"ʃ","(",2,"*","u","+",1,")/(","u","+",1,")²","*",1," /",{"$f":"+AX1539","v":0.44444444444444442},null,"*","du","=",{"$f":"+D1540","v":75},null," /",{"$f":"+G1540*Y1540","v":8.77914951989026E-2},null,null,"ʃ","(",2,"*","u","+",1,")/(","u","+",1,")²","*","du",null,null,"v","=","u","+",1,null,null,"u","=","v","-",1,null,null,"du","=","dv"]
[null,null,null,{"$f":"+AD1540","v":75},null," /",{"$f":"+AG1540","v":8.77914951989026E-2},null,null,"ʃ","(",2,"*(","v","-",1,")+",1,")/(","v","-",1,"+",1,")²","*","dv","=",{"$f":"+D1541","v":75},null," /",{"$f":"+G1541","v":8.77914951989026E-2},null,null,"ʃ","(",2,"*","v","-",1,")/","v²","*","dv","=",{"$f":"+AC1541","v":75},null," /",{"$f":"+AF1541","v":8.77914951989026E-2},null,null,"( ʃ",2,"*","v"," /","v²","*","dv","-","ʃ",1," /","v²","*","dv",")"]
[null,null,null,"E * Io * v' =",null,null,null,{"$f":"+AD1537","v":75},null,"*(",{"$f":"+AG1537","v":0.88888888888888884},null,"*","x","+",1,")/(",{"$f":"+AN1537","v":0.19753086419753085},null,null,"*(",{"$f":"+AR1537","v":0.19753086419753085},null,null,"*","x²","+",{"$f":"+AX1537","v":0.88888888888888884},null,"*","x","+",1,") ) +",null,"C1"]
[null,null,null,"x = L ; v' = 0",null,null,null,null,null,{"$f":"+H1544","v":75},null,"*(",{"$f":"+K1544","v":0.88888888888888884},null,"*",{"$f":"+AI1516","v":1.5},null,"+",1,")/(",{"$f":"+R1544","v":0.19753086419753085},null,null,"*(",{"$f":"+V1544","v":0.19753086419753085},null,null,"*",{"$f":"+P1547","v":1.5},null,"²+",{"$f":"+AB1544","v":0.88888888888888884},null,"*",{"$f":"+AC1547","v":1.5},null,"+",1,") ) +",null,"C1","=",0,null,null,"C1","=",{"$f":"-(J1547*(M1547*P1547+S1547)/(U1547*(Y1547*AC1547^2+AF1547*AI1547+AL1547)))","v":-318.9375}]
[null,null,null,"y = (",null,{"$f":"+I1549","v":75},null," /",{"$f":"+L1549","v":4.38957475994513E-2},null,null,"*","Ln  (",null,{"$f":"+R1549","v":0.44444444444444442},null,"*","x","+",1,")+",{"$f":"+Y1549","v":75},null," /(",{"$f":"+AB1549","v":8.77914951989026E-2},null,null,"*(",{"$f":"+AF1549","v":0.44444444444444442},null,"*","x","+",1,") ) +",null,{"$f":"+AV1547","v":-318.9375},null,null,"*","x","+",{"$f":"+BE1548","v":-906.96534310642301},null,null,") * 108 / ( E * Io )"]
[null,null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"AI1516*1000","v":1500},null,null," /",150,null,"=",{"$f":"+I1554/M1554","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",null,null,null,null,null,null,null,null,"mm"]
[null,null,{"$f":"+AS1565","v":300},null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+BA1566","v":500},null,null,null,null,null,null,null,null,300]
[null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"üç boyut çizimi"]
[]
[null,null,"SEHİM HESABI",null,null,null,null,null,null,"(boy için sistemin yarısı ele alınacak)"]
[null,null,"Ix =",null,{"$f":"+AP1569/1000","v":0.2},null,"*(",{"$f":"+F1577","v":0.3},null,"*(",1,"+",{"$f":"+K1577","v":0.66666666666666663},null,"*","x"," /",{"$f":"+P1577","v":2.5},null,") )3  /",null,12]
[null,null,"Ix =",null,{"$f":"+E1578","v":0.2},null,"*",{"$f":"+H1578","v":0.3},null,"3/",12,null,"*(",1,"+",{"$f":"+M1578","v":0.66666666666666663},null,"*","x"," /",{"$f":"+R1578","v":2.5},null,")3"]
[null,null,"E * Ix = E * Io * (",null,null,null,null,1,"+",{"$f":"+M1578","v":0.66666666666666663},null,"*","x"," /",{"$f":"+R1578","v":2.5},null,")3"]
[null,null,"E * Io * v'' = A * x / (",null,null,null,null,null,1,"+",{"$f":"+H1583","v":0.26666666666666666},null,"*","x",")3","=",{"$f":"+F1570","v":75},null,"*","x"," /(",1,"+",{"$f":"+K1584","v":0.26666666666666666},null,"*","x",")3"]
[null,null,{"$f":"+BG1587","v":75},null," /",{"$f":"+BJ1587","v":7.1111111111111111E-2},null,null,"*(",1," /","u","+",1," /(",2,"*","u²",") )","=",{"$f":"+C1588","v":75},null," /",{"$f":"+F1588","v":7.1111111111111111E-2},null,null,"*(",-2,"*","u","+",1,")/(",2,"*","u²",")=",{"$f":"-U1588","v":-75},null," /",{"$f":"+X1588","v":7.1111111111111111E-2},null,null,"*(",2,"*","u","-",1,")/(",2,"*","u²",")=",{"$f":"+AL1588/AS1588","v":-37.5},null," /",{"$f":"+AO1588","v":7.1111111111111111E-2},null,null,"*(",2,"*","u","-",1,")/","u²",null,null,"u  değeri yerine koyulursa"]
[null,null,"2.ci integral hesabı"]
[null,null,{"$f":"+AC1592","v":-37.5},null," /",{"$f":"+AF1592","v":1.8962962962962963E-2},null,null,"ʃ","(",2,"*(","v","-",1,")+",1,")/(","v","-",1,"+",1,")²","*","dv","=",{"$f":"+C1593","v":-37.5},null," /",{"$f":"+F1593","v":1.8962962962962963E-2},null,null,"ʃ","(",2,"*","v","-",1,")/","v²","*","dv","=",{"$f":"+AB1593","v":-37.5},null," /",{"$f":"+AE1593","v":1.8962962962962963E-2},null,null,"( ʃ",2,"*","v"," /","v²","*","dv","-","ʃ",1," /","v²","*","dv",")"]
[null,null,{"$f":"+AK1594","v":-37.5},null," /",{"$f":"+AN1594","v":9.4814814814814814E-3},null,null,"*","Ln  (",null,{"$f":"+AE1591","v":0.26666666666666666},null,"*","x","+",1,")+",{"$f":"+AX1594","v":-37.5},null," /(",{"$f":"+BA1594","v":1.8962962962962963E-2},null,null,"*(",{"$f":"+L1595","v":0.26666666666666666},null,"*","x","+",1,") ) +",null,"C1","*","x","+","C2"]
[null,null,"x = L / 2  ; v' = 0",null,null,null,null,null,null,{"$f":"+G1596","v":-37.5},null,"*(",{"$f":"+J1596","v":0.53333333333333333},null,"*",{"$f":"+M1571","v":2.5},null,"+",1,")/(",{"$f":"+Q1596","v":7.1111111111111111E-2},null,null,"*(",{"$f":"+U1596","v":7.1111111111111111E-2},null,null,"*",{"$f":"+P1599","v":2.5},null,"²+",{"$f":"+AA1596","v":0.53333333333333333},null,"*",{"$f":"+AC1599","v":2.5},null,"+",1,") ) +",null,"C1","=",0,null,null,"C1","=",{"$f":"-(J1599*(M1599*P1599+S1599)/(U1599*(Y1599*AC1599^2+AF1599*AI1599+AL1599)))","v":442.96874999999994}]
[null,null,"y = (",null,{"$f":"+H1601","v":-37.5},null," /",{"$f":"+K1601","v":9.4814814814814814E-3},null,null,"*","Ln  (",null,{"$f":"+Q1601","v":0.26666666666666666},null,"*","x","+",1,")+",{"$f":"+X1601","v":-37.5},null," /(",{"$f":"+AA1601","v":1.8962962962962963E-2},null,null,"*(",{"$f":"+AE1601","v":0.26666666666666666},null,"*","x","+",1,") ) +",null,{"$f":"+AV1599","v":442.96874999999994},null,null,"*","x","+",{"$f":"+BD1600","v":1977.5390625},null,null,") * 108 / ( E * Io )"]
[null,null,"y = (",null,{"$f":"+E1602","v":-37.5},null," /",{"$f":"+H1602","v":9.4814814814814814E-3},null,null,"*","Ln  (",null,{"$f":"+N1602","v":0.26666666666666666},null,"*",{"$f":"+D1603","v":2.5},null,"+",1,")+",{"$f":"+U1602","v":-37.5},null," /(",{"$f":"+X1602","v":1.8962962962962963E-2},null,null,"*(",{"$f":"+AB1602","v":0.26666666666666666},null,"*",{"$f":"+Q1604","v":2.5},null,"+",1,") ) +",null,{"$f":"+AJ1602","v":442.96874999999994},null,null,"*",{"$f":"+AF1604","v":2.5},null,"+",{"$f":"+AP1602","v":1977.5390625},null,null,")* 108 / (",null,null,{"$f":"+AH1576","v":200000},null,null,"*",{"$f":"+AP1571/10000","v":45000},null,null,")"]
[null,null,"y =",null,{"$f":"(E1604/H1604*LN(N1604*Q1604+T1604)+V1604/(Y1604*(AC1604*AF1604+AI1604))+AL1604*AP1604+AS1604)*100000000/(AY1604*BC1604)","v":-1.3546416694038876},null,null,"mm"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,"A","*",{"$f":"+BG1622","v":7},null,"-",{"$f":"+BG1612","v":15},null,"*",{"$f":"+BL1620","v":3.5},null,"=",0,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK1668","v":1.3157894736842106},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,90,null,"mm"]
[null,null,"B","=",{"$f":"+G1617-E1615","v":7.5},null,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x"]
[null,null,"b ( x ) =",null,null,{"$f":"+AS1627/1000","v":0.4},null,"+",{"$f":"(BV1627-AS1627)/AS1627","v":1},null,"*",{"$f":"+F1620","v":0.4},null,"*","x"," /",{"$f":"+AZ1620","v":3.5},null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+BG1622/2","v":3.5},null,"m",null,null,null,null,null,null,null,null,null,{"$f":"+BG1622-AZ1620","v":3.5},null,"m"]
[null,null,"Ix =",null,{"$f":"+F1622","v":0.4},null,"*(",1,"+",{"$f":"+K1622","v":0.2857142857142857},null,"*","x",")*",{"$f":"+BA1614/1000","v":0.09},null,null,"3/",12]
[null,null,"Ix =",null,{"$f":"+E1623","v":0.4},null,"*",{"$f":"+O1623","v":0.09},null,null,"3/",12,null,"*(",1,"+",{"$f":"+J1623","v":0.2857142857142857},null,"*","x",")",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plan"]
[null,null,"M = A * x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AS1627","v":400},null,null,800]
[null,null,"1.ci integral hesabı"]
[null,null,{"$f":"+V1632/AC1632","v":91.875000000000014},null,"ʃ","(","u","-",1,")/","u","*","du","=",{"$f":"+C1633","v":91.875000000000014},null,"ʃ",1,"-",1," /","u","*","du","=",{"$f":"+O1633","v":91.875000000000014},null,"*(","ʃ",1,"*","du","-","ʃ",1," /","u","*","du",")",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uygunluk koşulları"]
[null,null,"2.ci integral hesabı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = 0 ; v = 0"]
[null,null,"u","=",{"$f":"+O1638","v":0.2857142857142857},null,"*","x","+",1,null,null,"x"," =","(","u","-",1,")/",{"$f":"+E1639","v":0.2857142857142857},null,null,null,"dx","=","du"," /",{"$f":"+T1639","v":0.2857142857142857}]
[null,null,"E * Io * v' =",null,null,null,{"$f":"+C1635","v":26.250000000000004},null,"*","x","-",{"$f":"+H1635","v":91.875000000000014},null,"*","Ln","(",{"$f":"+M1635","v":0.2857142857142857},null,"*","x","+",1,")+","C1"]
[null,null,"E * Io * v =",null,null,null,{"$f":"+C1641","v":26.250000000000004},null,"*","x²"," /",2,"-",{"$f":"+J1641","v":91.875000000000014},null,"*((",{"$f":"+M1641","v":0.2857142857142857},null,"*","x","+",1,")*","Ln (",null,{"$f":"+Q1643","v":0.2857142857142857},null,"*","x","+",1,")/",{"$f":"+AC1641","v":0.2857142857142857},null,"-","(",{"$f":"+Z1643","v":0.2857142857142857},null,"*","x","+",1,")/",{"$f":"+AG1643","v":0.2857142857142857},null,"+",1," /",{"$f":"+AS1641","v":0.2857142857142857},null,")+","C1","*","x","+","C2"]
[null,null,"x = L / 2  ; v' = 0",null,null,null,null,null,null,{"$f":"+C1635","v":26.250000000000004},null,"*",{"$f":"+AZ1620","v":3.5},null,"-",{"$f":"+L1642","v":91.875000000000014},null,"*","Ln","(",{"$f":"+Q1642","v":0.2857142857142857},null,"*",{"$f":"+M1645","v":3.5},null,"+",1,")+","C1","=",0,null,null,"C1","=",{"$f":"-(J1645*M1645-P1645*LN(U1645*X1645+AA1645))","v":-28.192102786055031}]
[null,null,"y = (",null,{"$f":"+H1647","v":26.250000000000004},null,"*","x²"," /",2,"-",{"$f":"+O1647","v":91.875000000000014},null,"*((",{"$f":"+R1647","v":0.2857142857142857},null,"*","x","+",1,")*","Ln (",null,{"$f":"+O1648","v":0.2857142857142857},null,"*","x","+",1,")/",{"$f":"+AH1647","v":0.2857142857142857},null,"-","(",{"$f":"+X1648","v":0.2857142857142857},null,"*","x","+",1,")/",{"$f":"+AE1648","v":0.2857142857142857},null,")+",{"$f":"+AV1647","v":-28.192102786055031},null,null,"*","x","+",{"$f":"+BB1647","v":-321.56250000000006},null,null,") * 108 / ( E * Io )"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"BG1622*1000","v":7000},null,null," /",300,null,"=",{"$f":"+H1652/L1652","v":23.333333333333332},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"Vx =",null,{"$f":"+E1656","v":7.5},null,null,"-",{"$f":"+L1656","v":15},null,"=",{"$f":"+E1657-I1657","v":-7.5},null,null,"KN"]
[null,null,"x=",{"$f":"+AZ1620","v":3.5},null,null,"m. ' deki max moment miktarı"]
[null,null,"L / 4 =",null,{"$f":"+BG1622/4","v":1.75},null,null,"m. ' deki moment miktarı"]
[null,null,"MA =",null,{"$f":"+E1662","v":7.5},null,null,"*",{"$f":"+E1663","v":1.75},null,"=",{"$f":"+E1664*I1664","v":13.125},null,null,"KNm"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(M1660)","v":26.25},null,null," /(",2.5,null,"*",{"$f":"+H1668","v":26.25},null,null,"+",3,"*",{"$f":"ABS(L1664)","v":13.125},null,null,"+",4,"*",{"$f":"ABS(L1662)","v":26.25},null,null,"+",3,"*",{"$f":"ABS(U1666)","v":13.125},null,null,")=",{"$f":"E1668*H1668/(L1668*O1668+S1668*U1668+Y1668*AA1668+AE1668*AG1668)","v":1.3157894736842106}]
[]
[null,null,"MESNET TEPKİLERİ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,"KN"]
[null,null,"A","*",{"$f":"+AX1685","v":7},null,"-",{"$f":"+AX1673","v":15},null,"*",{"$f":"+BC1683","v":3.5},null,"-",{"$f":"+AR1674","v":5},null,"*",{"$f":"+AX1685","v":7},null,"*",{"$f":"+Q1675/2","v":3.5},null,"=",0]
[null,null,"B","=",{"$f":"+G1678+J1678*M1678-E1676","v":25},null,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(BN1680),ABS(BO1680),ABS(BP1680),ABS(BQ1680))","v":25},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,"Io = b * h3 / 12",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A=",{"$f":"+E1676","v":25},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E1679","v":25},null,"KN"]
[null,null,"Mx = A * x - w * x² / 2"]
[null,null,"E * Io * v'' =",null,null,null,{"$f":"+AM1682","v":25},null,"*","x","*",{"$f":"+AQ1683","v":3.5},null," /","x","-",{"$f":"+AR1674","v":5},null,"*","x²"," /",2,"*",{"$f":"+AQ1683","v":3.5},null," /","x","=",{"$f":"+G1685*L1685","v":87.5},null,"-",{"$f":"+Q1685*X1685/V1685","v":8.75},null,"*","x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,null,"m"]
[null,null,"sınır ve uygunluk şartları :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm"]
[null,null,"E * Io / 108 * y =",null,null,null,null,{"$f":"+G1687","v":87.5},null,"*","x²"," /",2,"-",{"$f":"+N1687","v":8.75},null,"*","x3"," /",6,"+","C1","*","x","+","C2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AR1679","v":200}]
[null,null,"y = (",null,{"$f":"+H1691","v":87.5},null,"*",{"$f":"+D1693","v":3.5},null,"² /",2,"-",{"$f":"+O1691","v":8.75},null,"*",{"$f":"+H1694","v":3.5},null,"3 /",6,"+",{"$f":"+AD1690","v":-252.65625},null,null,"*",{"$f":"+P1694","v":3.5},null,")* 108 / (",null,null,{"$f":"+AV1700","v":200000},null,null,"*",{"$f":"+BQ1697/10000","v":53333.333333333328},null,null,")",null,null,null,null,null,null,null,null,null,"Io =",null,{"$f":"BM1690*AR1679^3/12","v":533333333.33333331},null,null,null,null,"mm4"]
[null,null,"y=",{"$f":"+E1695","v":-3.8520507812500009},null,null,"mm",null,{"$f":"IF(ABS(D1697)<ABS(M1697),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O1696","v":23.333333333333332},null,null,"mm",null,{"$f":"IF(ABS(D1697)<ABS(M1697),\"uygun.\",\"uygun değil.\")","v":"uygun."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Io =",null,{"$f":"BR1695*BW1691^3/12","v":533333333.33333331},null,null,null,null,"mm4"]
[null,null,"Mx =",null,{"$f":"+AM1682","v":25},null,null,"*",{"$f":"+D1699","v":3.5},null,"-",{"$f":"+AR1674","v":5},null,"*",{"$f":"+D1699","v":3.5},null,"² /",2,"=",{"$f":"+E1700*I1700-L1700*O1700^2/R1700","v":56.875},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,"x=",{"$f":"+AQ1683","v":3.5},null,null,"m. ' deki max moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"üç boyut çizimi"]
[null,null,"MB =",null,{"$f":"+F1704","v":25},null,null,"*",{"$f":"+E1705","v":3.5},null,"-",{"$f":"+M1704","v":5},null,"*",{"$f":"+I1706","v":3.5},null,"² /",2,"=",{"$f":"+E1706*I1706-L1706*O1706^2/R1706","v":56.875},null,null,"KNm"]
[null,null,"L / 4 =",null,{"$f":"+AX1685/4","v":1.75},null,null,"m. ' deki moment miktarı"]
[null,null,"3 * L / 4 =",null,null,{"$f":"+AX1685*3/4","v":5.25},null,null,"m. ' deki moment miktarı"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(U1704)","v":56.875},null,null," /(",2.5,null,"*",{"$f":"+H1712","v":56.875},null,null,"+",3,"*",{"$f":"ABS(T1708)","v":36.09375},null,null,"+",4,"*",{"$f":"ABS(T1706)","v":56.875},null,null,"+",3,"*",{"$f":"ABS(AC1710)","v":36.09375},null,null,")=",{"$f":"E1712*H1712/(L1712*O1712+S1712*U1712+Y1712*AA1712+AE1712*AG1712)","v":1.2126865671641791}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",null,null,null,null,null,null,null,null,null,null,null,"mm"]
[]
[]
[null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca konsol kirişte Cb = 1 alınır.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AA1717","v":150},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(moment diyagramı)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT1721","v":225},null,"KNm",null,null,null,null,null,null,null,"konsol kiriş 3 boyut çizimi"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+BK1724","v":800},null,"mm"]
[null,null,"b ( x ) =",null,null,{"$f":"+F1736","v":0.4},null,"*(",1,"+",{"$f":"+I1736","v":1},null,"*","x"," /",{"$f":"+Q1736","v":1.5},null,")"]
[null,null,"Ix =",null,{"$f":"+F1738","v":0.4},null,"*(",1,"+",{"$f":"+K1738","v":0.66666666666666663},null,"*","x",")*",{"$f":"+BD1720/1000","v":0.3},null,"3 /",12,null,null,null,null,null,null,null,null,{"$f":"+AQ1727","v":150},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ1727","v":150},null,"KN",null,{"$f":"+BD1720","v":300},null,"mm"]
[null,null,"( E * Io * (",null,null,1,"+",{"$f":"+J1741","v":0.66666666666666663},null,"*","x",") ) * v'' = - P * x"]
[null,null,"u","=",{"$f":"+Y1744","v":0.66666666666666663},null,"*","x","+",1,null,null,"x"," =","(","u","-",1,")/",{"$f":"+E1746","v":0.66666666666666663},null,null,null,"dx","=","du"," /",{"$f":"+T1746","v":0.66666666666666663}]
[null,null,{"$f":"+V1747/AC1747","v":-337.5},null,"ʃ","(","u","-",1,")/","u","*","du","=",{"$f":"+C1748","v":-337.5},null,"ʃ",1,"-",1," /","u","*","du","=",{"$f":"+O1748","v":-337.5},null,"*(","ʃ",1,"*","du","-","ʃ",1," /","u","*","du",")"]
[null,null,{"$f":"+Z1748","v":-337.5},null,"*(","u","-","Ln ( u ) ) =",null,null,null,{"$f":"+C1749","v":-337.5},null,"*(",{"$f":"+E1746","v":0.66666666666666663},null,"*","x","+",1,"-","Ln","(",{"$f":"+E1746","v":0.66666666666666663},null,"*","x","+",1,") )"]
[null,null,{"$f":"+C1750","v":-225},null,"*","x","-",{"$f":"+H1750","v":-337.5},null,"*","Ln","(",{"$f":"+M1750","v":0.66666666666666663},null,"*","x","+",1,")"]
[null,null,"ʃ","Ln ( u ) /",null,null,{"$f":"+AB1754","v":0.66666666666666663},null,"*","du","=","u","*","Ln","(","u",")/",{"$f":"+G1755","v":0.66666666666666663},null,"-","u"," /",{"$f":"+R1755","v":0.66666666666666663},null,"=","(",{"$f":"+E1754","v":0.66666666666666663},null,"*","x","+",1,")*","Ln (",null,{"$f":"+AA1755","v":0.66666666666666663},null,"*","x","+",1,")/",{"$f":"+R1755","v":0.66666666666666663},null,"-","(",{"$f":"+AJ1755","v":0.66666666666666663},null,"*","x","+",1,")/",{"$f":"+AQ1755","v":0.66666666666666663},null,"+",1," /",{"$f":"+BB1755","v":0.66666666666666663}]
[null,null,"E * Io * v =",null,null,null,{"$f":"+C1756","v":-225},null,"*","x²"," /",2,"-",{"$f":"+J1756","v":-337.5},null,"*((",{"$f":"+M1756","v":0.66666666666666663},null,"*","x","+",1,")*","Ln (",null,{"$f":"+V1756","v":0.66666666666666663},null,"*","x","+",1,")/",{"$f":"+AC1756","v":0.66666666666666663},null,"-","(",{"$f":"+AG1756","v":0.66666666666666663},null,"*","x","+",1,")/",{"$f":"+AN1756","v":0.66666666666666663},null,"+",1," /",{"$f":"+AS1756","v":0.66666666666666663},null,")+","C1","*","x","+","C2"]
[null,null,"x = L ; v = 0",null,null,null,null,null,{"$f":"+C1756","v":-225},null,"*",{"$f":"+L1760","v":1.5},null,"² /",2,"-",{"$f":"+J1756","v":-337.5},null,"*((",{"$f":"+M1756","v":0.66666666666666663},null,"*",{"$f":"+L1761","v":1.5},null,"+",1,")*","Ln (",null,{"$f":"+V1756","v":0.66666666666666663},null,"*",{"$f":"+W1761","v":1.5},null,"+",1,")/",{"$f":"+AC1756","v":0.66666666666666663},null,"-","(",{"$f":"+AG1756","v":0.66666666666666663},null,"*",{"$f":"+AG1761","v":1.5},null,"+",1,")/",{"$f":"+AN1756","v":0.66666666666666663},null,"+",1," /",{"$f":"+AS1756","v":0.66666666666666663},null,")+",{"$f":"+AI1760","v":103.56282656101845},null,null,"*",{"$f":"+AS1761","v":1.5},null,"+","C2","=",0,null,null,"C2","=",{"$f":"-(I1761*L1761^2/O1761-Q1761*((T1761*W1761+Z1761)*LN(AD1761*AG1761+AJ1761)/AL1761-(AP1761*AS1761+AV1761)/AX1761+BA1761/BC1761)+BF1761*BJ1761)","v":-97.78076015847239}]
[null,null,"x=",0,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,{"$f":"IF(D1764<=AI1728,\"\",\"azalt.\")","v":""},null,null,null,"(konsol ucu sehim için  x = 0  giriniz.)"]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"AI1728*1000","v":1500},null,null," /",150,null,"=",{"$f":"+H1767/L1767","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E1766","v":-0.54322644532484654},null,null,"mm",null,{"$f":"IF(ABS(D1768)<ABS(M1768),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O1767","v":10},null,null,"mm",null,{"$f":"IF(ABS(D1768)<ABS(M1768),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,"TEKİL YÜKLÜ ÇELİK KONSOL KİRİŞ SEHİM HESABI (değişken kesit)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,150,null,"KN",null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kiriş ucu enkesiti",null,null,null,null,null,null,null,null,null,"kiriş mesnet enkesiti",null,null,null,null,null,null,null,null,null,null,null,null,null,"(moment diyagramı)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+X1777","v":225},null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+E1773*M1784","v":225},null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600,{"$f":"IF(AR1777>AH1776,\"\",\"artır.\")","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Io =",null,{"$f":"PI()*AH1776^4/64","v":397607820.21995819},null,null,null,null,"mm4",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U1783","v":150},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U1783","v":150},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"PI()*AR1777^4/64","v":6361725123.519331},null,null,null,null,"mm4",null,null,null,null,null,null,null,null,null,null,null,null,null,"+"]
[null,null,null,"SEHİM HESABI"]
[null,null,null,"d ( x ) =",null,null,{"$f":"+AH1776/1000","v":0.3},null,"+",{"$f":"(AR1777-AH1776)/AH1776","v":1},null,"*",{"$f":"+G1787","v":0.3},null,"*","x"," /",{"$f":"+M1784","v":1.5}]
[null,null,null,"Io = p * d4 / 64"]
[null,null,null,"( E * Io * (",null,null,1,"+",{"$f":"+AD1790","v":0.66666666666666663},null,"*","x",")4",")*","v''","=","-","P","*","x"]
[null,null,null,"u","=",{"$f":"+L1795","v":0.66666666666666663},null,"*","x","+",1,null,null,"x","=","(","u","-",1,")/",{"$f":"+F1796","v":0.66666666666666663},null,null,null,null,"dx","=",1," /",{"$f":"+U1796","v":0.66666666666666663}]
[null,null,null,{"$f":"+D1797","v":-150},null," /",{"$f":"+L1797","v":0.44444444444444442},null,"ʃ",1," /","u3","-",1," /","u4","*","du"]
[null,null,null,{"$f":"+D1800/G1800","v":-337.5},null,null,"*(",{"$f":"J1800/L1800","v":-0.5},null," /(",{"$f":"+N1800","v":0.66666666666666663},null,"*","x","+",1," )² ","-",{"$f":"+V1800/X1800","v":-0.33333333333333331},null," /(",{"$f":"+Z1800","v":0.66666666666666663},null,"*","x","+",1," )3 ",")"]
[null,null,null,"2.ci integral hesabı"]
[null,null,null,{"$f":"+D1805","v":168.75},null,null,"*",-1," /(",{"$f":"+J1805","v":0.66666666666666663},null,"*","u",")-",{"$f":"+T1805","v":112.5},null,null,"*",-1," /(",{"$f":"Z1805*2","v":1.3333333333333333},null,"*","u²",")"]
[null,null,null,"E * Io * v' =",null,null,null,{"$f":"+D1802","v":168.75},null,null," /(",{"$f":"+H1802","v":0.66666666666666663},null,"*","x","+",1," )² ","-",{"$f":"+P1802","v":112.5},null,null," /(",{"$f":"+T1802","v":0.66666666666666663},null,"*","x","+",1," )3 ","+","C1"]
[null,null,null,"sınır ve uygunluk şartları :"]
[null,null,null,"x = L ; v' = 0",null,null,null,null,null,{"$f":"+H1810","v":168.75},null,null," /(",{"$f":"+J1805","v":0.66666666666666663},null,"*",{"$f":"+M1784","v":1.5},null,"+",1,")²","-",{"$f":"+T1810","v":112.5},null,null," /(",{"$f":"+X1810","v":0.66666666666666663},null,"*",{"$f":"+Q1813","v":1.5},null,"+",1," )3 ","+","C1","=",0,null,null,"C1","=",{"$f":"-(J1813/(N1813*Q1813+T1813)^2-W1813/(AA1813*AD1813+AG1813)^3)","v":-28.125}]
[null,null,null,"y = (",null,{"$f":"+I1815","v":-253.125},null,null,"/(",{"$f":"+M1815","v":0.66666666666666663},null,"*","x","+",1," )-",{"$f":"+T1815","v":-84.375},null,null,"/(",{"$f":"+X1815","v":0.66666666666666663},null,"*","x","+",1,")² ","+",{"$f":"+AQ1813","v":-28.125},null,null,"*","x","+",{"$f":"+AW1814","v":147.65625},null,null,") * 108 / ( E * Io )"]
[null,null,null,"y =",null,{"$f":"(F1818/(J1818*M1818+P1818)-R1818/(V1818*Y1818+AB1818)^2+AE1818*AI1818+AL1818)*100000000/(AR1818*AV1818)","v":-0.26525823848649227},null,null,"mm"]
[]
[null,null,null,150,null,"KN",null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kiriş ucu enkesiti",null,null,null,null,null,null,null,null,null,"kiriş mesnet enkesiti",null,null,null,null,null,null,null,null,null,null,null,null,null,"(moment diyagramı)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+W1830","v":225},null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",null,null,null,null,null,null,null,null,{"$f":"+AB1830","v":5}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(kesme kuvveti diyagramı)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"PI()*AK1831*(AR1830-AK1831)^3/8","v":413600244.88521266},null,null,null,null,"mm4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"+"]
[null,null,null,null,null,null,null,null,null,null,null,1.5,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,null,"( t / dm )² = (",null,null,null,{"$f":"+AB1830","v":5},null," /",{"$f":"+AH1829-AB1830","v":295},null,")² =",null,{"$f":"(H1841/K1841)^2","v":2.8727377190462512E-4},null,null,{"$f":"IF(O1841<S1841,\"<\",\">\")","v":"<"},1,null,null,{"$f":"IF(O1841<S1841,\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,null,"Ix = p * t * d3 / 8 =",null,null,null,null,null,"p","*",{"$f":"+AB1830/1000","v":5.0000000000000001E-3},null,null,"*(",{"$f":"+U1843","v":0.29499999999999998},null,null,"*(",1,"+",{"$f":"+AA1843","v":0.67796610169491522},null,"*","x",") )3 /",null,8,"=","Io","*(",1,"+",{"$f":"+V1844","v":0.67796610169491522},null,"*","x",")3"]
[null,null,null,"E * Io * v'' =",null,null,null,"-","P","*","x"," /(",1,"+",{"$f":"+I1846","v":0.67796610169491522},null,"*","x",")3","=",{"$f":"-D1826","v":-150},null,"*","x"," /(",1,"+",{"$f":"+O1847","v":0.67796610169491522},null,"*","x",")3"]
[null,null,null,"u","=",{"$f":"+L1849","v":0.67796610169491522},null,"*","x","+",1,null,null,"x","=","(","u","-",1,")/",{"$f":"+F1850","v":0.67796610169491522},null,null,null,null,"dx","=",1," /",{"$f":"+U1850","v":0.67796610169491522}]
[null,null,null,{"$f":"+E1849","v":-150},null,"ʃ","(","u","-",1,")/(",{"$f":"+U1850*AD1850","v":0.45963803504740014},null,"*","u3",")*","du"]
[null,null,null,{"$f":"+D1852","v":-150},null," /",{"$f":"+G1852","v":0.45963803504740014},null,"*(",-1," /","u","-",-1," /(",2,"*","u²","))"]
[null,null,null,{"$f":"+D1855*H1855","v":326.34375},null,null," /(",{"$f":"+J1855","v":0.67796610169491522},null,"*","x","+",1," )- ",{"$f":"+D1855*Q1855","v":163.171875},null,null," /(",{"$f":"+T1855","v":0.67796610169491522},null,"*","x","+",1," )² "]
[null,null,null,{"$f":"+D1859","v":326.34375},null,null,"* Ln (",null,{"$f":"+J1859","v":0.67796610169491522},null,"*","x","+",1,")/",{"$f":"+I1860","v":0.67796610169491522},null,"-",{"$f":"+S1859","v":163.171875},null,null,"*(",-1," /(",{"$f":"+Y1859","v":0.67796610169491522},null,"*(",{"$f":"+Y1859","v":0.67796610169491522},null,"*","x","+",1,") ) )"]
[null,null,null,"E * Io * v' =",null,null,null,{"$f":"+D1856","v":326.34375},null,null," /(",{"$f":"+H1856","v":0.67796610169491522},null,"*","x","+",1," )- ",{"$f":"+O1856","v":163.171875},null,null," /(",{"$f":"+S1856","v":0.67796610169491522},null,"*","x","+",1," )² ","+","C1"]
[null,null,null,"x = L ; v' = 0",null,null,null,null,null,{"$f":"+D1856","v":326.34375},null,null," /(",{"$f":"+H1856","v":0.67796610169491522},null,"*",{"$f":"+L1837","v":1.5},null,"+",1,")-",{"$f":"+O1856","v":163.171875},null,null," /(",{"$f":"+S1856","v":0.67796610169491522},null,"*",{"$f":"+Q1865","v":1.5},null,"+",1," )² ","+","C1","=",0,null,null,"C1","=",{"$f":"-(J1865/(N1865*Q1865+T1865)-V1865/(Z1865*AC1865+AF1865)^2)","v":-121.69042948061579}]
[null,null,null,"E * Io / 108 * y =",null,null,null,null,{"$f":"+H1863","v":481.35703125000003},null,null,"* Ln (",null,{"$f":"+M1863","v":0.67796610169491522},null,"*","x","+",1,")-",{"$f":"+T1863","v":-240.67851562500002},null,null," /(",{"$f":"+X1863","v":0.67796610169491522},null,"*","x","+",1,")+","C1","*","x","+","C2"]
[null,null,null,"y =",null,{"$f":"(F1870*LN(K1870*N1870+Q1870)-S1870/(W1870*Z1870+AC1870)+AE1870*AI1870+AL1870)*100000000/(AR1870*AV1870)","v":-3.3553698180859035},null,null,"mm"]
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK KONSOL KİRİŞ SEHİM HESABI (değişken kesit)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"a",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"b",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kesit b - b"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,"z"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0.8,null,"m",null,null,null,{"$f":"+Q1894-N1892","v":0.7},null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(Y1888,$CG$6:$CG$120,0),0)","v":19}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(Y1888,$CG$6:$CG$120,0),0)","v":220}]
[null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AN1879","v":85}]
[null,null,"SEHİM HESABI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"2*(AN1879*AG1882^3/12+AG1882*AN1879*(AP1899/2+AG1882/2)^2)","v":158156666.66666666},null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(Y1888,$CG$6:$CG$120,0),0)","v":600}]
[null,null,"1.ci bölgede :"]
[null,null,"v1 =",null,{"$f":"+E1904","v":-2.2336392873362229E-3},null,null,"*","x²"," /",2,"+",{"$f":"+K1904","v":1.7609604339995119E-3},null,null,"*","x3"," /",6,"+",{"$f":"+S1904","v":2.3170532026309365E-4},null,null,"*","x4"," /",12,null,"+","C1","*","x","+","C2"]
[null,null,"v2' =",null,{"$f":"+AO1907","v":-2.6172893136403126E-3},null,null,"*","z","+",{"$f":"+AU1907","v":2.0634231103388357E-3},null,null,"*(",{"$f":"+AY1907","v":0.8},null,"+","z",")²"," /",2,"+",{"$f":"+BD1907","v":4.3440486533449172E-4},null,null,"*(",{"$f":"+BH1907","v":0.4},null,"+","z",")²"," /",2,"+","D1"]
[null,null,"x = 0 ; v1' = 0",null,null,null,null,null,"C1 = 0"]
[null,null,"z = 0 ; v2' =",null,null,null,{"$f":"+K1908","v":2.0634231103388357E-3},null,null,"*",{"$f":"+O1908","v":0.8},null,"² /",2,"+",{"$f":"+W1908","v":4.3440486533449172E-4},null,null,"*",{"$f":"+AA1908","v":0.4},null,"² /",2,"+","D1","=","D1","+",{"$f":"G1914*K1914^2/N1914+P1914*T1914^2/W1914","v":6.9504778453518688E-4}]
[null,null,"( x = L ; v1' ) = ( x = L ; v2' )",null,null,null,null,null,null,null,null,null,"D1","+",{"$f":"+AC1914","v":6.9504778453518688E-4},null,null,"=",{"$f":"+AF1913","v":-1.1838597163309E-3},null,null,null,null,"D1","=",{"$f":"+S1915-O1915","v":-1.8789075008660869E-3}]
[null,null,"z = 0 ; v2 =",null,null,null,{"$f":"+M1909","v":2.0634231103388357E-3},null,null,"*",{"$f":"+Q1909","v":0.8},null,"3 /",6,"+",{"$f":"+Y1909","v":4.3440486533449172E-4},null,null,"*",{"$f":"+AC1909","v":0.4},null,"3 /",6,"+","D2","=","D2","+",{"$f":"G1917*K1917^3/N1917+P1917*T1917^3/W1917","v":1.8071242397914861E-4}]
[null,null,"E / 108 * y =",null,null,null,{"$f":"+E1905","v":-2.2336392873362229E-3},null,null,"*","x²"," /",2,"+",{"$f":"+M1905","v":1.7609604339995119E-3},null,null,"*","x3"," /",6,"+",{"$f":"+U1905","v":2.3170532026309365E-4},null,null,"*","x4"," /",12,null,"+","C1","*","x","+","C2"]
[null,null,"y =",null,{"$f":"(E1923*I1923^2/L1923+N1923*R1923^3/U1923+W1923*AA1923^4/AD1923)*100000000/AI1923","v":-0.27829353665732642},null,null,"mm"]
[null,null,"y=",{"$f":"+E1924","v":-0.27829353665732642},null,null,"mm",null,{"$f":"IF(ABS(D1926)<ABS(M1926),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O1925","v":10},null,null,"mm",null,{"$f":"IF(ABS(D1926)<ABS(M1926),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"y = (",null,{"$f":"+G1928","v":-2.6172893136403126E-3},null,null,"*","z²"," /",2,"+",{"$f":"+O1928","v":2.0634231103388357E-3},null,null,"*(",{"$f":"+S1928","v":0.8},null,"+","z",")3"," /",6,"+",{"$f":"+AA1928","v":4.3440486533449172E-4},null,null,"*(",{"$f":"+AE1928","v":0.4},null,"+","z",")3"," /",6,"+",{"$f":"+Z1915","v":-1.8789075008660869E-3},null,null,"*","z","+",{"$f":"+Z1918","v":-7.3729949729380148E-4},null,null,") * 108 /  E "]
[null,null,"y = (",null,{"$f":"+E1929","v":-2.6172893136403126E-3},null,null,"*",{"$f":"+D1930","v":0},null,"² /",2,"+",{"$f":"+M1929","v":2.0634231103388357E-3},null,null,"*(",{"$f":"+Q1929","v":0.8},null,"+",{"$f":"+I1931","v":0},null,")3"," /",6,"+",{"$f":"+Y1929","v":4.3440486533449172E-4},null,null,"*(",{"$f":"+AC1929","v":0.4},null,"+",{"$f":"+I1931","v":0},null,")3"," /",6,"+",{"$f":"+AK1929","v":-1.8789075008660869E-3},null,null,"*",{"$f":"+I1931","v":0},null,"+",{"$f":"+AQ1929","v":-7.3729949729380148E-4},null,null,")* 108 /",null,null,{"$f":"+AI1923","v":200000}]
[]
[]
[null,null,null,null,null,null,"(moment diyagramı)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT1943","v":225},null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(2.ci bölge)",null,null,null,null,null,null,"(1.ci bölge)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"mm"]
[]
[null,null,{"$f":"+AQ1949","v":150},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ1949","v":150},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.8,null,"m",null,null,null,null,null,{"$f":"+AI1952-AE1950","v":0.7},null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"I1 =",null,{"$f":"BI1948*BL1943^3/12","v":2083333333.3333333},null,null,null,null,"mm4"]
[null,null,"SEHİM HESABI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,"Mx2 =",null," -Ma+",null,"A","*(",{"$f":"+AM1950","v":0.7},null,"+","z",")=",{"$f":"-AT1943","v":-225},null,"+",{"$f":"+AQ1949","v":150},null,"*(",{"$f":"+AM1950","v":0.7},null,"+","z",")=",{"$f":"+Q1956","v":150},null,"*","z","+",{"$f":"+Q1956*T1956+N1956","v":-120},null,null,"(2.ci bölge)"]
[null,null,"1.ci bölgede :"]
[null,null,"v1 =",null,{"$f":"+E1959","v":7.2000000000000005E-4},null,null,"*","x3"," /",6,"+",{"$f":"+M1959","v":-1.08E-3},null,null,"*","x²"," /",2,"+","C1","*","x","+","C2"]
[null,null,"v2' =",null,{"$f":"+W1962","v":3.3333333333333335E-3},null,null,"*","z²"," /",2,"+",{"$f":"+AC1962","v":-2.6666666666666666E-3},null,null,"*","z","+","D1"]
[null,null,"x = 0 ; v1' = 0",null,null,null,null,null,"C1 = 0"]
[null,null,"z = 0 ; v2' =",null,null,null,"D1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca konsol kirişte Cb = 1 alınır."]
[null,null,"z = 0 ; v2 =",null,null,null,"D2"]
[null,null,"E / 108 * y =",null,null,null,{"$f":"+E1960","v":7.2000000000000005E-4},null,null,"*","x3"," /",6,"+",{"$f":"+M1960","v":-1.08E-3},null,null,"*","x²"," /",2,"+","C1","*","x","+","C2"]
[null,null,"y = (",null,{"$f":"+E1976","v":7.2000000000000005E-4},null,null,"*",{"$f":"+D1977","v":0.7},null,"3/",6,"+",{"$f":"+M1976","v":-1.08E-3},null,null,"*",{"$f":"+I1978","v":0.7},null,"² /",2,")* 108 /",null,null,{"$f":"+AH1954","v":200000}]
[null,null,"y =",null,{"$f":"(E1978*I1978^3/L1978+N1978*R1978^2/U1978)*100000000/Y1978","v":-0.11172},null,null,"mm"]
[null,null,"y=",{"$f":"+E1979","v":-0.11172},null,null,"mm",null,{"$f":"IF(ABS(D1981)<ABS(M1981),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O1980","v":10},null,null,"mm",null,{"$f":"IF(ABS(D1981)<ABS(M1981),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"y = (",null,{"$f":"+G1983","v":3.3333333333333335E-3},null,null,"*","z3"," /",6,"+",{"$f":"+O1983","v":-2.6666666666666666E-3},null,null,"*","z²"," /",2,"+",{"$f":"+O1970","v":-5.7959999999999999E-4},null,null,"*","z","+",{"$f":"+O1973","v":-2.2343999999999999E-4},null,null,") * 108 /  E "]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"AI1952*1000","v":1500},null,null," /",150,null,"=",{"$f":"+H1988/L1988","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"(1.ci bölge)",null,null,null,null,null,null,null,"(2.ci bölge)",null,null,null,null,null,null,null,"(3.cü bölge)",null,null,null,null,150,null,"KN"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"I3 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(AC2000,$CG$6:$CG$120,0),0)","v":8360},null,null,"cm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,"I1 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(M2001,$CG$6:$CG$120,0),0)","v":92080},null,null,"cm4",null,null,"I2 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(U2001,$CG$6:$CG$120,0),0)","v":48200},null,null,"cm4",null,null,"IPE 300"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.8,null,"m",null,null,null,null,null,0.9,null,"m",null,null,null,null,null,0.5,null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+O2004+W2004+AE2004","v":2.2000000000000002},null,"m"]
[null,null,"Mx2 =",null," -Ma +",null,"A","*(",{"$f":"+O2004","v":0.8},null,"+","z",")=",{"$f":"-F1998","v":-330},null,"+",{"$f":"+K2003","v":150},null,"*(",{"$f":"+I2009","v":0.8},null,"+","z",")=",{"$f":"+Q2009","v":150},null,"*","z","+",{"$f":"+Q2009*T2009+N2009","v":-210},null,null,"(2.ci bölge)"]
[null,null,"1.ci bölgede :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(M2001,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(U2001,$CG$6:$CG$120,0),0)","v":16},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(AC2000,$CG$6:$CG$120,0),0)","v":10.7}]
[null,null,"2.ci bölgede :"]
[null,null,"v2 =",null,{"$f":"+E2017","v":3.1120331950207467E-3},null,null,"*","z3"," /",6,"+",{"$f":"+M2017","v":-1.5560165975103729E-3},null,null,"*","z²"," /",2,"+","D1","*","z","+","D2"]
[null,null,"v3'' =",null,{"$f":"+Y2010","v":150},null,"*","k"," /",{"$f":"+AE1999","v":8360},null,null,null,"+",{"$f":"+AD2010","v":-74.999999999999972},null," /",{"$f":"+J2020","v":8360},null,null,null,"=",{"$f":"+E2020/J2020","v":1.7942583732057416E-2},null,null,"*","k","+",{"$f":"+O2020/R2020","v":-8.9712918660287046E-3}]
[null,null,"v3' =",null,{"$f":"+W2020","v":1.7942583732057416E-2},null,null,"*","k²"," /",2,"+",{"$f":"+AC2020","v":-8.9712918660287046E-3},null,null,"*","k","+","E1"]
[null,null,"x = 0 ; v1' = 0",null,null,null,null,null,"C1 = 0"]
[null,null,"z = 0 ; v2' =",null,null,null,"D1"]
[null,null,"z = 0 ; v2 =",null,null,null,"D2"]
[null,null,"k = 0 ; v3' =",null,null,null,"E1"]
[null,null,"k = 0 ; v3 =",null,null,null,"E2"]
[null,null,"E / 108 * y =",null,null,null,{"$f":"+E2014","v":1.6290182450043439E-3},null,null,"*","x3"," /",6,"+",{"$f":"+M2014","v":-3.5838401390095569E-3},null,null,"*","x²"," /",2,"+","C1","*","x","+","C2"]
[null,null,"y = (",null,{"$f":"+E2040","v":1.6290182450043439E-3},null,null,"*",{"$f":"+D2041","v":0.8},null,"3/",6,"+",{"$f":"+M2040","v":-3.5838401390095569E-3},null,null,"*",{"$f":"+I2042","v":0.8},null,"² /",2,")* 108 /",null,null,{"$f":"+AN1998","v":200000}]
[null,null,"y =",null,{"$f":"(E2042*I2042^3/L2042+N2042*R2042^2/U2042)*100000000/Y2042","v":-0.50390964378801051},null,null,"mm"]
[null,null,"y=",{"$f":"+E2043","v":-0.50390964378801051},null,null,"mm",null,{"$f":"IF(ABS(D2045)<ABS(M2045),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O2044","v":14.666666666666666},null,null,"mm",null,{"$f":"IF(ABS(D2045)<ABS(M2045),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"z=",0.9,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,{"$f":"IF(D2049>W2004,\"azalt.\",\"\")","v":""}]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"W2006*1000","v":2200},null,null," /",150,null,"=",{"$f":"+H2052/L2052","v":14.666666666666666},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"3.cü bölgede :"]
[null,null,"y = (",null,{"$f":"+E2056","v":1.7942583732057416E-2},null,null,"*",{"$f":"+D2057","v":0.5},null,"3/",6,"+",{"$f":"+M2056","v":-8.9712918660287046E-3},null,null,"*",{"$f":"+I2058","v":0.5},null,"² /",2,"+",{"$f":"+U2056","v":-2.4858277665821887E-3},null,null,"*",{"$f":"+R2058","v":0.5},null,"+",{"$f":"+AA2056","v":-3.3711016218983311E-3},null,null,")* 108 /",null,null,{"$f":"+AJ2050","v":200000}]
[null,null,"y =",null,{"$f":"(E2058*I2058^3/L2058+N2058*R2058^2/U2058+W2058*AA2058+AD2058)*100000000/AJ2058","v":-2.6808115803459085},null,null,"mm"]
[null,null,"y=",{"$f":"+E2059","v":-2.6808115803459085},null,null,"mm",null,{"$f":"IF(ABS(D2061)<ABS(M2061),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O2060","v":14.666666666666666},null,null,"mm",null,{"$f":"IF(ABS(D2061)<ABS(M2061),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,"YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI (değişken kesit)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,8,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,"KN/m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK2115","v":1.1683963872378638},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,null,null,"I1 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(I2074,$CG$6:$CG$120,0),0)","v":8360},null,null,"cm4",null,null,null,null,null,null,null,null,null,null,"I3 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(Y2074,$CG$6:$CG$120,0),0)","v":48200},null,null,"cm4",null,null,null,null,null,null,null,null,null,{"$f":"+G2075","v":29.94318181818182},{"$f":"+AN2073-K2068*K2077","v":15.94318181818182},{"$f":"+AO2073-S2067*S2077","v":-11.05681818181818},{"$f":"+AP2073-AA2068*AA2077","v":-24.05681818181818}]
[null,null,null,null,null,"A=",{"$f":"+E2088","v":29.94318181818182},null,"KN",null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E2091","v":24.05681818181818},null,"KN",null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+K2077+S2077+AA2077","v":6.6},null,"m"]
[]
[null,null,null,null,null,null,null,null,null,null,"(x = L ; v1 ) = (z = 0 ; v2 )",null,null,null,null,null,null,null,null,null,"(z = L ; v2 ) = (k = 0 ; v3 )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(I2074,$CG$6:$CG$120,0),0)","v":300},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(Q2075,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(Y2074,$CG$6:$CG$120,0),0)","v":500}]
[null,null,"MESNET TEPKİLERİ"]
[null,null,"Fy = 0    (düşey denge denklemi yazılırsa)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(I2074,$CG$6:$CG$120,0),0)","v":150},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(Q2075,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(Y2074,$CG$6:$CG$120,0),0)","v":200}]
[null,null,"B =",null,{"$f":"+G2090*J2090+M2090*P2090+S2090*V2090-E2088","v":24.05681818181818},null,"KN",null,"(sağ mesnet tepkisi)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"I1 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(I2074,$CG$6:$CG$120,0),0)","v":8360},null,null,null,"cm4",null,null,null,null,null,null,null,"I2 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(Q2075,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,null,null,null,null,"I3 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(Y2074,$CG$6:$CG$120,0),0)","v":48200},null,null,null,"cm4"]
[null,null,"x=",1,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D2094<=K2077,\"\",\"azalt.\")","v":""}]
[null,null,"Vx =",null,{"$f":"+E2095","v":29.94318181818182},null,"-",{"$f":"+K2095","v":8},null,"*",{"$f":"+N2095","v":1},null,"=",{"$f":"+E2096-H2096*K2096","v":21.94318181818182},null,null,"KN"]
[null,null,"Vx =",null,{"$f":"+E2099","v":29.94318181818182},null,"-",{"$f":"+N2099","v":8},null,"*",{"$f":"+Q2099","v":1.75},null,"-",{"$f":"+Z2099","v":12},null,"*",{"$f":"+AC2099","v":1},null,"=",{"$f":"+E2100-H2100*K2100-N2100*Q2100","v":3.9431818181818201},null,null,"KN"]
[null,null,"Mx =",null,{"$f":"+G2075","v":29.94318181818182},null,"*(",{"$f":"+K2077+S2077","v":4},null,"+",{"$f":"+D2102","v":1},null,")-",{"$f":"+K2068","v":8},null,"*",{"$f":"+K2077","v":1.75},null,"*(",{"$f":"+K2077/2+S2077","v":3.125},null,"+",{"$f":"+D2102","v":1},null,")-",{"$f":"+S2067","v":12},null,"*",{"$f":"+S2077","v":2.25},null,"*(",{"$f":"+S2077/2","v":1.125},null,"+",{"$f":"+D2102","v":1},null,")-",{"$f":"+AA2068","v":5},null,"*",{"$f":"+D2102","v":1},null,"² /",2,"=",{"$f":"+E2103*(H2103+K2103)-N2103*Q2103*(T2103+W2103)-Z2103*AC2103*(AF2103+AI2103)-AL2103*AO2103^2/AR2103","v":32.090909090909093},null,null,"KNm"]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,"z=",{"$f":"((G2075-K2068*K2077+S2067*K2077)/S2067)-K2077","v":1.3285984848484849},null,null,"m. ' deki max moment miktarı"]
[null,null,"MB =",null,{"$f":"+F2107","v":29.94318181818182},null,"*(",{"$f":"+I2107","v":1.75},null,"+",{"$f":"+F2108","v":1.5499999999999998},null,")-",{"$f":"+O2107","v":8},null,"*",{"$f":"+R2107","v":1.75},null,"*(",{"$f":"+U2107","v":0.875},null,"+",{"$f":"+F2108","v":1.5499999999999998},null,")-",{"$f":"+AA2107","v":12},null,"*",{"$f":"+F2108","v":1.5499999999999998},null,"² /",2,"=",{"$f":"E2109*(H2109+K2109)-N2109*Q2109*(T2109+W2109)-Z2109*AC2109^2/AF2109","v":50.447500000000019},null,null,"KNm"]
[null,null,"k=","3 * L / 4 =",null,null,{"$f":"+S2079*3/4-K2077-S2077","v":0.94999999999999929},null,null,"m. ' deki moment miktarı"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AI2107)","v":50.741611785468322},null,null," /(",2.5,null,"*",{"$f":"+H2115","v":50.741611785468322},null,null,"+",3,"*",{"$f":"ABS(S2111)","v":38.516249999999999},null,null,"+",4,"*",{"$f":"ABS(AH2109)","v":50.447500000000019},null,null,"+",3,"*",{"$f":"ABS(AT2113)","v":32.887500000000045},null,null,")=",{"$f":"E2115*H2115/(L2115*O2115+S2115*U2115+Y2115*AA2115+AE2115*AG2115)","v":1.1683963872378638}]
[null,null,"v1' =",null,{"$f":"+Y2118","v":3.5817203131796437E-3},null,null,"*","x²"," /",2,"-",{"$f":"+AE2118","v":4.7846889952153111E-4},null,null,"*","x3"," /",3,"+","C1"]
[null,null,"2.ci bölgede :"]
[null,null,"v2 =",null,{"$f":"+E2123","v":3.2518659663533688E-4},null,null,"*(",{"$f":"+I2123","v":1.75},null,"+","z",")3"," /",6,"-",{"$f":"+Q2123","v":1.5204170286707211E-4},null,null,"*(",{"$f":"+U2123","v":0.875},null,"+","z",")3"," /",6,"-",{"$f":"+AC2123","v":6.5160729800173764E-5},null,null,"*","z4"," /",12,null,"+","D1","*","z","+","D2"]
[null,null,"3.cü bölgede :"]
[null,null,"v3' =",null,{"$f":"+E2127","v":6.2122783855149009E-4},null,null,"*(",{"$f":"+I2127","v":4},null,"+","k",")²"," /",2,"-",{"$f":"+N2127","v":2.9045643153526973E-4},null,null,"*(",{"$f":"+R2127","v":3.125},null,"+","k",")²"," /",2,"-",{"$f":"+W2127","v":5.6016597510373447E-4},null,null,"*(",{"$f":"+AA2127","v":1.125},null,"+","k",")²"," /",2,"-",{"$f":"+AF2127","v":5.1867219917012447E-5},null,null,"*","k3"," /",3,"+","E1"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"x = L ; v1 =",null,null,null,{"$f":"+E2120","v":3.5817203131796437E-3},null,null,"*",{"$f":"+K2077","v":1.75},null,"3 /",6,"-",{"$f":"+M2120","v":4.7846889952153111E-4},null,null,"*",{"$f":"+K2134","v":1.75},null,"4 /",12,null,"+","C1","*",{"$f":"+T2134","v":1.75},null,"=","C1","*",{"$f":"+AB2134","v":1.75},null,"+",{"$f":"G2134*K2134^3/N2134-P2134*T2134^4/W2134","v":2.8253374712284333E-3}]
[null,null,"x = L ; v1' =",null,null,null,{"$f":"+E2119","v":3.5817203131796437E-3},null,null,"*",{"$f":"+K2077","v":1.75},null,"² /",2,"-",{"$f":"+M2119","v":4.7846889952153111E-4},null,null,"*",{"$f":"+K2137","v":1.75},null,"3 /",3,"+","C1","=","C1","+",{"$f":"+G2137*K2137^2/N2137-P2137*T2137^3/W2137","v":4.6297444767652608E-3}]
[null,null,"z = L ; v2 = ",null,null,null,{"$f":"+E2124","v":3.2518659663533688E-4},null,null,"*(",{"$f":"+I2124","v":1.75},null,"+",{"$f":"+S2077","v":2.25},null,")3"," /",6,"-",{"$f":"+Q2124","v":1.5204170286707211E-4},null,null,"*(",{"$f":"+U2124","v":0.875},null,"+",{"$f":"+N2140","v":2.25},null,")3"," /",6,"-",{"$f":"+AC2124","v":6.5160729800173764E-5},null,null,"*",{"$f":"+AA2140","v":2.25},null,"4 /",12,null,"+","D1","*",{"$f":"+AK2140","v":2.25},null,"+","D2","=","D1","*",{"$f":"+AS2140","v":2.25},null,"+","D2","+",{"$f":"G2140*(K2140+N2140)^3/R2140-T2140*(X2140+AA2140)^3/AE2140-AG2140*AK2140^4/AN2140","v":2.556166420257089E-3}]
[null,null,"z = L ; v2' =",null,null,null,{"$f":"+E2123","v":3.2518659663533688E-4},null,null,"*(",{"$f":"+I2123","v":1.75},null,"+",{"$f":"+S2077","v":2.25},null,")²"," /",2,"+",{"$f":"+Q2123","v":1.5204170286707211E-4},null,null,"*(",{"$f":"+U2123","v":0.875},null,"+",{"$f":"+N2143","v":2.25},null,")²"," /",2,"-",{"$f":"+AC2123","v":6.5160729800173764E-5},null,null,"*",{"$f":"+AA2143","v":2.25},null,"3 /",3,"+","D1","=","D1","+",{"$f":"G2143*(K2143+N2143)^2/R2143+T2143*(X2143+AA2143)^2/AE2143-AG2143*AK2143^3/AN2143","v":3.0964767544032859E-3}]
[null,null,"k = 0 ; v3' =",null,null,null,{"$f":"+E2128","v":6.2122783855149009E-4},null,null,"*",{"$f":"+I2128","v":4},null,"² /",2,"-",{"$f":"+Q2128","v":2.9045643153526973E-4},null,null,"*",{"$f":"+U2128","v":3.125},null,"² /",2,"-",{"$f":"+AC2128","v":5.6016597510373447E-4},null,null,"*",{"$f":"+AG2128","v":1.125},null,"² /",2,"+","E1","=","E1","+",{"$f":"G2144*K2144^2/N2144-P2144*T2144^2/W2144-Y2144*AC2144^2/AF2144","v":3.1970983826857795E-3}]
[null,null,"beş adet denklem beş adet bilinmeyen çözülürse :"]
[null,null,"D2 =",null,-6.9437361927349919E-3,null,null,null,1,-1,0,0,0,{"$f":"-AD2139","v":-4.1900059650462019E-3},null,0.26515151515151514,-0.73484848484848486,1.2859848484848486,0.26515151515151514,0.68939393939393945,-6.9437361927349919E-3]
[null,null,"E / 108 * y =",null,null,null,{"$f":"+E2120","v":3.5817203131796437E-3},null,null,"*","x3"," /",6,"-",{"$f":"+M2120","v":4.7846889952153111E-4},null,null,"*","x4"," /",12,null,"+","C1","*","x","+","C2"]
[null,null,"y = (",null,{"$f":"+G2153","v":3.5817203131796437E-3},null,null,"*",{"$f":"+D2154","v":1.75},null,"3 /",6,"-",{"$f":"+O2153","v":4.7846889952153111E-4},null,null,"*",{"$f":"+I2155","v":1.75},null,"4 /",12,null,"+",{"$f":"+E2147","v":-5.4260477266762815E-3},null,null,"*",{"$f":"+R2155","v":1.75},null,") * 108 /",null,null,{"$f":"+AN2075","v":200000}]
[null,null,"y=",{"$f":"+E2156","v":-3.3351230252275297},null,null,"mm",null,{"$f":"IF(ABS(D2158)<ABS(M2158),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O2157","v":22},null,null,"mm",null,{"$f":"IF(ABS(D2158)<ABS(M2158),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"E / 108 * y =",null,null,null,{"$f":"+E2124","v":3.2518659663533688E-4},null,null,"*(",{"$f":"+I2124","v":1.75},null,"+","z",")3"," /",6,"-",{"$f":"+Q2124","v":1.5204170286707211E-4},null,null,"*(",{"$f":"+U2124","v":0.875},null,"+","z",")3"," /",6,"-",{"$f":"+AC2124","v":6.5160729800173764E-5},null,null,"*","z4"," /",12,null,"+","D1","*","z","+","D2"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"S2079*1000","v":6600},null,null," /",300,null,"=",{"$f":"+H2164/L2164","v":22},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"E / 108 * y =",null,null,null,{"$f":"+E2129","v":6.2122783855149009E-4},null,null,"*(",{"$f":"+I2129","v":4},null,"+","k",")3"," /",6,"-",{"$f":"+Q2129","v":2.9045643153526973E-4},null,null,"*(",{"$f":"+U2129","v":3.125},null,"+","k",")3"," /",6,"-",{"$f":"+AC2129","v":5.6016597510373447E-4},null,null,"*(",{"$f":"+AG2129","v":1.125},null,"+","k",")3"," /",6,"-",{"$f":"+AO2129","v":5.1867219917012447E-5},null,null,"*","k4"," /",12,null,"+","E1","*","k","+","E2"]
[null,null,"y = (",null,{"$f":"+G2167","v":6.2122783855149009E-4},null,null,"*(",{"$f":"+K2167","v":4},null,"+",{"$f":"+D2168","v":0},null,")3"," /",6,"-",{"$f":"+S2167","v":2.9045643153526973E-4},null,null,"*(",{"$f":"+W2167","v":3.125},null,"+",{"$f":"+L2169","v":0},null,")3"," /",6,"-",{"$f":"+AE2167","v":5.6016597510373447E-4},null,null,"*(",{"$f":"+AI2167","v":1.125},null,"+",{"$f":"+Y2169","v":0},null,")3"," /",6,"-",{"$f":"+AQ2167","v":5.1867219917012447E-5},null,null,"*",{"$f":"+AL2169","v":0},null,"4 /",12,null,"+",{"$f":"+E2150","v":-1.3366633899125719E-3},null,null,"*",{"$f":"+AV2169","v":0},null,"+",{"$f":"+E2151","v":-1.2184826195476964E-2},null,null,") * 108 / ",null,null,{"$f":"+BB2162","v":200000}]
[null,null,"y =",null,{"$f":"(E2169*(I2169+L2169)^3/P2169-R2169*(V2169+Y2169)^3/AC2169-AE2169*(AI2169+AL2169)^3/AP2169-AR2169*AV2169^4/AY2169+BB2169*BF2169+BI2169)*100000000/BO2169","v":-3.5843318680727894},null,null,"mm"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"w =",null,30,null,"KN/m",null,null,null,null,null,null,null,"w =",null,20,null,"KN/m",null,null,null,null,null,"IPE 300"]
[null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O2179,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(BB2179,$CG$6:$CG$120,0),0)","v":300}]
[null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(O2179,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(BB2179,$CG$6:$CG$120,0),0)","v":7.1}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O2179,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,"z",null,null,null,null,"B =",null,{"$f":"+E2204","v":71.305327868852459},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(BB2179,$CG$6:$CG$120,0),0)","v":10.7}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A =",null,{"$f":"+E2201","v":89.194672131147541},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AG2190+AR2190","v":6.1},null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uygunluk koşulları"]
[null,null,"MESNET TEPKİLERİ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = 0 ; v1 = 0",null,null,null,null,null,null,null,null,"( x = L ; v1 ) = ( z = 0 ; v2 )",null,null,null,null,null,null,null,null,null,null,null,null,"z = L ; v2 = 0",null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK2224","v":1.1416835277834068}]
[null,null,"A =",null,{"$f":"(H2200*K2200+N2200*Q2200*T2200+W2200*Z2200*AC2200)/E2200","v":89.194672131147541},null,"KN",null,"(sol mesnet tepkisi)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AB2189","v":89.194672131147541},{"$f":"AZ2201-AY2216*AH2179","v":0},null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(AZ2201),ABS(BA2201))","v":89.194672131147541},null,null,"KN",null,"(1.ci bölge için max kesme kuvveti)"]
[null,null,"B =",null,{"$f":"(G2203+J2203*M2203+P2203*S2203-E2201)","v":71.305327868852459},null,"KN",null,"(sağ mesnet tepkisi)"]
[null,null,"x=",1,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D2207<=AG2190,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+AB2189","v":89.194672131147541},null,"*",{"$f":"+D2207","v":1},null,"-",{"$f":"+AH2179","v":30},null,"*",{"$f":"+D2207","v":1},null,"² /",2,"=",{"$f":"+E2208*H2208-K2208*N2208^2/Q2208","v":74.194672131147541},null,null,"KNm"]
[null,null,"2.ci bölgede :"]
[null,null,"Vx =",null,{"$f":"+E2212","v":89.194672131147541},null,"-",{"$f":"+N2212","v":30},null,"*",{"$f":"+Q2212","v":2.35},null,"-",{"$f":"+Z2212","v":15},null,"-",{"$f":"+AF2212","v":20},null,"*",{"$f":"+AI2212","v":1},null,"=",{"$f":"+E2213-H2213*K2213-N2213-Q2213*T2213","v":-16.305327868852459},null,null,"KN"]
[null,null,"L / 2 =",null,{"$f":"+AM2192/2","v":3.05},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AB2189-AH2179*AG2190-AM2178+AT2179*AG2190)/AT2179","v":2.5347336065573769},null,{"$f":"+BW2228","v":140.13496382440871}]
[null,null,"L / 4 =",null,{"$f":"+AM2192/4","v":1.5249999999999999},null,null,"m. ' deki moment miktarı"]
[null,null,"MC =",null,null,{"$f":"+F2220","v":89.194672131147541},null,"*",{"$f":"+F2221","v":4.5749999999999993},null,"-",{"$f":"IF((O2222-R2222)<=0,0,+AM2178)","v":15},null,"*(",{"$f":"+I2222","v":4.5749999999999993},null,"-",{"$f":"+AG2190","v":2.35},null,")-",{"$f":"+AH2179","v":30},null,"*",{"$f":"IF(F2221<AG2190,F2221/2,AG2190)","v":2.35},null,"*(",{"$f":"+F2221","v":4.5749999999999993},null,"-",{"$f":"IF(F2221<AG2190,0,AG2190/2)","v":1.175},null,")-",{"$f":"IF((AJ2222-AM2222)<0,0,AT2179)","v":20},null,"*(",{"$f":"+F2221","v":4.5749999999999993},null,"-",{"$f":"+AG2190","v":2.35},null,")²"," /",2,"=",{"$f":"+F2222*I2222-L2222*(O2222-R2222)-U2222*X2222*(AA2222-AD2222)-AG2222*(AJ2222-AM2222)^2/AQ2222","v":85.484375000000028},null,null,"KNm"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AS2216)","v":125.18910491131416},null,null," /(",2.5,null,"*",{"$f":"+H2224","v":125.18910491131416},null,null,"+",3,"*",{"$f":"ABS(AS2220)","v":101.13749999999999},null,null,"+",4,"*",{"$f":"ABS(AS2218)","v":124.45625000000003},null,null,"+",3,"*",{"$f":"ABS(AS2222)","v":85.484375000000028},null,null,")=",{"$f":"E2224*H2224/(L2224*O2224+S2224*U2224+Y2224*AA2224+AE2224*AG2224)","v":1.1416835277834068}]
[null,null,"v1'' =",null,{"$f":"+E2227/J2227","v":9.6866498839213229E-4},null,null,"*","x","-",{"$f":"+N2227/S2227/U2227","v":1.6290182450043442E-4},null,null,"*","x²",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mmax =",null,null,{"$f":"+F2218","v":89.194672131147541},null,"*",{"$f":"+AH2227","v":2.5347336065573769},null,"-",{"$f":"IF((AS2228-AV2228)<=0,0,+AM2178)","v":15},null,"*(",{"$f":"+AM2228","v":2.5347336065573769},null,"-",{"$f":"+AG2190","v":2.35},null,")-",{"$f":"+AH2179","v":30},null,"*",{"$f":"IF(AH2227<AG2190,AH2227/2,AG2190)","v":2.35},null,"*(",{"$f":"IF(AH2227<AG2190,AH2227,AG2190)","v":2.35},null,"-",{"$f":"IF(AH2227<AG2190,0,AG2190/2)","v":1.175},null,")-",{"$f":"IF((BN2228-BQ2228)<0,0,AT2179)","v":20},null,"*(",{"$f":"+AH2227","v":2.5347336065573769},null,"-",{"$f":"+AG2190","v":2.35},null,")²"," /",2,"=",{"$f":"+AJ2228*AM2228-AP2228*(AS2228-AV2228)-AY2228*BB2228*(BE2228-BH2228)-BK2228*(BN2228-BQ2228)^2/BU2228","v":140.13496382440871},null,null,"KNm"]
[null,null,"v1' =",null,{"$f":"+E2228","v":9.6866498839213229E-4},null,null,"*","x²"," /",2,"-",{"$f":"+K2228","v":1.6290182450043442E-4},null,null,"*","x3"," /",6,"+","C1"]
[null,null,"v2'' =",null,{"$f":"+E2232/M2232","v":1.0669219154443486E-2},null,null,"*(",{"$f":"+H2232","v":2.35},null,"+","z",")-",{"$f":"+Q2232*T2232/AB2232","v":8.4330143540669849E-3},null,null,"*(",{"$f":"+W2232","v":1.175},null,"+","z",")-",{"$f":"+AF2232/AK2232","v":1.7942583732057417E-3},null,null,"*","z","-",{"$f":"+AO2232/AT2232/AV2232","v":1.1961722488038277E-3},null,null,"*","z²"]
[null,null,"v2' =",null,{"$f":"+E2233","v":1.0669219154443486E-2},null,null,"*(",{"$f":"+H2232","v":2.35},null,"+","z",")²"," /",2,"-",{"$f":"+N2233","v":8.4330143540669849E-3},null,null,"*(",{"$f":"+W2232","v":1.175},null,"+","z",")²"," /",2,"-",{"$f":"+W2233","v":1.7942583732057417E-3},null,null,"*","z²"," /",2,"-",{"$f":"+AC2233","v":1.1961722488038277E-3},null,null,"*","z3"," /",6,"+","D1"]
[null,null,"z = L ; v2 = 0",null,null,null,null,null,{"$f":"+E2235","v":1.0669219154443486E-2},null,null,"*(",{"$f":"+I2235","v":2.35},null,"+",{"$f":"+AR2190","v":3.75},null,")3"," /",6,"-",{"$f":"+Q2235","v":8.4330143540669849E-3},null,null,"*(",{"$f":"+U2235","v":1.175},null,"+",{"$f":"+P2238","v":3.75},null,")3"," /",6,"-",{"$f":"+AC2235","v":1.7942583732057417E-3},null,null,"*",{"$f":"+AC2238","v":3.75},null,"3 /",6,"-",{"$f":"+AK2235","v":1.1961722488038277E-3},null,null,"*",{"$f":"+AM2238","v":3.75},null,"4 /",24,null,"+","D1","*",{"$f":"+AV2238","v":3.75},null,"+","D2",null,null,"D1","*",{"$f":"+BD2238","v":3.75},null,"+","D2","+",{"$f":"I2238*(M2238+P2238)^3/T2238-V2238*(Z2238+AC2238)^3/AG2238-AI2238*AM2238^3/AP2238-AR2238*AV2238^4/AY2238","v":0.21009248981384562},null,null,"=",0,null,"(1.ci denklem)"]
[null,null,"z = 0 ; v2' =",null,null,null,{"$f":"+E2234","v":1.0669219154443486E-2},null,null,"*",{"$f":"+I2234","v":2.35},null,"² /",2,"-",{"$f":"+Q2234","v":8.4330143540669849E-3},null,null,"*",{"$f":"+U2234","v":1.175},null,"² /",2,"+","D1",null,null,"D1","+",{"$f":"G2240*K2240^2/N2240-P2240*T2240^2/W2240","v":2.3638966168915216E-2}]
[null,null,"z = 0 ; v2 =",null,null,null,{"$f":"+E2235","v":1.0669219154443486E-2},null,null,"*",{"$f":"+I2235","v":2.35},null,"3/",6,"-",{"$f":"+Q2235","v":8.4330143540669849E-3},null,null,"*",{"$f":"+U2235","v":1.175},null,"3/",6,"+","D2",null,null,"D2","+",{"$f":"G2243*K2243^3/N2243-P2243*T2243^3/W2243","v":2.0797244460656231E-2}]
[null,null,"D1 =",null,{"$f":"+Q2247","v":-3.9553677717887835E-2},null,null,null,1,-1,0,{"$f":"-AD2241","v":2.1316593222323869E-2},null,0.16393442622950821,-0.38524590163934425,0.16393442622950821,-3.9553677717887835E-2]
[null,null,"1.ci bölgede :"]
[null,null,"E / 108 * y =",null,null,null,{"$f":"+E2230","v":9.6866498839213229E-4},null,null,"*","x3"," /",6,"-",{"$f":"+M2230","v":1.6290182450043442E-4},null,null,"*","x4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"y = (",null,{"$f":"+E2251","v":9.6866498839213229E-4},null,null,"*",{"$f":"+D2252","v":2.35},null,"3/",6,"-",{"$f":"+M2251","v":1.6290182450043442E-4},null,null,"*",{"$f":"+I2253","v":2.35},null,"4 /",24,null,"+",{"$f":"+E2246","v":-1.8237084495563959E-2},null,null,"*",{"$f":"+R2253","v":2.35},null,")* 108 / ",null,null,{"$f":"+F2194","v":200000}]
[null,null,"y=",{"$f":"+E2254","v":-20.484476955554996},null,null,"mm",null,{"$f":"IF(ABS(D2256)<ABS(M2256),\"<\",\">\")","v":">"},"ymax =",null,null,{"$f":"+O2255","v":20.333333333333332},null,null,"mm",null,{"$f":"IF(ABS(D2256)<ABS(M2256),\"uygun.\",\"uygun değil.\")","v":"uygun değil."}]
[null,null,"y = (",null,{"$f":"+G2258","v":1.0669219154443486E-2},null,null,"*(",{"$f":"+K2258","v":2.35},null,"+","z",")3"," /",6,"-",{"$f":"+S2258","v":8.4330143540669849E-3},null,null,"*(",{"$f":"+W2258","v":1.175},null,"+","z",")3"," /",6,"-",{"$f":"+AE2258","v":1.7942583732057417E-3},null,null,"*","z3"," /",6,"-",{"$f":"+AM2258","v":1.1961722488038277E-3},null,null,"*","z4"," /",24,null,"+",{"$f":"+E2247","v":-3.9553677717887835E-2},null,null,"*","z","+",{"$f":"+E2248","v":-6.176619837176623E-2},null,null,") * 108 / E "]
[null,null,"y =",null,{"$f":"(E2261*(I2261+L2261)^3/P2261-R2261*(V2261+Y2261)^3/AC2261-AE2261*AI2261^3/AL2261-AN2261*AR2261^4/AU2261+AX2261*BB2261+BE2261)*100000000/BK2261","v":-20.484476955554996},null,null,"mm"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,"A",null,null,null,null,null,null,null,null,15,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,"D"]
[]
[null,null,null,null,null,null,null,null,null,null,null,"I1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"üstteki kiriş enkesiti",null,null,null,null,null,null,null,null,null,null,null,null,"alttaki kiriş enkesiti"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(V2281,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(W2270,$CG$6:$CG$120,0),0)","v":7.1}]
[null,null,null,null,null,null,null,{"$f":"+M2292/2","v":3},null,"m"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,6,null,"m",null,null,null,null,null,{"$f":"+M2292/2","v":3},null,"m"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,"m"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,"(1.ci bölge)",null,null,null,null,null,null,null,null,null,"(2.ci bölge)"]
[null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,"z"]
[null,null,null,null,"A=",{"$f":"+W2375","v":50.233485569194499},null,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+E2376","v":50.233485569194499},null,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+M2292","v":6},null,"m"]
[null,null,"B mesnetinde moment sıfır şartından"]
[null,null,"1.ci bölge için"]
[null,null,"v1 = (",null,{"$f":"+E2325","v":45},null,"-","P","*",{"$f":"+J2325","v":0.5},null,")*","x3"," /",6,"-",{"$f":"+Q2325","v":15},null,"*","x4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"v2' = (",null,{"$f":"+E2328","v":45},null,"-","P","*",{"$f":"+J2328","v":0.5},null,")*(",{"$f":"+M2328","v":3},null,"+","z",")²"," /",2,"-",{"$f":"+R2328*U2328","v":45},null,"*(",{"$f":"+X2328","v":1.5},null,"+","z",")²"," /",2,"-",{"$f":"+AC2328","v":15},null,"*","z3"," /",6,"+","P","*","z²"," /",2,"+","D1"]
[null,null,"x = 0 ; v1 = 0",null,null,null,null,null,"C2 = 0"]
[null,null,"x = L ; v1 = (",null,null,null,{"$f":"+E2326","v":45},null,"-","P","*",{"$f":"+J2326","v":0.5},null,")*",{"$f":"+K2315","v":3},null,"3 /",6,"-",{"$f":"+Q2326","v":15},null,"*",{"$f":"+O2335","v":3},null,"4/",24,null,"+","C1","*",{"$f":"+W2335","v":3},null,"=","C1","*",{"$f":"+AE2335","v":3},null,"+","P","*",{"$f":"-L2335*O2335^3/R2335","v":-2.25},null,null,"+",{"$f":"G2335*O2335^3/R2335-T2335*W2335^4/Z2335","v":151.875}]
[null,null,"z = 0 ; v2 = (",null,null,null,{"$f":"+E2330","v":45},null,"-","P","*",{"$f":"+J2330","v":0.5},null,")*",{"$f":"+M2330","v":3},null,"3 /",6,"-",{"$f":"+U2330","v":45},null,"*",{"$f":"+X2330","v":1.5},null,"3 /",6,"+","D2","=","D2","+","P","*",{"$f":"-L2336*O2336^3/R2336","v":-2.25},null,null,"+",{"$f":"G2336*O2336^3/R2336-T2336*W2336^3/Z2336","v":177.1875}]
[null,null,"x = L ; v1' = (",null,null,null,{"$f":"+E2325","v":45},null,"-","P","*",{"$f":"+J2325","v":0.5},null,")*",{"$f":"+K2315","v":3},null,"² /",2,"-",{"$f":"+Q2325","v":15},null,"*",{"$f":"+O2338","v":3},null,"3 /",6,"+","C1","=","C1","+","P","*",{"$f":"-L2338*O2338^2/R2338","v":-2.25},null,null,"+",{"$f":"G2338*O2338^2/R2338-T2338*W2338^3/Z2338","v":135}]
[null,null,"( E * I1 ) * y = (",null,null,null,null,null,{"$f":"+E2326","v":45},null,"-","P","*",{"$f":"+J2326","v":0.5},null,")*",{"$f":"+K2315","v":3},null,"3 /",6,"-",{"$f":"+Q2326","v":15},null,"*",{"$f":"+Q2342","v":3},null,"4 /",24,null,"+","C1","*",{"$f":"+Y2342","v":3},null,"=","C1","*",{"$f":"+AG2342","v":3},null,"-","P","*",{"$f":"N2342*Q2342^3/T2342","v":2.25},null,"+",{"$f":"+I2342*Q2342^3/T2342-V2342*Y2342^4/AB2342","v":151.875}]
[]
[null,null,null,null,null,"C",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D"]
[]
[null,null,null,null,"C=",{"$f":"+O2377","v":5.2334855691944977},null,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D=",{"$f":"+E2378","v":5.2334855691944977},null,null,"KN"]
[]
[null,null,"y2 = P * L3 / ( 48 * E * I2 ) =",null,null,null,null,null,null,null,"P","*",{"$f":"+P2355","v":5},null,"3/(",48,null,"*","E","*","I2",")=",{"$f":"+M2357^3/P2357","v":2.6041666666666665},null,"*","P"," /(","E","*","I2",")",null,"(E noktasındaki sehim)"]
[null,null,"C1","*",{"$f":"+L2360","v":3},null," /","I1","-","P","*",{"$f":"+S2360","v":2.25},null," /","I1","+",{"$f":"+X2360","v":151.875},null,null," /","I1","-",{"$f":"+C2360","v":2.6041666666666665},null,"*","P"," /","I2","=",0]
[null,null,"C1","*",{"$f":"+E2362","v":3.2580364900086882E-9},null,null,"-","P","*",{"$f":"+K2362+S2362","v":3.359384634677286E-8},null,null,"+",{"$f":"+O2362","v":1.6493809730668982E-7},null,null,"=",0,null,"(4.cü denklem)"]
[null,null,"D1 =",null,{"$f":"+S2366","v":-175.42568506137528},null,null,null,{"$f":"+AQ2337","v":3},0,-1,0,{"$f":"-AV2337","v":25.3125},null,0.21318653839283999,0.21318653839283996,-0.36044038482147994,-85670995.770920753,-175.42568506137528]
[null,null,"P =",null,-10.466971138388995,null,null,null,{"$f":"+E2363","v":3.2580364900086882E-9},0,0,{"$f":"-K2363","v":-3.359384634677286E-8},{"$f":"-O2363","v":-1.6493809730668982E-7},null,2.0675498544965917E-2,2.0675498544965917E-2,6.2026495634897753E-2,-38075998.120409228,-10.466971138388995]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"P2355*1000","v":5000},null,null," /",300,null,"=",{"$f":"+H2372/L2372","v":16.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"A","=",{"$f":"+P2322","v":45},null,"-","P","*",{"$f":"+U2322","v":0.5},null,"=",{"$f":"+E2375","v":45},null,"-",{"$f":"+E2368","v":-10.466971138388995},null,null,"*",{"$f":"+J2375","v":0.5},null,"=",{"$f":"+M2375-P2375*T2375","v":50.233485569194499},null,null,"KN"]
[null,null,"C","=","P"," /",2,"=",{"$f":"-E2368","v":10.466971138388995},null,null," /",2,"=",{"$f":"+I2377/M2377","v":5.2334855691944977},null,null,"KN"]
[null,null,"D","=",{"$f":"+O2377","v":5.2334855691944977},null,null,"KN"]
[null,"YAYILI & TEKİL YÜKLÜ BİNDİRMELİ ÇELİK BASİT KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"üstteki kiriş",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(Y2392,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(AA2404,$CG$6:$CG$120,0),0)","v":7.1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,null,"KN"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(Y2392,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(AA2404,$CG$6:$CG$120,0),0)","v":150}]
[null,null,null,null,null,null,null,null,null,{"$f":"+J2394/2","v":1.5},null,"m"]
[]
[]
[null,null,null,null,null,null,null,"A"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AH2394","v":15},null,"KN/m"]
[]
[]
[null,null,null,null,null,null,null,null,null,"(1.ci bölge)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(2.ci bölge)"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+W2401","v":1},null,"m",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AK2401","v":1.5},null,"m"]
[null,null,null,"D noktasına göre moment sıfır şartından"]
[null,null,null,"P","=",{"$f":"-I2429/F2429","v":46.875},null,null,"KN"]
[null,null,null,"P","+",{"$f":"+X2415","v":15},null,"*",{"$f":"+M2425+AA2425","v":2.5},null,"+",{"$f":"+AH2414","v":25},null,"-","D","=",0]
[null,null,null,"v1'' =",null,{"$f":"-F2414","v":-46.875},null,null,"*","x","-",{"$f":"+X2415","v":15},null,"*","x²"," /",2]
[null,null,null,"2.ci bölge için"]
[null,null,null,"v2' =",null,{"$f":"+F2440","v":-46.875},null,null,"*(",{"$f":"+J2440","v":1},null,"+","z",")²"," /",2,"-",{"$f":"+O2440*R2440","v":15},null,"*(",{"$f":"+U2440","v":0.5},null,"+","z",")²"," /",2,"-",{"$f":"+Z2440","v":15},null,"*","z3"," /",6,"+",{"$f":"+AG2440","v":109.375},null,null,"*","z²"," /",2,"+","D1"]
[null,null,null,"v2 =",null,{"$f":"+F2441","v":-46.875},null,null,"*(",{"$f":"+J2441","v":1},null,"+","z",")3"," /",6,"-",{"$f":"+R2441","v":15},null,"*(",{"$f":"+U2441","v":0.5},null,"+","z",")3"," /",6,"-",{"$f":"+AC2441","v":15},null,"*","z4"," /",24,null,"+",{"$f":"+AJ2441","v":109.375},null,null,"*","z3"," /",6,"+","D1","*","z","+","D2"]
[null,null,null,"x = L ; v1' =",null,null,null,{"$f":"+F2437","v":-46.875},null,null,"*",{"$f":"+M2425","v":1},null,"² /",2,"-",{"$f":"+N2437","v":15},null,"*",{"$f":"+L2446","v":1},null,"3 /",6,"+","C1","=","C1","+",{"$f":"H2446*L2446^2/O2446-Q2446*T2446^3/W2446","v":-25.9375}]
[null,null,null,"( x = L ; v1' ) = ( z = 0 ; v2' )",null,null,null,null,null,null,null,null,null,"C1","+",{"$f":"+AC2446","v":-25.9375},null,null,"=","D1","+",{"$f":"+AD2447","v":-25.3125},null,null,null,null,"C1","-","D1","+",{"$f":"+P2448-V2448","v":-0.625},null,null,"=",0,null,"(2.ci denklem)"]
[null,null,null,"y = C2 / ( E * I1 )"]
[null,null,null,"C2","=",{"$f":"+I2454","v":26.3671875},null,null,"*","I1"," /","I2","=",{"$f":"+F2455","v":26.3671875},null,null,"*",{"$f":"+BN2399","v":8360},null,null," /",{"$f":"+AZ2399","v":92080},null,null,"=",{"$f":"+N2455*R2455/V2455","v":2.39389321785404}]
[null,null,null,"C1","=",{"$f":"(-AS2444-F2456)/AN2444","v":6.04360678214596}]
[null,null,null,"E noktasındaki (konsol ucu) sehim"]
[null,null,null,"y = (",null,{"$f":"+F2442","v":-46.875},null,null,"*(",{"$f":"+J2442","v":1},null,"+",{"$f":"+AA2425","v":1.5},null,")3"," /",6,"-",{"$f":"+R2442","v":15},null,null,"*(",{"$f":"+U2442","v":0.5},null,"+",{"$f":"+M2461","v":1.5},null,")3"," /",6,"-",{"$f":"+AC2442","v":15},null,"*",{"$f":"+Z2461","v":1.5},null,"4/",24,null,"+",{"$f":"+AK2442","v":109.375},null,null,"*",{"$f":"+AI2461","v":1.5},null,"3 /"," /",6,"+",{"$f":"+F2458","v":5.41860678214596},null,null,"*",{"$f":"+AS2461","v":1.5},null,"+",{"$f":"+AI2445","v":8.125},null,null,")*108 / (",null,null,{"$f":"+AF2386","v":200000},null,null,"*",{"$f":"+BN2399","v":8360},null,null,")"]
[null,null,null,"y =",null,{"$f":"+F2462","v":-4.0345710123672882},null,null,"mm",null,{"$f":"IF(ABS(F2464)<ABS(O2464),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+P2463","v":10},null,null,"mm",null,{"$f":"IF(ABS(F2464)<ABS(O2464),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,null,null,null,null,"A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"P =",null,{"$f":"F2430","v":46.875},null,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"+J2400","v":1.5},null,"m",null,null,null,null,null,null,null,{"$f":"+Q2389","v":1.5},null,"m"]
[]
[null,null,null,"y2 =",null,{"$f":"L2478*P2478^3/(T2478*W2478*AA2478*AE2478)","v":0.14317543168983493},null,null,"mm"]
[null,null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"Q2475*1000","v":3000},null,null," /",300,null,"=",{"$f":"+I2480/M2480","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"I1",null,null,null,null,null,null,null,null,"I1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,"z",null,null,"B=",{"$f":"+G2562","v":102.54882819297963},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+N2497","v":3.75},null,"m",null,null,null,null,null,null,null,{"$f":"+U2503","v":2.25},null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AH2506/2","v":2.25},null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kirişlerin elastisite modülü)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.5,null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AH2506/2","v":2.25},null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(Q2488,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(N2508,$CG$6:$CG$120,0),0)","v":10.7}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(Q2488,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(N2508,$CG$6:$CG$120,0),0)","v":150}]
[null,null,null,null,"v1' =",null,"Ma *",null,"x","+","A","*","x²"," /",2,"-",{"$f":"+M2518","v":2.5},null,"*","x3"," /",6,"+","C1"]
[null,null,null,null,"2.ci bölge için"]
[null,null,null,null,"v2'' =",null,"Ma +",null,"A","*(",{"$f":"+BD2496","v":3.75},null,"+","z",")-",{"$f":"+BC2487","v":2.5},null,"*",{"$f":"+BD2496","v":3.75},null,"*(",{"$f":"+BD2496/2","v":1.875},null,"+","z",")-",{"$f":"+BJ2486","v":150},null,"*","z"]
[null,null,null,null,"sınır ve uygunluk şartları :"]
[null,null,null,null,"x = L ; v1 =",null,null,null,"Ma *",null,{"$f":"+BD2496","v":3.75},null,"² /",2,"+","A","*",{"$f":"+K2528","v":3.75},null,"3 /",6,"-",{"$f":"+S2520","v":2.5},null,"*",{"$f":"+R2528","v":3.75},null,"4 /",24,null,"=","Ma *",null,{"$f":"K2528^2/N2528","v":7.03125},null,"+","A","*",{"$f":"+R2528^3/U2528","v":8.7890625},null,"-",{"$f":"W2528*Z2528^4/AC2528","v":20.599365234375}]
[null,null,null,null,"x = L ; v1' =",null,null,null,"Ma *",null,{"$f":"+BD2496","v":3.75},null,"+","A","*",{"$f":"+K2531","v":3.75},null,"² /",2,"-",{"$f":"+Q2519","v":2.5},null,"*",{"$f":"+P2531","v":3.75},null,"3 /",6,"=","Ma *",null,{"$f":"+K2531","v":3.75},null,"+","A","*",{"$f":"P2531^2/S2531","v":7.03125},null,"-",{"$f":"U2531*X2531^3/AA2531","v":21.97265625}]
[null,null,null,null,"düşey denge denkleminden"]
[null,null,null,null,"z = L ; v2'' = 0",null,null,null,null,null,null,"Ma +",null,"A","*(",{"$f":"+K2522","v":3.75},null,"+",{"$f":"+BN2496","v":2.25},null,")-",{"$f":"+P2522","v":2.5},null,"*",{"$f":"+S2522","v":3.75},null,"*(",{"$f":"+V2522","v":1.875},null,"+",{"$f":"+BN2496","v":2.25},null,")-",{"$f":"+AA2522","v":150},null,"*",{"$f":"+BN2496","v":2.25},null,"=",0,null,null,"Ma +",null,"A","*",{"$f":"+P2537+S2537","v":6},null,"-",{"$f":"+V2537*Y2537*(AB2537+AE2537)+AH2537*AK2537","v":376.171875},null,null,"=",0,null,"(4.cü denklem)"]
[null,null,null,null,"y1 = (",null,"Ma *",null,{"$f":"+L2539^2/O2539","v":2.53125},null,"+","A","*",{"$f":"(S2539+V2539)^3/Z2539","v":36},null,"+","D1","*",{"$f":"+AX2539","v":2.25},null,"+","D2","-",{"$f":"AB2539*(AE2539+AH2539)^3/AL2539+AN2539*AQ2539^3/AT2539","v":394.4366455078125},null,null,")/(","E","*","I1",")"]
[]
[null,null,null,null,null,null,null,"C",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D"]
[]
[null,null,null,null,null,null,"C=",{"$f":"+R2541/2","v":51.274414096489814},null,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D=",{"$f":"+R2541/2","v":51.274414096489814},null,null,"KN"]
[]
[null,null,null,null,"y1 = y2 (iki kirişin çökmeleri eşitliği prensibinden)"]
[null,null,null,null,"beş adet denklem beş adet bilinmeyen çözülürse :"]
[null,null,null,null,"Ma =",null,{"$f":"+W2560","v":1.4648441578777001},null,null,{"$f":"+AQ2530","v":7.03125},0,0,0,-1,{"$f":"+AV2530","v":10.2996826171875},null,null,{"$f":"MINVERSE(J2560:N2564)","v":0.14222222192210385},3.1999999932473364E-9,2.9738755918106308E-8,-1.3489792635010615E-8,1.3095822194587321,{"$f":"MMULT(R2560:V2564,O2560:O2564)","v":1.4648441578777001}]
[null,null,null,null,"D2 =",null,2.8678900772246412E-6,null,null,{"$f":"+G2558","v":2.7489682884448305E-9},{"$f":"+M2558","v":3.9096437880104255E-8},{"$f":"-S2558","v":-2.2708582535885169E-8},{"$f":"+Y2558","v":2.443527367506516E-9},{"$f":"+AE2558","v":0.10860121633362294},{"$f":"+AI2558","v":4.2836299468702489E-7},null,null,-2.1102073320701504E-9,2.2499999952520335E-8,2.0910062754918497E-7,-9.4850104464918384E-8,9.2079999805692108,2.8678900772246412E-6]
[null,null,null,null,"( C-D kirişi ) Alttaki kirişin B noktasındaki sehim"]
[null,null,null,null,"y2 =",null,{"$f":"+G2567","v":11.643692644892928},null,null,"mm",null,{"$f":"IF(ABS(G2569)<ABS(P2569),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+Q2568","v":15},null,null,"mm",null,{"$f":"IF(ABS(G2569)<ABS(P2569),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,null,null,"( A-B kirişi ) üstteki kirişin sehimi"]
[null,null,null,null,"y =",null,{"$f":"(G2573*K2573^2/N2573+P2573*T2573^3/W2573-Y2573*AB2573^4/AE2573)*100000000/(AJ2573*AN2573)","v":2.9245632735710392},null,null,"mm"]
[null,null,null,null,"y=",{"$f":"+G2574","v":2.9245632735710392},null,null,"mm",null,{"$f":"IF(ABS(F2576)<ABS(O2576),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+Q2575","v":20},null,null,"mm",null,{"$f":"IF(ABS(F2576)<ABS(O2576),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,null,null,"y = (",null,{"$f":"+G2560","v":1.4648441578777001},null,null,"*",{"$f":"+F2579","v":0},null,"² /",2,"+",{"$f":"+G2561","v":62.45117180702038},null,null,"*(",{"$f":"+O2578","v":3.75},null,"+",{"$f":"+K2580","v":0},null,")3"," /",6,"-",{"$f":"+W2578","v":9.375},null,"*(",{"$f":"+Z2578","v":1.875},null,"+",{"$f":"+W2580","v":0},null,")3"," /",6,"+",{"$f":"+AH2578","v":150},null,"*",{"$f":"+AI2580","v":0},null,"3 /",6,"+",{"$f":"+G2563","v":1.5295413738195014E-6},null,null,"*",{"$f":"+AR2580","v":0},null,"+",{"$f":"+G2564","v":2.8678900772246412E-6},null,null,")* 108 / (",null,null,{"$f":"+AJ2573","v":200000},null,null,"*",{"$f":"+AN2573","v":92080},null,null,")"]
[null,null,null,null,"y=",{"$f":"+G2581","v":2.9245632735710392},null,null,"mm",null,{"$f":"IF(ABS(F2583)<ABS(O2583),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+Q2582","v":20},null,null,"mm",null,{"$f":"IF(ABS(F2583)<ABS(O2583),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[null,"YAYILI & TEKİL YÜKLÜ BİNDİRMELİ ÇELİK BASİT KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,"üstteki kiriş",null,null,null,null,null,null,null,null,null,null,null,null,null,"D",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+N2593","v":2.5},null,"KN/m"]
[null,null,null,null,null,"I1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ma =",null,{"$f":"+G2664","v":1.4648468187449191},null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"z"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+I2600","v":3.75},null,"m",null,null,null,null,null,null,null,{"$f":"+Q2606","v":2.25},null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B"]
[null,null,null,null,null,null,null,null,{"$f":"+I2600+Q2606","v":6},null,"m"]
[null,null,null,"alttaki kiriş",null,null,null,null,null,null,null,null,null,null,null,null,2.25,null,"m"]
[null,null,null,"IPE 300"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(K2590,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(D2607,$CG$6:$CG$120,0),0)","v":300}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AC2609/2","v":2.25},null,"m"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"I1 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(K2590,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,null,null,null,null,null,"I2 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(D2607,$CG$6:$CG$120,0),0)","v":8360},null,null,null,"cm4"]
[null,null,null,null,"v1'' =",null,"Ma +",null,"A","*","x","-",{"$f":"+BC2589","v":2.5},null,"*","x²"," /",2]
[null,null,null,null,"2.ci bölge için"]
[null,null,null,null,"v2 =",null,"Ma *",null,"z²"," /",2,"+","A","*(",{"$f":"+M2627","v":3.75},null,"+","z",")3"," /",6,"-",{"$f":"+U2627","v":9.375},null,"*(",{"$f":"+X2627","v":1.875},null,"+","z",")3"," /",6,"+","D1","*","z","+","D2"]
[null,null,null,null,"sınır ve uygunluk şartları :"]
[null,null,null,null,"x = 0 ; v1' = 0",null,null,null,null,null,"C1 = 0"]
[null,null,null,null,"x = L ; v1' =",null,null,null,"Ma *",null,{"$f":"+BD2598","v":3.75},null,"+","A","*",{"$f":"+K2635","v":3.75},null,"² /",2,"-",{"$f":"+Q2623","v":2.5},null,"*",{"$f":"+P2635","v":3.75},null,"3 /",6,"=","Ma *",null,{"$f":"+K2635","v":3.75},null,"+","A","*",{"$f":"P2635^2/S2635","v":7.03125},null,"-",{"$f":"U2635*X2635^3/AA2635","v":21.97265625}]
[null,null,null,null,"düşey denge denkleminden"]
[null,null,null,null,"sağ uçta moment sıfır şartından"]
[null,null,null,null,"y1 = (",null,"Ma *",null,{"$f":"+L2643^2/O2643","v":2.53125},null,"+","A","*",{"$f":"(S2643+V2643)^3/Z2643","v":36},null,"+","D1","*",{"$f":"+AP2643","v":2.25},null,"+","D2","-",{"$f":"AB2643*(AE2643+AH2643)^3/AL2643","v":109.6710205078125},null,null,")/(","E","*","I1",")"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B =",null,{"$f":"+G2666","v":108.79882863645746},null,null,"KN"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+R2656/2","v":2.25},null,"m",null,null,null,null,null,null,null,{"$f":"+R2656/2","v":2.25},null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AC2609","v":4.5},null,"m"]
[null,null,null,null,"y1 = y2 (iki kirişin çökmeleri eşitliği prensibinden)"]
[null,null,null,null,"Ma *",null,{"$f":"+H2660/(BA2619*10000)","v":2.7489682884448305E-9},null,null,"+","A","*",{"$f":"+M2660/(BA2619*10000)","v":3.9096437880104255E-8},null,null,"+","D1","*",{"$f":"+R2660/(BA2619*10000)","v":2.443527367506516E-9},null,null,"+","D2","*",{"$f":"1/(BA2619/10000)","v":0.10860121633362294},null,null,"-",{"$f":"+W2660/(BA2619*10000)","v":1.1910406223698143E-7},null,null,"=","B","*",{"$f":"+AE2660/(BO2619*10000)","v":2.2708582535885169E-8}]
[null,null,null,null,"A =",null,{"$f":"+W2665","v":6.2011713635425139},null,null,{"$f":"+AQ2637","v":3.75},0,0,-1,0,{"$f":"+AV2637","v":5.4931640625},null,null,-2.3703703653683975E-2,-5.333333322078894E-10,-4.9564593196843846E-9,0.16666666891496543,-0.21826370324312203,6.2011713635425139]
[null,null,null,null,"D2 =",null,2.1577112712684496E-5,null,null,{"$f":"+G2662","v":2.7489682884448305E-9},{"$f":"+M2662","v":3.9096437880104255E-8},{"$f":"-S2662","v":-2.2708582535885169E-8},{"$f":"+Y2662","v":2.443527367506516E-9},{"$f":"+AE2662","v":0.10860121633362294},{"$f":"+AI2662","v":1.1910406223698143E-7},null,null,-2.1102073320701504E-9,2.2499999952520335E-8,2.0910062754918497E-7,-9.4850104464918384E-8,9.2079999805692108,2.1577112712684496E-5]
[null,null,null,null,"y2 = P * L3 / ( 48 * E * I2 ) =",null,null,null,null,null,null,null,{"$f":"+R2645*1000","v":108798.82863645746},null,null,"*",{"$f":"+R2656*1000","v":4500},null,null,"3/(",48,null,"*",{"$f":"+BA2603","v":200000},null,null,"*",{"$f":"+BO2619","v":8360},null,null,"*",10000,null,null,")"]
[null,null,null,null,"y2 =",null,{"$f":"M2670*Q2670^3/(U2670*X2670*AB2670*AF2670)","v":12.353335899493105},null,null,"mm"]
[null,null,null,null,"( A-B kirişi ) üstteki kirişin sehimi"]
[null,null,null,null,"y = (",null,{"$f":"+G2664","v":1.4648468187449191},null,null,"*",{"$f":"+F2676","v":3.75},null,"² /",2,"+",{"$f":"+G2665","v":6.2011713635425139},null,null,"*",{"$f":"+K2677","v":3.75},null,"3 /",6,"-",{"$f":"+S2675","v":2.5},null,"*",{"$f":"+T2677","v":3.75},null,"4 /",24,null,")* 108 / (",null,null,{"$f":"+BA2603","v":200000},null,null,"*",{"$f":"+BA2619","v":92080},null,null,")"]
[null,null,null,null,"y=",{"$f":"+G2678","v":0.24002400981380637},null,null,"mm",null,{"$f":"IF(ABS(F2680)<ABS(O2680),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+Q2679","v":20},null,null,"mm",null,{"$f":"IF(ABS(F2680)<ABS(O2680),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,null,null,"y = (",null,{"$f":"+G2664","v":1.4648468187449191},null,null,"*",{"$f":"+F2683","v":2.25},null,"² /",2,"+",{"$f":"+G2665","v":6.2011713635425139},null,null,"*(",{"$f":"+O2682","v":3.75},null,"+",{"$f":"+K2684","v":2.25},null,")3"," /",6,"-",{"$f":"+W2682","v":9.375},null,"*(",{"$f":"+Z2682","v":1.875},null,"+",{"$f":"+W2684","v":2.25},null,")3"," /",6,"+",{"$f":"+G2667","v":1.1507793446064756E-5},null,null,"*",{"$f":"+AI2684","v":2.25},null,"+",{"$f":"+G2668","v":2.1577112712684496E-5},null,null,")* 108 / (",null,null,{"$f":"+AJ2677","v":200000},null,null,"*",{"$f":"+AN2677","v":92080},null,null,")"]
[null,null,null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"+I2604*1000","v":6000},null,null," /",150,null,"=",{"$f":"+J2686/N2686","v":40},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[]
[null,"YAYILI & TEKİL YÜKLÜ BİNDİRMELİ ÇELİK KONSOL KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,"KN",null,null,null,null,null,6,null,"KN"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"D",null,null,null,null,null,null,null,null,null,null,null,"E","I2"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.5,null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+T2694","v":15},null,"KN/m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"üstteki kiriş enkesiti",null,null,null,null,null,null,null,null,null,null,null,null,"alttaki kiriş enkesiti"]
[null,null,null,null,null,null,"Ma =",null,{"$f":"+E2754","v":74.913307807329574},null,null,"KNm",null,"A",null,null,null,null,null,null,null,null,null,null,null,"C",null,null,null,null,null,null,null,"B"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+E2756","v":3.8229846843977349},null,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(O2692,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(Q2701,$CG$6:$CG$120,0),0)","v":300}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"X=",{"$f":"+Y2714","v":3.8229846843977349},null,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O2692,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(Q2701,$CG$6:$CG$120,0),0)","v":10.7}]
[]
[null,null,"SEHİM HESABI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+T2716","v":1.6666666666666667},null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"I1 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(O2692,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,null,null,null,null,null,"I2 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(Q2701,$CG$6:$CG$120,0),0)","v":8360},null,null,null,"cm4"]
[null,null,"v1'' =",null,"Ma +",null,"A","*","x","-",{"$f":"+T2716","v":1.6666666666666667},null,"*","x²"," /",2]
[null,null,"v2'' =",null,"Ma +",null,"A","*(",{"$f":"+T2716","v":1.6666666666666667},null,"+","z",")-",{"$f":"+T2708","v":15},null,"*",{"$f":"+T2716","v":1.6666666666666667},null,"*(",{"$f":"+T2716/2","v":0.83333333333333337},null,"+","z",")-",{"$f":"+Y2707","v":4},null,"*","z","+","X","*","z","-",{"$f":"+T2708","v":15},null,"*","z²"," /",2]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"x = 0 ; v1' = 0",null,null,null,null,null,"C1 = 0"]
[null,null,"x = L ; v1 =",null,null,null,"Ma *",null,{"$f":"+T2716","v":1.6666666666666667},null,"² /",2,"+","A","*",{"$f":"+I2735","v":1.6666666666666667},null,"3 /",6,"-",{"$f":"+Q2727","v":1.6666666666666667},null,"*",{"$f":"+P2735","v":1.6666666666666667},null,"4 /",24,null,"=","Ma *",null,{"$f":"I2735^2/L2735","v":1.3888888888888891},null,"+","A","*",{"$f":"+P2735^3/S2735","v":0.77160493827160515},null,"-",{"$f":"U2735*X2735^4/AA2735","v":0.53583676268861469}]
[null,null,"z = 0 ; v2' =",null,null,null,"A","*",{"$f":"+K2730","v":1.6666666666666667},null,"² /",2,"-",{"$f":"+S2730","v":25},null,"*",{"$f":"+V2730","v":0.83333333333333337},null,"² /",2,"+","D1","=","A","*",{"$f":"+I2739^2/L2739","v":1.3888888888888891},null,"+","D1","-",{"$f":"+N2739*Q2739^2/T2739","v":8.6805555555555571}]
[null,null,"düşey denge denkleminden"]
[null,null,"z = L ; v2'' = 0",null,null,null,null,null,null,"Ma +",null,"A","*(",{"$f":"+I2729","v":1.6666666666666667},null,"+",{"$f":"+AC2716","v":0.83333333333333326},null,")-",{"$f":"+N2729","v":15},null,"*",{"$f":"+Q2729","v":1.6666666666666667},null,"*(",{"$f":"+T2729","v":0.83333333333333337},null,"+",{"$f":"+Q2744","v":0.83333333333333326},null,")-",{"$f":"+Y2729","v":4},null,"*",{"$f":"+AC2744","v":0.83333333333333326},null,"+","X","*",{"$f":"+AI2744","v":0.83333333333333326},null,"-",{"$f":"+AH2729","v":15},null,"*",{"$f":"+AN2744","v":0.83333333333333326},null,"² /",2,"=",0,null,null,"Ma +",null,"A","*",{"$f":"+N2744+Q2744","v":2.5},null,"+","X","*",{"$f":"+AN2744","v":0.83333333333333326},null,"-",{"$f":"+T2744*W2744*(Z2744+AC2744)+AF2744*AI2744+AQ2744*AT2744^2/AW2744","v":50.208333333333329},null,null,"=",0,null,"(4.cü denklem)"]
[null,null,"y2 = X * L3 / ( 3 * E * I2 ) =",null,null,null,null,null,null,null,"X","*",{"$f":"+T2723","v":1.6666666666666667},null,"3/(",3,"*","E","*","I2",")=",{"$f":"+M2748^3/P2748","v":1.5432098765432103},null,"*","X"," /(","E","*","I2",")",null,"(E noktasındaki sehim)"]
[null,null,"(","Ma *",null,{"$f":"+G2747","v":1.3888888888888891},null,"+","A","*",{"$f":"+L2747","v":0.77160493827160515},null,"-",{"$f":"+O2747","v":0.53583676268861469},null,null,")/(","E","*","I1",")=",{"$f":"+V2748","v":1.5432098765432103},null,"*","X"," /(","E","*","I2",")"]
[null,null,"beş adet denklem beş adet bilinmeyen çözülürse :"]
[null,null,"Ma =",null,{"$f":"+V2754","v":74.913307807329574},null,null,null,{"$f":"+AO2737","v":1.3888888888888891},0,0,0,-1,{"$f":"+AT2737","v":-1.8754286694101512},null,null,{"$f":"MINVERSE(I2754:M2758)","v":0},0,-2.7912486064659983,1.1497849976110848,-99303858.576206401,{"$f":"MMULT(Q2754:U2758,N2754:N2758)","v":74.913307807329574}]
[null,null,"D1 =",null,132.25006033731881,null,null,null,1,{"$f":"+BF2744","v":2.5},{"$f":"+BK2744","v":0.83333333333333326},0,0,{"$f":"-BN2744","v":-50.208333333333329},null,null,0,-1,-4.6520810107766639,1.9163083293518079,-165506430.96034402,132.25006033731881]
[null,null,"1.ci bölgede elastik eğri denklemi"]
[null,null,"y = (",null,{"$f":"+E2754","v":74.913307807329574},null,null,"*",{"$f":"+D2762","v":1.6666666666666667},null,"² /",2,"+",{"$f":"+E2755","v":-51.322984684397731},null,null,"*",{"$f":"+I2763","v":1.6666666666666667},null,"3 /",6,"-",{"$f":"+Q2761","v":1.6666666666666667},null,"*",{"$f":"+R2763","v":1.6666666666666667},null,"4 /",24,null,")* 108 / (",null,null,{"$f":"+AT2707","v":200000},null,null,"*",{"$f":"+AT2723","v":92080},null,null,")"]
[null,null,"y=",{"$f":"+E2764","v":0.34703168794257944},null,null,"mm",null,{"$f":"IF(ABS(D2766)<ABS(M2766),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O2765","v":16.666666666666668},null,null,"mm",null,{"$f":"IF(ABS(D2766)<ABS(M2766),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"z=",0,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D2769<=AC2703,\"\",\"azalt.\")","v":""}]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"X2705*1000","v":2500},null,null," /",150,null,"=",{"$f":"+H2772/L2772","v":16.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E2771","v":0.34703168794257944},null,null,"mm",null,{"$f":"IF(ABS(D2773)<ABS(M2773),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O2772","v":16.666666666666668},null,null,"mm",null,{"$f":"IF(ABS(D2773)<ABS(M2773),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"y2 = X * L3 / ( 3 * E * I2 ) =",null,null,null,null,null,null,null,{"$f":"+E2756*1000","v":3822.9846843977348},null,null,"*",{"$f":"+T2723*1000","v":1666.6666666666667},null,null,"3/(",3,"*",{"$f":"+AT2707","v":200000},null,null,"*",{"$f":"+BH2723","v":8360},null,null,"*",10000,null,null,")"]
[null,null,"y2 =",null,{"$f":"+E2776","v":0.35285094036100539},null,null,"mm",null,{"$f":"IF(ABS(E2778)<ABS(N2778),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O2777","v":8.3333333333333339},null,null,"mm",null,{"$f":"IF(ABS(E2778)<ABS(N2778),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kirişlerin elastisite modülü)"]
[null,null,null,null,null,null,null,null,"A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B"]
[null,null,null,null,null,null,null,null,null,null,null,null,"I1",null,null,null,null,"C",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D",null,"alttaki kiriş"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(Y2796-Y2794)/2","v":2},null,"m",null,null,null,null,null,null,null,null,null,4,null,"m",null,null,null,null,null,null,null,null,null,{"$f":"+M2794","v":2},null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Y2783","v":50},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(AG2784,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(AI2790,$CG$6:$CG$120,0),0)","v":150}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+N2784","v":12},null,"KN/m"]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C=",{"$f":"+Y2813/2","v":10.518369401107197},null,null,"KN",null,null,null,null,null,null,null,null,null,"D=",{"$f":"+Y2813/2","v":10.518369401107197},null,null,"KN"]
[null,null,null,null,null,null,"yayılı yükten dolayı sehim"]
[null,null,null,null,null,null,"y2 = ( P -  X ) * L3 / ( 48 * E * I2x ) = (",null,null,null,null,null,null,null,null,null,null,{"$f":"+Y2783*1000","v":50000},null,null,"-","X","*",1000,null,null,")*",{"$f":"+V2825","v":8000},null,null,"3/(",48,null,"*",{"$f":"+AC2825","v":200000},null,null,"*",{"$f":"+AG2825","v":92080},null,null,"*",10000,null,null,")=",{"$f":"+AB2827^3/(AF2827*AI2827*AM2827*AQ2827)","v":5.7920648711265567E-5},null,null,"*(",{"$f":"+R2827","v":50000},null,null,"-","X","*",1000,null,null,")"]
[null,null,null,null,null,null,"tekil yükten dolayı sehim"]
[null,null,null,null,null,null,"y3 = y4 "]
[null,null,null,null,null,null,{"$f":"+G2835","v":2.8960324355632783},null,null,"=",{"$f":"+Q2835+K2835","v":0.13766546529818741},null,null,"*","X"]
[null,null,null,null,null,null,"X","=",{"$f":"+G2836/K2836","v":21.036738802214394},null,null,"KN"]
[null,null,null,null,null,null,"yayılı yükten dolayı sehim"]
[null,null,null,null,null,null,"y2 = ( P -  X ) * L3 / ( 48 * E * I2x ) = (",null,null,null,null,null,null,null,null,null,null,{"$f":"+Y2783*1000","v":50000},null,null,"-",{"$f":"+I2837*1000","v":21036.738802214393},null,null,")*",{"$f":"+AB2827","v":8000},null,null,"3/(",48,null,"*",{"$f":"+AI2827","v":200000},null,null,"*",{"$f":"+AM2827","v":92080},null,null,"*",{"$f":"+AQ2827","v":10000},null,null,")=",{"$f":"(R2842-V2842)*Z2842^3/(AD2842*AG2842*AK2842*AO2842)","v":1.6775708773695688},null,null,"mm"]
[null,null,null,null,null,null,"y3 =",null,{"$f":"+I2844","v":5.1528098000455032},null,null,"mm",null,{"$f":"IF(ABS(I2846)<ABS(R2846),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+S2845","v":26.666666666666668},null,null,"mm",null,{"$f":"IF(ABS(I2846)<ABS(R2846),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,null,null,null,null,"tekil yükten dolayı sehim"]
[null,null,null,null,null,null,"y4 =",null,{"$f":"+I2850","v":1.677570877369569},null,null,"mm",null,{"$f":"IF(ABS(I2852)<ABS(R2852),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+S2851","v":13.333333333333334},null,null,"mm",null,{"$f":"IF(ABS(I2852)<ABS(R2852),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,"C"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"(1.ci bölge)",null,null,null,null,null,null,null,null,null,null,"(2.ci bölge)",null,null,null,null,null,null,null,null,null,null,"A-B-D çubuğu için :"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,"KN/m",null,null,null,null,null,null,null,null,null,null,25,null,"KN",null,null,null,null,null,"I1 =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(L2868,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+O2863","v":15},null,"KN/m"]
[null,null,"Ax =",null,0,null,"KN"]
[null,null,null,null,null,null,null,null,"A",null,null,null,null,null,null,null,null,null,null,null,null,null,"B",null,null,null,null,null,"D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+P2870","v":3},null,"m",null,null,null,null,null,null,{"$f":"+Y2870","v":1.5},null,"m"]
[null,null,null,null,"P","*",{"$f":"+P2882","v":3},null,"-",{"$f":"+P2876","v":15},null,"*",{"$f":"+P2882+Y2882","v":4.5},null,"*",{"$f":"+M2885/2","v":2.25},null,"-",{"$f":"+AB2875","v":25},null,"*",{"$f":"+P2882+Y2882","v":4.5},null,"=",0]
[null,null,null,null,"Ay  +",null,"P","-",{"$f":"+P2876","v":15},null,"*",{"$f":"+P2882+Y2882","v":4.5},null,"-",{"$f":"+AB2875","v":25},null,"=",0]
[null,null,null,null,"D =  P * L / ( A * E )"]
[null,null,null,null,"v1' =",null,{"$f":"+G2893","v":4.375},null,null,"*","x²"," /",2,"-",{"$f":"+M2893","v":15},null,"*","x3"," /",6,"+","C1"]
[null,null,null,null,"v2'' =",null,{"$f":"+H2881","v":4.375},null,null,"*(",{"$f":"+P2882","v":3},null,"+","z",")-",{"$f":"+P2876","v":15},null,"*",{"$f":"+P2882","v":3},null,"*(",{"$f":"+P2882/2","v":1.5},null,"+","z",")+",{"$f":"+V2875","v":88.125},null,null,"*","z","-",{"$f":"+O2863","v":15},null,"*","z²"," /",2]
[null,null,null,null,"sınır ve uygunluk şartları :"]
[null,null,null,null,"x = 0 ; v1 = 0",null,null,null,null,null,"C2 = 0"]
[null,null,null,null,"z = 0 ; v2 =",null,null,null,{"$f":"+G2899","v":4.375},null,null,"*",{"$f":"+K2899","v":3},null,"3/",6,"-",{"$f":"+S2899","v":45},null,null,"*",{"$f":"+V2899","v":1.5},null,"3/",6,"+","D2","=","D2","+",{"$f":"I2903*M2903^3/P2903-R2903*V2903^3/Y2903","v":-5.625}]
[null,null,null,null,"( x = L ; v1' ) = ( z = 0 ; v2' )",null,null,null,null,null,null,null,null,null,"D1","+",{"$f":"+AE2906","v":-30.9375},null,null,"=","C1","+",{"$f":"+AD2905","v":-47.8125},null,null,null,null,"C1","-","D1","+",{"$f":"+W2907-Q2907","v":-16.875},null,null,"=","=",0,null,"(2.ci denklem)"]
[null,null,null,null,"y = (",null,{"$f":"+AF2909","v":-30.9375},null,null,"+","C1","*",{"$f":"+AL2909","v":3},null,")/(","E","*","I1",")"]
[null,null,null,null,"D =  P * L / ( A * E ) = y = (",null,null,null,null,null,null,null,{"$f":"+G2910","v":-30.9375},null,null,"+","C1","*",{"$f":"+M2910","v":3},null,")/(","E","*","I1",")"]
[null,null,null,null,"D2","=",{"$f":"+G2914*AG2904+AL2904","v":-505.28103966346151}]
[null,null,null,null,"1.ci bölgede"]
[null,null,null,null,"( E * I ) / 108 * y =",null,null,null,null,null,{"$f":"+G2895","v":4.375},null,null,"*",{"$f":"+F2918","v":3},null,"3/",6,"-",{"$f":"+O2895","v":15},null,"*",{"$f":"+O2919","v":3},null,"4/",24,null,"+",{"$f":"+G2914","v":15.514134615384615},null,null,"*",{"$f":"+W2919","v":3}]
[null,null,null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"P2870*1000","v":3000},null,null," /",300,null,"=",{"$f":"+J2922/N2922","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,null,null,"( E * I ) / 108 * y =",null,null,null,null,null,{"$f":"+G2899","v":4.375},null,null,"*(",{"$f":"+K2899","v":3},null,"+",{"$f":"+F2925","v":1.5},null,")3"," /",6,"-",{"$f":"+S2899","v":45},null,"*(",{"$f":"+V2899","v":1.5},null,"+",{"$f":"+R2926","v":1.5},null,")3"," /",6,"+",{"$f":"+AD2899","v":88.125},null,null,"*",{"$f":"+AD2926","v":1.5},null,"3/",6,"-",{"$f":"+AL2899","v":15},null,"*",{"$f":"+AN2926","v":1.5},null,"4/",24,null,"+",{"$f":"+G2915","v":-1.3608653846153853},null,null,"*",{"$f":"+AV2926","v":1.5},null,"+",{"$f":"+G2916","v":-505.28103966346151}]
[null,null,null,null,"y =",null,{"$f":"(G2927*(K2927+N2927)^3/R2927-T2927*(W2927+Z2927)^3/AD2927+AF2927*AJ2927^3/AM2927-AO2927*AR2927^4/AU2927+AX2927*BB2927+BE2927)*100000000/(BK2927*BO2927)","v":-3.2415876153365804},null,null,"mm"]
[null,null,null,null,"ARA KESİT TESİRLERİ"]
[null,null,null,null,"x=",1,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(F2933<=P2870,\"\",\"azalt.\")","v":""}]
[null,null,null,null,"z=",1,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(F2937<=Y2882,\"\",\"azalt.\")","v":""}]
[]
[null,"TEKİL & YAYILI YÜKLÜ ASKILI ÇELİK KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yatay çubuk enkesiti",null,null,null,null,null,null,null,null,null,null,null,null,"düşey çubık enkesiti"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A-B-D çubuğu için :"]
[null,null,null,null,null,null,null,"A",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D",null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(L2955,$CG$6:$CG$120,0),0)","v":12},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(P2945,$CG$6:$CG$120,0),0)","v":12}]
[null,null,null,null,null,null,null,null,null,"I1 =",null,"IPE 600",null,null,null,null,null,null,null,null,null,null,"B",null,"(2. bölge)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(L2955,$CG$6:$CG$120,0),0)","v":19},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(P2945,$CG$6:$CG$120,0),0)","v":19}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(L2955,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(P2945,$CG$6:$CG$120,0),0)","v":220}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"P=",{"$f":"+H3006","v":101.32449295260604},null,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+O2950","v":40},null,"KN/m"]
[null,null,null,null,null,null,null,null,"A",null,null,null,null,null,null,null,null,null,null,null,null,null,"B",null,null,null,null,null,"D"]
[null,null,null,null,null,"Ay =",null,{"$f":"+AB3023","v":19.943412294269983},null,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dy =",null,{"$f":"+H3025","v":10.732094753123974},null,null,"KN"]
[null,null,null,null,null,"D =  P * L / ( A * E )"]
[null,null,null,null,null,"Ay = (",null,{"$f":"+K2973*N2973*Q2973","v":217.79999999999998},null,null,"-","P","*",{"$f":"+V2973","v":1.5},null,")/",{"$f":"+H2973","v":3.3},null,"=",{"$f":"+H2974/Q2974","v":66},null,null,"-","P","*",{"$f":"+N2974/Q2974","v":0.45454545454545459}]
[null,null,null,null,null,"v1' =",null,"(",{"$f":"+I2976","v":66},null,null,"-","P","*",{"$f":"+O2976","v":0.45454545454545459},null,")*","x²"," /",2,"-",{"$f":"+T2976","v":40},null,"*","x3"," /",6,"+","C1"]
[null,null,null,null,null,"v2'' =",null,"(",{"$f":"+T2974","v":66},null,null,"-","P","*",{"$f":"+Z2974","v":0.45454545454545459},null,")*(",{"$f":"+P2968","v":1.8},null,"+","z",")-",{"$f":"+P2962","v":40},null,"*",{"$f":"+P2968","v":1.8},null,"*(",{"$f":"+P2968/2","v":0.9},null,"+","z",")+","P","*","z","-",{"$f":"+O2950","v":40},null,"*","z²"," /",2]
[null,null,null,null,null,"v2' =",null,"(",{"$f":"+I2980","v":66},null,null,"-","P","*",{"$f":"+O2980","v":0.45454545454545459},null,")*(",{"$f":"+R2980","v":1.8},null,"+","z",")²"," /",2,"-",{"$f":"+Z2980*W2980","v":72},null,"*(",{"$f":"+AC2980","v":0.9},null,"+","z",")²"," /",2,"+","P","*","z²"," /",2,"-",{"$f":"+AL2980","v":40},null,"*","z3"," /",6,"+","D1"]
[null,null,null,null,null,"sınır ve uygunluk şartları :"]
[null,null,null,null,null,null,null,null,null,null,null,"(",{"$f":"+M2985","v":66},null,null,"-","P","*",{"$f":"+S2985","v":0.45454545454545459},null,")*",{"$f":"(V2985+Y2985)^3/AC2985","v":5.9894999999999996},null,null,"+",{"$f":"-AE2985*(AH2985+AK2985)^3/AO2985-AX2985*BA2985^4/BD2985","v":-174.32550000000001},null,null,"+","P","*",{"$f":"+AS2985^3/AV2985","v":0.5625},null,null,"+","D1","*",{"$f":"+BI2985","v":1.5},null,"+","D2","=",0]
[null,null,null,null,null,"( x = L ; v1 ) = ( z = 0 ; v2 )",null,null,null,null,null,null,null,null,null,"C1","*",{"$f":"+AO2988","v":1.8},null,"-","P","*",{"$f":"+AT2988","v":0.44181818181818189},null,"+",{"$f":"+AW2988","v":46.655999999999992},null,null,"=","D2","-","P","*",{"$f":"+AM2989","v":0.44181818181818189},null,"+",{"$f":"+AP2989","v":55.403999999999996},null,null,null,null,"C1","*",{"$f":"+R2990","v":1.8},null,"-","D2","+",{"$f":"+Z2990-AK2990","v":-8.7480000000000047},null,null,"=",0,null,"(2.ci denklem)"]
[null,null,null,null,null,"z = 0 ; v2' =",null,null,null,"(",{"$f":"+I2981","v":66},null,null,"-","P","*",{"$f":"+O2981","v":0.45454545454545459},null,")*",{"$f":"+R2981","v":1.8},null,"² /",2,"-",{"$f":"+Z2981","v":72},null,"*",{"$f":"+AC2981","v":0.9},null,"² /",2,"+","D1","=","D1","-","P","*",{"$f":"+Q2992*T2992^2/W2992","v":0.73636363636363644},null,"+",{"$f":"+K2992*T2992^2/W2992-Y2992*AB2992^2/AE2992","v":77.759999999999991}]
[null,null,null,null,null,"( E * I ) / y =",null,null,null,"(",{"$f":"+I2978","v":66},null,null,"-","P","*",{"$f":"+O2978","v":0.45454545454545459},null,")*",{"$f":"+P2968","v":1.8},null,"3 /",6,"-",{"$f":"+V2978","v":40},null,"*",{"$f":"+T2995","v":1.8},null,"4 /",24,null,"+","C1","*",{"$f":"+AB2995","v":1.8},null,"=","C1","*",{"$f":"+AJ2995","v":1.8},null,"-","P","*",{"$f":"Q2995*T2995^3/W2995","v":0.44181818181818189},null,"+",{"$f":"+K2995*T2995^3/W2995-Y2995*AB2995^4/AE2995","v":46.655999999999992}]
[null,null,null,null,null,"B-C çubuğu uzamasıyla B noktası çökmesi eşitliği ilkesinden"]
[null,null,null,null,null,"C1","*",{"$f":"+N3000","v":1954.8218940052127},null,null,"-","P","*",{"$f":"+T3000+H3000","v":624.05068866841248},null,null,"+",{"$f":"+X3000","v":50668.983492615109},null,null,"=",0,null,"(4.ci denklem)"]
[null,null,null,null,null,"D1 =",null,{"$f":"+V3004","v":-3.293513703748765},null,null,null,{"$f":"+AR2990","v":1.8},0,-1,0,{"$f":"-AW2990","v":8.7480000000000047},null,-0.28850524045087739,-0.28850524045087739,-1.4327578606763158,9.9859086880203004E-4,-3.293513703748765]
[null,null,null,null,null,"P =",null,101.32449295260604,null,null,null,{"$f":"+H3001","v":1954.8218940052127},0,0,{"$f":"-N3001","v":-624.05068866841248},{"$f":"-R3001","v":-50668.983492615109},null,-0.90373485809624776,-0.90373485809624776,-1.3556022871443716,1.5256249384475457E-3,101.32449295260604]
[null,null,null,null,null,"A-B-C Kirişinde sehim hesabı"]
[null,null,null,null,null,"y = (",null,{"$f":"+K3008","v":66},null,null,"-",{"$f":"+H3006","v":101.32449295260604},null,null,"*",{"$f":"+Q3008","v":0.45454545454545459},null,")*",{"$f":"+G3010","v":1.75},null,"3 /",6,"-",{"$f":"+X3008","v":40},null,"*",{"$f":"+S3011","v":1.75},null,"4 /",24,null,"+",{"$f":"+H3003","v":6.4264862962512339},null,null,"*",{"$f":"+AA3011","v":1.75},null,") * 108 / (",null,null,{"$f":"+AK2952","v":200000},null,null,"*",{"$f":"+AK2950","v":92080},null,null,")"]
[null,null,null,null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"R2959*1000","v":3300},null,null," /",300,null,"=",{"$f":"+K3013/O3013","v":11},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,null,null,null,"( E * I ) / y =",null,null,null,"(",{"$f":"+I2982","v":66},null,null,"-","P","*",{"$f":"+O2982","v":0.45454545454545459},null,")*(",{"$f":"+R2982","v":1.8},null,"+","z",")3"," /",6,"-",{"$f":"+Z2982","v":72},null,"*(",{"$f":"+AC2982","v":0.9},null,"+","z",")3"," /",6,"+","P","*","z3"," /",6,"-",{"$f":"+AQ2982","v":40},null,"*","z4"," /",24,null,"+","D1","*","z","+","D2"]
[null,null,null,null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"R2959*1000","v":3300},null,null," /",300,null,"=",{"$f":"+K3020/O3020","v":11},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,null,null,null,"mesnet tepkileri"]
[null,null,null,null,null,"Dy =",null,{"$f":"(R3024*U3024*X3024-K3024*O3024)/H3024","v":10.732094753123974},null,null,"KN"]
[null,null,null,null,null,"ARA KESİT TESİRLERİ"]
[null,null,null,null,null,"Mx =",null,"(",{"$f":"+I2976","v":66},null,null,"-",{"$f":"+H3006","v":101.32449295260604},null,null,"*",{"$f":"+O2976","v":0.45454545454545459},null,")*",{"$f":"+G3028","v":1},null,null,"-",{"$f":"+T2976","v":40},null,"*",{"$f":"+G3028","v":1},null,"² /",2,"=",{"$f":"(I3029-M3029*Q3029)*T3029-X3029*AA3029^2/AD3029","v":-5.6587705730017035E-2},null,null,"KNm"]
[null,null,null,null,null,"z=",1,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(G3032<=Y2968,\"\",\"azalt.\")","v":""}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,"KN"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"I1 =",null,92080,null,null,"cm4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"I1 =",null,92080,null,null,"cm4"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"L=",1.5,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",1.5,null,"m"]
[null,null,null,null,null,null,"y =",null,{"$f":"+T3041*1000","v":15000},null,null,"*",{"$f":"+N3050*1000","v":1500},null,null,"3/(",3,"*",{"$f":"+X3048","v":200000},null,null,"*",{"$f":"+X3045","v":92080},null,null,"*",10000,null,null,")",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y = (",null,{"$f":"+BF3041*1000","v":15000},null,null," /",2,")*",{"$f":"+AZ3050*1000","v":1500},null,null,"3/(",3,"*",{"$f":"+BJ3048","v":200000},null,null,"*",{"$f":"+BJ3045","v":92080},null,null,"*",10000,null,null,")"]
[null,null,null,null,null,null,"y = w4 * L4 / ( 8 * E * I )      (yayılı yüklü konsol kiriş ucu sehim formülü)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y = w4 * L4 / ( 8 * E * I )      (yayılı yüklü konsol kiriş ucu sehim formülü)"]
[null,null,null,null,null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"N3050*1000","v":1500},null,null," /",150,null,"=",{"$f":"+L3059/P3059","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"AZ3050*1000","v":1500},null,null," /",150,null,"=",{"$f":"+AX3059/BB3059","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,"w =",null,5,null,"KN/m"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"I3 =",null,{"$f":"+X3069","v":92080},null,null,"cm4",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"I4 =",null,{"$f":"+BJ3069","v":92080},null,null,"cm4"]
[]
[null,null,null,null,null,null,"y = P * L3 / ( 3 * E * I )      (tekil yüklü konsol kiriş ucu sehim formülü)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y = P * L3 / ( 3 * E * I )      (tekil yüklü konsol kiriş ucu sehim formülü)"]
[null,null,null,null,null,null,"y = (",null,{"$f":"+T3064*1000","v":15000},null,null," /",3,")*",{"$f":"+N3073*1000","v":1500},null,null,"3/(",3,"*",{"$f":"+X3072","v":200000},null,null,"*",{"$f":"+X3068","v":92080},null,null,"*",10000,null,null,")",null,null,null,null,null,null,null,null,null,null,null,null,"y = (",null,{"$f":"+BF3063*1000","v":15000},null,null," /",4,")*",{"$f":"+AZ3073*1000","v":1500},null,null,"3/(",3,"*",{"$f":"+BJ3072","v":200000},null,null,"*",{"$f":"+BJ3067","v":92080},null,null,"*",10000,null,null,")"]
[null,null,null,null,null,null,"y = (",null,{"$f":"+N3065","v":5},null," /",3,")4","*",{"$f":"+N3073*1000","v":1500},null,null,"4/(",8,"*",{"$f":"+U3077","v":200000},null,null,"*",{"$f":"+Y3077","v":92080},null,null,"*",10000,null,null,")",null,null,null,null,null,null,null,null,null,null,null,null,"y = (",null,{"$f":"+AZ3064","v":5},null," /",4,")4","*",{"$f":"+AZ3073*1000","v":1500},null,null,"4/(",8,"*",{"$f":"+BG3077","v":200000},null,null,"*",{"$f":"+BK3077","v":92080},null,null,"*",10000,null,null,")"]
[]
[null,"TEKİL YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kiriş enkesiti"]
[null,null,null,null,null,null,null,null,null,null,null,null,"(1.ci bölge)",null,null,null,null,null,null,null,null,null,null,null,"(2.ci bölge)"]
[null,null,null,null,null,"A=",{"$f":"AA3088*Y3097/O3097","v":75},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"AA3088+G3096","v":225},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(M3089,$CG$6:$CG$120,0),0)","v":12}]
[null,null,null,null,null,null,null,null,null,null,null,"sınır ve uygunluk şartları :",null,null,null,null,null,null,null,null,"( x = L ; v1' ) = ( z = 0 ; v2' )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(M3089,$CG$6:$CG$120,0),0)","v":19}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(M3089,$CG$6:$CG$120,0),0)","v":220}]
[null,null,"1.ci bölgede :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,"v1 =",null,{"$f":"+E3107","v":-75},null,"*","x3"," /",6,"+","C1","*","x","+","C2"]
[null,null,"2.ci bölgede :"]
[null,null,"v2' =",null,{"$f":"+E3110","v":-75},null,"*(",{"$f":"+H3110","v":3},null,"+","z",")²"," /",2,"+",{"$f":"+M3110","v":225},null,"*","z²"," /",2,"+","D1"]
[null,null,"x = 0 ; v1 = 0",null,null,null,null,null,"C2 = 0"]
[null,null,"( x = L ; v1 ) = ( z = 0 ; v2 )",null,null,null,null,null,null,null,null,null,"C1","*",{"$f":"+V3116","v":3},null,"+",{"$f":"+Y3116","v":-337.5},null,null,"=","D2","+",{"$f":"+S3117","v":-337.5},null,null,null,null,"C1","*",{"$f":"+O3118","v":3},null,"-",{"$f":"+X3115","v":337.5},null,null,"=",0,null,null,"C1","=",{"$f":"+AH3118/AE3118","v":112.5}]
[null,null,"z = 0 ; v2' =",null,null,null,{"$f":"+E3111","v":-75},null,"*",{"$f":"+H3111","v":3},null,"² /",2,"+","D1","=","D1","+",{"$f":"+G3120*J3120^2/M3120","v":-337.5}]
[null,null,"y = (",null,{"$f":"+H3123","v":-75},null,"*","x3"," /",6,"+",{"$f":"+AQ3118","v":112.5},null,null,"*","x",") * 108 / ( E * I )"]
[null,null,"x=",1,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D3125<=O3097,\"\",\"azalt.\")","v":""}]
[null,null,"y=",{"$f":"+E3127","v":0.5430060816681147},null,null,"mm",null,{"$f":"IF(ABS(D3129)<ABS(M3129),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O3128","v":10},null,null,"mm",null,{"$f":"IF(ABS(D3129)<ABS(M3129),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"2.ci bölgede elastik eğri denklemi"]
[null,null,"y = (",null,{"$f":"+E3132","v":-75},null,"*(",{"$f":"+H3132","v":3},null,"+",{"$f":"+D3133","v":1.5},null,")3"," /",6,"+",{"$f":"+P3132","v":225},null,"*",{"$f":"+D3133","v":1.5},null,"3 /",6,"+",{"$f":"+W3132","v":112.5},null,null,"*",{"$f":"+T3134","v":1.5},null,"+",{"$f":"+AC3132","v":337.5},null,null,")* 108 / (",null,null,{"$f":"+AM3105","v":200000},null,null,"*",{"$f":"+AM3104","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E3134*(H3134+K3134)^3/O3134+Q3134*T3134^3/W3134+Y3134*AC3134+AF3134)*100000000/(AL3134*AP3134)","v":-2.7489682884448308},null,null,"mm"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[]
[]
[null,null,null,null,null,null,null,null,null,"A=",{"$f":"(G3142*(I3151+S3153)+T3142*X3151-AE3142*AC3151)/S3153","v":300},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+G3142+T3142+AE3142-K3150","v":300},null,"KN"]
[null,null,null,null,null,null,null,null,1.5,null,"m",null,null,null,2.5,null,"m",null,null,null,null,null,null,{"$f":"+S3153-O3151","v":2.5},null,"m",null,null,1.5,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(O3147,$CG$6:$CG$120,0),0)","v":19}]
[null,null,null,null,null,null,null,null,"( x = L ; v1' ) = ( z = 0 ; v2' )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( k = L ; v3' ) = ( m = 0 ; v4' )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( z = L ; v2' ) = ( k = 0 ; v3' )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,"v1'' =",null,{"$f":"-G3142","v":-150},null,"*","x"]
[null,null,"v1 =",null,{"$f":"+E3161","v":-150},null,"*","x3"," /",6,"+","C1","*","x","+","C2"]
[null,null,"v2 =",null,{"$f":"+E3165","v":-150},null,"*(",{"$f":"+H3165","v":1.5},null,"+","z",")3"," /",6,"+",{"$f":"+P3165","v":300},null,"*","z3"," /",6,"+","D1","*","z","+","D2"]
[null,null,"v3' =",null,{"$f":"+E3168","v":-150},null,"*(",{"$f":"+H3168","v":4},null,"+","k",")²"," /",2,"+",{"$f":"+M3168","v":300},null,"*(",{"$f":"+P3168","v":2.5},null,"+","k",")²"," /",2,"-",{"$f":"+U3168","v":300},null,"*","k²"," /",2,"+","E1"]
[null,null,"4.cü bölgede :"]
[null,null,"v4'' =",null,{"$f":"-G3142","v":-150},null,"*(",{"$f":"+I3151+S3153","v":6.5},null,"+","m",")+",{"$f":"+K3150","v":300},null,"*(",{"$f":"+S3153","v":5},null,"+","m",")-",{"$f":"+T3142","v":300},null,"*(",{"$f":"+X3151","v":2.5},null,"+","m",")+",{"$f":"+AA3150","v":300},null,"*","m"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"x = L ; v1 =",null,null,null,{"$f":"+E3162","v":-150},null,"*",{"$f":"+I3151","v":1.5},null,"3 /",6,"+","C1","*",{"$f":"+J3178","v":1.5},null,"+","C2","=","C1","*",{"$f":"+Q3178","v":1.5},null,"+","C2","+",{"$f":"+G3178*J3178^3/M3178","v":-84.375}]
[null,null,"x = L ; v1' =",null,null,null,{"$f":"+E3161","v":-150},null,"*",{"$f":"+I3151","v":1.5},null,"² /",2,"+","C1","=","C1","+",{"$f":"+G3181*J3181^2/M3181","v":-168.75}]
[null,null,"z = L ; v2 =",null,null,null,{"$f":"+E3166","v":-150},null,"*(",{"$f":"+H3166","v":1.5},null,"+",{"$f":"+O3151","v":2.5},null,")3"," /",6,"+",{"$f":"+P3166","v":300},null,"*",{"$f":"+M3184","v":2.5},null,"3 /",6,"+","D1","*",{"$f":"+V3184","v":2.5},null,"+","D2","=","D1","*",{"$f":"+AC3184","v":2.5},null,"+","D2","+",{"$f":"+G3184*(J3184+M3184)^3/Q3184+S3184*V3184^3/Y3184","v":-818.75}]
[null,null,"z = L ; v2' =",null,null,null,{"$f":"+E3165","v":-150},null,"*(",{"$f":"+H3165","v":1.5},null,"+",{"$f":"+O3151","v":2.5},null,")²"," /",2,"+",{"$f":"+P3165","v":300},null,"*",{"$f":"+M3187","v":2.5},null,"² /",2,"+","D1","=","D1","+",{"$f":"+G3187*(J3187+M3187)^2/Q3187+S3187*V3187^2/Y3187","v":-262.5}]
[null,null,"k = L ; v3 =",null,null,null,{"$f":"+E3170","v":-150},null,"*(",{"$f":"+H3170","v":4},null,"+",{"$f":"+X3151","v":2.5},null,")3"," /",6,"+",{"$f":"+P3170","v":300},null,"*(",{"$f":"+S3170","v":2.5},null,"+",{"$f":"+M3190","v":2.5},null,")3"," /",6,"-",{"$f":"+AA3170","v":300},null,"*",{"$f":"+Y3190","v":2.5},null,"3 /",6,"+","E1","*",{"$f":"+AH3190","v":2.5},null,"+","E2","=","E1","*",{"$f":"+AO3190","v":2.5},null,"+","E2","+",{"$f":"G3190*(J3190+M3190)^3/Q3190+S3190*(V3190+Y3190)^3/AC3190-AE3190*AH3190^3/AK3190","v":-1396.875}]
[null,null,"k = L ; v3' =",null,null,null,{"$f":"+E3169","v":-150},null,"*(",{"$f":"+H3169","v":4},null,"+",{"$f":"+X3151","v":2.5},null,")²"," /",2,"+",{"$f":"+P3169","v":300},null,"*(",{"$f":"+S3169","v":2.5},null,"+",{"$f":"+M3193","v":2.5},null,")²"," /",2,"-",{"$f":"+AA3169","v":300},null,"*",{"$f":"+Y3193","v":2.5},null,"² /",2,"+","E1","=","E1","+",{"$f":"G3193*(J3193+M3193)^2/Q3193+S3193*(V3193+Y3193)^2/AC3193-AE3193*AH3193^2/AK3193","v":-356.25}]
[null,null,"m = 0 ; v4' =",null,null,null,{"$f":"+E3173","v":-150},null,"*",{"$f":"+H3173","v":6.5},null,"² /",2,"+",{"$f":"+P3173","v":300},null,"*",{"$f":"+S3173","v":5},null,"² /",2,"-",{"$f":"+AA3173","v":300},null,"*",{"$f":"+AD3173","v":2.5},null,"² /",2,"+","F1","=","F1","+",{"$f":"G3194*J3194^2/M3194+O3194*R3194^2/U3194-W3194*Z3194^2/AC3194","v":-356.25}]
[null,null,"sekiz adet denklem sekiz adet bilinmeyen çözülürse :"]
[null,null,"D2 =",null,84.375,null,null,null,1,0,-1,0,0,0,0,0,0,null,null,1,0,-1,0,0,0,0,0,84.375]
[null,null,"F1 =",null,262.5,null,null,null,0,0,0,0,{"$f":"+AG3192","v":2.5},1,0,-1,0,null,null,-0.2,0.2,0.2,0,0.2,-0.5,0,-1,262.5]
[null,null,"1.ci bölgede elastik eğri denklemi"]
[null,null,"y = (",null,{"$f":"+E3207","v":-150},null,"*",{"$f":"+D3208","v":0},null,"3 /",6,"+",{"$f":"+L3207","v":262.50000000000006},null,null,"*",{"$f":"+D3208","v":0},null,"+",{"$f":"+R3207","v":-309.37500000000006},null,null,")* 108 / (",null,null,{"$f":"+AO3157","v":200000},null,null,"*",{"$f":"+AO3156","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E3209*H3209^3/K3209+M3209*Q3209+T3209)*100000000/(Z3209*AD3209)","v":-1.67992506516073},null,null,"mm"]
[null,null,"y=",{"$f":"+E3210","v":-1.67992506516073},null,null,"mm",null,{"$f":"IF(ABS(D3212)<ABS(M3212),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O3211","v":10},null,null,"mm",null,{"$f":"IF(ABS(D3212)<ABS(M3212),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"y = (",null,{"$f":"+H3214","v":-150},null,"*(",{"$f":"+K3214","v":1.5},null,"+","z",")3"," /",6,"+",{"$f":"+S3214","v":300},null,"*","z3"," /",6,"+",{"$f":"+E3199","v":262.5},null,null,"*","z","+",{"$f":"+E3200","v":84.375},null,null,") * 108 / ( E * I )"]
[null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"S3153*1000","v":5000},null,null," /",300,null,"=",{"$f":"+H3219/L3219","v":16.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"3.cü bölgede elastik eğri denklemi"]
[null,null,"k=",0,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D3224<=X3151,\"\",\"azalt.\")","v":""}]
[null,null,"y =",null,{"$f":"(E3225*(H3225+K3225)^3/O3225+Q3225*(T3225+W3225)^3/AA3225-AC3225*AF3225^3/AI3225+AK3225*AO3225+AR3225)*100000000/(AX3225*BB3225)","v":-0.42422350130321462},null,null,"mm"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E3174","v":-150},null,"*(",{"$f":"+H3174","v":6.5},null,"+","m",")3"," /",6,"+",{"$f":"+P3174","v":300},null,"*(",{"$f":"+S3174","v":5},null,"+","m",")3"," /",6,"-",{"$f":"+AA3174","v":300},null,"*(",{"$f":"+AD3174","v":2.5},null,"+","m",")3"," /",6,"+",{"$f":"+AL3174","v":300},null,"*","m3"," /",6,"+","F1","*","m","+","F2"]
[null,null,"y = (",null,{"$f":"+E3231","v":-150},null,"*(",{"$f":"+H3231","v":6.5},null,"+",{"$f":"+D3232","v":1.5},null,")3"," /",6,"+",{"$f":"+P3231","v":300},null,"*(",{"$f":"+S3231","v":5},null,"+",{"$f":"+K3233","v":1.5},null,")3"," /",6,"-",{"$f":"+AA3231","v":300},null,"*(",{"$f":"+AD3231","v":2.5},null,"+",{"$f":"+W3233","v":1.5},null,")3"," /",6,"+",{"$f":"+AL3231","v":300},null,"*",{"$f":"+AI3233","v":1.5},null,"3 /",6,"+",{"$f":"+AS3231","v":262.5},null,null,"*",{"$f":"+AR3233","v":1.5},null,"+",{"$f":"+AY3231","v":1396.875},null,null,")* 108 / (",null,null,{"$f":"+AX3225","v":200000},null,null,"*",{"$f":"+BB3225","v":92080},null,null,")"]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"AC3151*1000","v":1500},null,null," /",150,null,"=",{"$f":"+H3235/L3235","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E3234","v":-1.6799250651607298},null,null,"mm",null,{"$f":"IF(ABS(D3236)<ABS(M3236),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O3235","v":10},null,null,"mm",null,{"$f":"IF(ABS(D3236)<ABS(M3236),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,"KN/m"]
[null,null,null,null,null,null,"Ma =",null,{"$f":"-E3299","v":529.37499999999898},null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+U3252+AG3252+AO3252","v":7.5},null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(AA3241,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( x = L ; v1'' ) = 0",null,null,null,null,null,null,null,null,null,"( z = L ; v2' ) = ( m = 0 ; v3' )"]
[]
[null,null,"1.ci bölgede :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m = L ; v3'' = 0"]
[null,null,"v1 =",null,"Ma *",null,"x²"," /",2,"+","A","*","x3"," /",6,"-",{"$f":"+O3266","v":5},null,"*","x4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"v2' =",null,"Ma *",null,"z","+","A","*(",{"$f":"+I3269","v":3.5},null,"+","z",")²"," /",2,"-",{"$f":"+N3269*Q3269","v":17.5},null,"*(",{"$f":"+T3269","v":1.75},null,"+","z",")²"," /",2,"-",{"$f":"+Y3269","v":15},null,"*","z3"," /",6,"+","D1"]
[null,null,"v3'' =",null,"Ma +",null,"A","*(",{"$f":"+U3252+AG3252","v":6},null,"+","m",")-",{"$f":"+Q3243","v":5},null,"*",{"$f":"+U3252","v":3.5},null,"*(",{"$f":"+U3252/2+AG3252","v":4.25},null,"+","m",")-",{"$f":"+AH3242","v":15},null,"*",{"$f":"+AG3252","v":2.5},null,"*(",{"$f":"+AG3252/2","v":1.25},null,"+","m",")-",{"$f":"+AL3241","v":300},null,"*","m","-",{"$f":"+AH3242","v":15},null,"*","m²"," /",2]
[null,null,"v3' =",null,"Ma *",null,"m","+","A","*(",{"$f":"+I3273","v":6},null,"+","m",")²"," /",2,"-",{"$f":"+N3273*Q3273","v":17.5},null,"*(",{"$f":"+T3273","v":4.25},null,"+","m",")²"," /",2,"-",{"$f":"+Y3273*AB3273","v":37.5},null,"*(",{"$f":"+AE3273","v":1.25},null,"+","m",")²"," /",2,"-",{"$f":"+AJ3273","v":300},null,"*","m²"," /",2,"-",{"$f":"+AO3273","v":15},null,"*","m3"," /",6,"+","E1"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"m = L ; v3 = 0",null,null,null,null,null,"Ma *",null,{"$f":"+AO3252","v":1.5},null,"² /",2,"+","A","*(",{"$f":"+M3275","v":6},null,"+",{"$f":"+K3279","v":1.5},null,")3"," /",6,"-",{"$f":"+U3275","v":17.5},null,"*(",{"$f":"+X3275","v":4.25},null,"+",{"$f":"+U3279","v":1.5},null,")3"," /",6,"-",{"$f":"+AF3275","v":37.5},null,"*(",{"$f":"+AI3275","v":1.25},null,"+",{"$f":"+AG3279","v":1.5},null,")3"," /",6,"-",{"$f":"+AQ3275","v":300},null,"*",{"$f":"+AS3279","v":1.5},null,"3 /",6,"-",{"$f":"+AX3275","v":15},null,"*",{"$f":"+BB3279","v":1.5},null,"4 /",24,null,"+","E1","*",{"$f":"+BJ3279","v":1.5},null,"+","E2","=",0]
[null,null,"( x = L ; v1'' ) = 0",null,null,null,null,null,null,"Ma +",null,"A","*",{"$f":"+U3252","v":3.5},null,"-",{"$f":"+K3265","v":5},null,"*",{"$f":"+N3283","v":3.5},null,"² /",2,"=",0,null,null,"Ma +",null,"A","*",{"$f":"+N3283","v":3.5},null,"-",{"$f":"+Q3283*T3283^2/W3283","v":30.625},null,null,"=",0,null,"(3.cü denklem)"]
[null,null,"z = 0 ; v2 =",null,null,null,"A","*",{"$f":"+M3271","v":3.5},null,"3 /",6,"-",{"$f":"+U3271","v":17.5},null,"*",{"$f":"+X3271","v":1.75},null,"3 /",6,"+","D2","=","A","*",{"$f":"+I3285^3/L3285","v":7.145833333333333},null,"+","D2","-",{"$f":"+N3285*Q3285^3/T3285","v":15.631510416666666}]
[null,null,"z = L ; v2 =",null,null,null,"Ma *",null,{"$f":"+AG3252","v":2.5},null,"² /",2,"+","A","*(",{"$f":"+M3271","v":3.5},null,"+",{"$f":"+I3288","v":2.5},null,")3"," /",6,"-",{"$f":"+U3271","v":17.5},null,"*(",{"$f":"+X3271","v":1.75},null,"+",{"$f":"+S3288","v":2.5},null,")3"," /",6,"-",{"$f":"+AF3271","v":15},null,"*",{"$f":"+AE3288","v":2.5},null,"4 /",24,null,"+","D1","*",{"$f":"+AN3288","v":2.5},null,"+","D2","=","Ma *",null,{"$f":"+I3288^2/L3288","v":3.125},null,"+","A","*",{"$f":"(P3288+S3288)^3/W3288","v":36},null,"+","D1","*",{"$f":"+AV3288","v":2.5},null,"+","D2","-",{"$f":"Y3288*(AB3288+AE3288)^3/AI3288+AK3288*AN3288^4/AQ3288","v":248.31380208333334}]
[null,null,"( z = L ; v2 ) = ( m = 0 ; v3 )",null,null,null,null,null,null,null,null,null,"Ma *",null,{"$f":"+BC3288","v":3.125},null,"+","A","*",{"$f":"+BH3288","v":36},null,"+","D1","*",{"$f":"+BM3288","v":2.5},null,"+","D2","-",{"$f":"+BR3288","v":248.31380208333334},null,null,"=","A","*",{"$f":"+AH3289","v":36},null,"+","E2","-",{"$f":"+AM3289","v":236.10677083333334},null,null,null,null,"Ma *",null,{"$f":"+O3290","v":3.125},null,"+","D1","*",{"$f":"+Y3290","v":2.5},null,"+","D2","-","E2","-",{"$f":"+AD3290-AO3290","v":12.20703125},null,null,"=",0,null,"(5.ci denklem)"]
[null,null,"( z = L ; v2' ) = ( m = 0 ; v3' )",null,null,null,null,null,null,null,null,null,"Ma *",null,{"$f":"+AU3292","v":2.5},null,"+","A","*",{"$f":"+AZ3292","v":18},null,"+","D1","-",{"$f":"+BE3292","v":197.109375},null,null,"=","A","*",{"$f":"+AH3293","v":18},null,"+","E1","-",{"$f":"+AM3293","v":187.34375},null,null,null,null,"Ma *",null,{"$f":"+O3294","v":2.5},null,"+","D1","-","E1","-",{"$f":"+Y3294-AJ3294","v":9.765625},null,null,"=",0,null,"(6.cı denklem)"]
[null,null,"A","+","B","-",{"$f":"+G3296*J3296+M3296*P3296+S3296","v":377.5},null,null,"=",0,null,"(7.ci denklem)"]
[null,null,"Ma =",null,{"$f":"+Z3299","v":-529.37499999999898},null,null,null,{"$f":"+K3280","v":1.125},{"$f":"+P3280","v":70.3125},0,0,0,{"$f":"+U3280","v":1.5},1,{"$f":"+Z3280","v":856.38020833333337},null,null,{"$f":"MINVERSE(I3299:O3305)","v":-6.9388939039072271E-17},-0.87499999999999822,1.8749999999999989,-3.6252180395923476E-17,-2.3129646346357426E-17,0,0,{"$f":"MMULT(S3299:Y3305,P3299:P3305)","v":-529.37499999999898}]
[null,null,"A =",null,{"$f":"+Z3300","v":159.9999999999998},null,null,null,1,{"$f":"+N3282","v":7.5},0,0,0,0,0,{"$f":"+Q3282","v":670.625},null,null,1.2631870857957337E-17,0.24999999999999969,-0.24999999999999969,-2.3684757858670005E-18,-2.3684757858670005E-18,1.5789838572446672E-18,0,159.9999999999998]
[null,null,"E1 =",null,-2051.6308593749982,null,null,null,{"$f":"+AQ3294","v":2.5},0,0,1,0,-1,0,{"$f":"+AX3294","v":9.765625},null,null,0.24999999999999983,-3.4921874999999964,2.460937499999996,0.25000000000000006,0.25000000000000006,-0.625,0,-2051.6308593749982]
[null,null,"1.ci bölgede elastik eğri denklemi"]
[null,null,"x=",1,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D3309<=U3252,\"\",\"azalt.\")","v":""}]
[null,null,"y=",{"$f":"+E3311","v":-1.2935988633072664},null,null,"mm",null,{"$f":"IF(ABS(D3313)<ABS(M3313),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O3312","v":25},null,null,"mm",null,{"$f":"IF(ABS(D3313)<ABS(M3313),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"E * I / 108 * y =",null,null,null,null,"Ma *",null,"z²"," /",2,"+","A","*(",{"$f":"+M3271","v":3.5},null,"+","z",")3"," /",6,"-",{"$f":"+U3271","v":17.5},null,"*(",{"$f":"+X3271","v":1.75},null,"+","z",")3"," /",6,"-",{"$f":"+AF3271","v":15},null,"*","z4"," /",24,null,"+","D1","*","z","+","D2"]
[null,null,"y = (",null,{"$f":"+E3316","v":-529.37499999999898},null,null,"*",{"$f":"+D3317","v":1},null,"² /",2,"+",{"$f":"+M3316","v":159.9999999999998},null,null,"*(",{"$f":"+Q3316","v":3.5},null,"+",{"$f":"+I3318","v":1},null,")3"," /",6,"-",{"$f":"+Y3316","v":17.5},null,"*(",{"$f":"+AB3316","v":1.75},null,"+",{"$f":"+U3318","v":1},null,")3"," /",6,"-",{"$f":"+AJ3316","v":15},null,"*",{"$f":"+AG3318","v":1},null,"4 /",24,null,"+",{"$f":"+AR3316","v":-718.42773437500045},null,null,"*",{"$f":"+AP3318","v":1},null,"+",{"$f":"+AX3316","v":-3258.0533854166601},null,null,")* 108 / (",null,null,{"$f":"+AH3310","v":200000},null,null,"*",{"$f":"+AL3310","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E3318*I3318^2/L3318+N3318*(R3318+U3318)^3/Y3318-AA3318*(AD3318+AG3318)^3/AK3318-AM3318*AP3318^4/AS3318+AV3318*AZ3318+BC3318)*100000000/(BI3318*BM3318)","v":-10.167523739547116},null,null,"mm"]
[null,null,"3.cü bölgede elastik eğri denklemi"]
[null,null,"m=",1,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D3325<=AO3252,\"\",\"azalt.\")","v":""}]
[null,null,"y =",null,{"$f":"(E3326*I3326^2/L3326+N3326*(R3326+U3326)^3/Y3326-AA3326*(AD3326+AG3326)^3/AK3326-AM3326*(AP3326+AS3326)^3/AW3326-AY3326*BB3326^3/BE3326-BG3326*BJ3326^4/BM3326+BP3326*BT3326+F3327)*100000000/(L3327*P3327)","v":-2.3574365107108051},null,null,"mm"]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"Mx =",null,"Ma +",null,"A","*","x","-",{"$f":"+K3265","v":5},null,"*","x²"," /",2,"=",{"$f":"+E3299","v":-529.37499999999898},null,null,"+",{"$f":"+E3300","v":159.9999999999998},null,null,"*",{"$f":"+D3333","v":1},null,"-",{"$f":"+K3334","v":5},null,"*",{"$f":"+Z3334","v":1},null,"² /",2,"=",{"$f":"+R3334+V3334*Z3334-AC3334*AF3334^2/AI3334","v":-371.8749999999992},null,null,"KNm"]
[null,null,"z=",1,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D3337<=AG3252,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,"Ma +",null,"A","*(",{"$f":"+I3269","v":3.5},null,"+","z",")-",{"$f":"+N3269","v":5},null,"*",{"$f":"+Q3269","v":3.5},null,"*(",{"$f":"+T3269","v":1.75},null,"+","z",")-",{"$f":"+Y3269","v":15},null,"*","x²"," /",2,"=",{"$f":"+E3299","v":-529.37499999999898},null,null,"+",{"$f":"+E3300","v":159.9999999999998},null,null,"*(",{"$f":"+I3338","v":3.5},null,"+",{"$f":"+D3337","v":1},null,")-",{"$f":"+N3338","v":5},null,"*",{"$f":"+Q3338","v":3.5},null,"*(",{"$f":"+T3338","v":1.75},null,"+",{"$f":"+AQ3338","v":1},null,")-",{"$f":"+Y3338","v":15},null,"*",{"$f":"+BC3338","v":1},null,"² /",2,"=",{"$f":"AF3338+AJ3338*(AN3338+AQ3338)-AT3338*AW3338*(AZ3338+BC3338)-BF3338*BI3338^2/BL3338","v":135.00000000000011},null,null,"KNm"]
[null,null,"3.ci bölgede :"]
[null,null,"Mx =",null,{"$f":"+E3299","v":-529.37499999999898},null,null,"+",{"$f":"+E3300","v":159.9999999999998},null,null,"*(",{"$f":"+I3342","v":6},null,"+",{"$f":"+D3341","v":1},null,")-",{"$f":"+N3342","v":5},null,"*",{"$f":"+Q3342","v":3.5},null,"*(",{"$f":"+T3342","v":4.25},null,"+",{"$f":"+P3343","v":1},null,")-",{"$f":"+Y3342","v":15},null,"*",{"$f":"+AB3342","v":2.5},null,"*(",{"$f":"+AE3342","v":1.25},null,"+",{"$f":"+AB3343","v":1},null,")-",{"$f":"+AJ3342","v":300},null,"*",{"$f":"+AN3343","v":1},null,"-",{"$f":"+AO3342","v":15},null,"*",{"$f":"+AT3343","v":1},null,"² /",2,"=",{"$f":"E3343+I3343*(M3343+P3343)-S3343*V3343*(Y3343+AB3343)-AE3343*AH3343*(AK3343+AN3343)-AQ3343*AT3343-AW3343*AZ3343^2/BC3343","v":106.87499999999966},null,null,"KNm"]
[null,"YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"q=",35,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kiriş enkesiti"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AO3409","v":1.606425702811245}]
[null,null,"Ma =",null,{"$f":"+R3392","v":49.291666666666671},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(K3350,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(J3359),ABS(Y3359))","v":49.291666666666657},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(K3350,$CG$6:$CG$120,0),0)","v":19}]
[null,null,null,null,null,null,null,null,"A=",{"$f":"-Q3393","v":26.541666666666668},null,null,"KN",null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+AC3394","v":49.291666666666657},null,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sınır ve uygunluk şartları :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(K3350,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4"]
[null,null,null,null,null,null,null,null,"x = 0 ; v' = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v'' = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v = 0"]
[null,null,null,null,null,null,"v'''' =",null,{"$f":"+Y3349","v":35},null,"*","x²"," /",{"$f":"+Q3360","v":6.5},null,"² =",{"$f":"+I3370/N3370^2","v":0.82840236686390534},null,"*","x²"]
[null,null,null,null,null,null,"v' =",null,{"$f":"+I3372","v":0.82840236686390534},null,"*","x5"," /",{"$f":"+N3372*5","v":60},null,"+","C1","*","x²"," /",2,"+","C2","*","x","+","C3"]
[null,null,null,null,null,null,"x = 0 ; v' = 0",null,null,null,null,null,"C3 = 0"]
[null,null,null,null,null,null,"x = L ; v'' = 0",null,null,null,null,null,{"$f":"+I3372","v":0.82840236686390534},null,"*",{"$f":"+Q3360","v":6.5},null,"4 /",12,null,"+","C1","*",{"$f":"+P3379","v":6.5},null,"+","C2","=",0,null,null,"C1","*",{"$f":"+X3379","v":6.5},null,"+","C2","+",{"$f":"+M3379*P3379^4/S3379","v":123.22916666666667},null,null,"=",0,null,"(2.ci denklem)"]
[null,null,null,null,null,null,"iki adet denklem iki adet bilinmeyen çözülürse :"]
[null,null,null,null,null,null,"elastik eğri denklemi"]
[null,null,null,null,null,null,"x=",1,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(H3386<=Q3360,\"\",\"azalt.\")","v":""}]
[null,null,null,null,null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"Q3360*1000","v":6500},null,null," /",300,null,"=",{"$f":"+L3389/P3389","v":21.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,null,null,null,null,"Ma = E * I / 108 * ( x = 0 ) v'' =",null,null,null,null,null,null,null,null,"C2","=",{"$f":"+I3382","v":49.291666666666671},null,null,"KNm"]
[null,null,null,null,null,null,"ARA KESİT TESİRLERİ"]
[null,null,null,null,null,null,"Vx =",null,{"$f":"+I3371","v":0.82840236686390534},null,"*","x3"," /",3,null,"+","C1","=",{"$f":"+I3398","v":0.82840236686390534},null,"*",{"$f":"+H3396","v":1},null,"3 /",{"$f":"+N3398","v":3},null,"+",{"$f":"+I3381","v":-26.541666666666668},null,null,"=",{"$f":"+S3398*V3398^3/Y3398+AB3398","v":-26.265532544378701},null,null,"KN"]
[null,null,null,null,null,null,"Mmax =",null,null,{"$f":"+W3397","v":0.82840236686390534},null,"*",{"$f":"+H3400","v":0},null,"4 /",{"$f":"+AC3397","v":12},null,"+",{"$f":"+AF3397","v":-26.541666666666668},null,null,"*",{"$f":"+M3401","v":0},null,"+",{"$f":"+AM3397","v":49.291666666666671},null,null,"=",{"$f":"+J3401*M3401^4/P3401+S3401*W3401+Z3401","v":49.291666666666671},null,null,"KNm",null,null,null,null,null,null,null,{"$f":"(-I3381*N3371/I3371)^(1/3)","v":4.5807441758421801},null,{"$f":"ABS(I3372*AO3401^4/N3372+I3381*AO3401+I3382)","v":41.893772083691715},null,{"$f":"MAX(AQ3401:AR3402)","v":49.291666666666671},null,{"$f":"INDEX(AO3401:AO3402,MATCH(AS3401,AQ3401:AQ3402,0),0)","v":0}]
[null,null,null,null,null,null,"L / 2 =",null,{"$f":"+Q3360/2","v":3.25},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,{"$f":"ABS(E3354)","v":49.291666666666671}]
[null,null,null,null,null,null,"L / 4 =",null,{"$f":"+Q3360/4","v":1.625},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,null,null,null,"MC =",null,null,{"$f":"+J3405","v":0.82840236686390534},null,"*",{"$f":"+J3406","v":4.875},null,"4 /",{"$f":"+P3405","v":12},null,"+",{"$f":"+S3405","v":-26.541666666666668},null,null,"*",{"$f":"+M3407","v":4.875},null,"+",{"$f":"+Z3405","v":49.291666666666671},null,null,"=",{"$f":"+J3407*M3407^4/P3407+S3407*W3407+Z3407","v":-41.108479817708329},null,null,"KNm"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK3472","v":2.2138364779874196}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"+AA3464","v":135.55208333333326},null,null,"KNm",null,"(max moment)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(X3416,$CG$6:$CG$120,0),0)","v":10.7}]
[null,null,null,null,null,null,null,null,"x = 0 ; v' = 0",null,null,null,null,null,null,"sınır ve uygunluk şartları :"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v'' = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(X3416,$CG$6:$CG$120,0),0)","v":8360},null,null,null,"cm4"]
[null,null,"SEHİM HESABI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v = 0"]
[null,null,"v''' =",null,{"$f":"+AB3433","v":10.76923076923077},null,null,"*","x²"," /",2,"-",{"$f":"+AH3433","v":0.82840236686390534},null,null,"*","x3"," /",3,"+","C1","=",{"$f":"+E3434/K3434","v":5.384615384615385},null,null,"*","x²","-",{"$f":"+M3434/S3434","v":0.27613412228796846},null,null,"*","x3","+","C1"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"x = L ; v' = 0",null,null,null,null,null,{"$f":"+AG3436","v":0.44871794871794873},null,null,"*",{"$f":"+Q3425","v":6.5},null,"4-",{"$f":"+AM3436","v":1.3806706114398423E-2},null,null,"*",{"$f":"+M3441","v":6.5},null,"5+","C1","*",{"$f":"+T3441","v":6.5},null,"² /",2,"+","C3","=",0,null,null,"C1","*",{"$f":"+Y3441^2/AB3441","v":21.125},null,"+","C3","+",{"$f":"I3441*M3441^4-P3441*T3441^5","v":640.79166666666674},null,null,"=",0,null,"(1.ci denklem)"]
[null,null,"iki adet denklem iki adet bilinmeyen çözülürse :"]
[null,null,"C1 =",null,{"$f":"+O3444","v":-36.020833333333343},null,null,null,{"$f":"+AK3441","v":21.125},1,{"$f":"-AP3441","v":-640.79166666666674},null,{"$f":"MINVERSE(I3444:J3445)","v":7.1005917159763315E-2},-1.0923987255348202E-2,{"$f":"MMULT(M3444:N3445,K3444:K3445)","v":-36.020833333333343}]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+AM3437","v":8.9743589743589744E-2},null,null,"*","x5","-",{"$f":"+AS3437","v":2.3011176857330707E-3},null,null,"*","x6","+","C1","*","x3"," /",6,"+","C2","*","x²"," /",2,"+","C3","*","x","+","C4"]
[null,null,"y = (",null,{"$f":"+E3448","v":8.9743589743589744E-2},null,null,"*",{"$f":"+D3449","v":1},null,"5-",{"$f":"+K3448","v":2.3011176857330707E-3},null,null,"*",{"$f":"+I3450","v":1},null,"6+",{"$f":"+Q3448","v":-36.020833333333343},null,null,"*",{"$f":"+P3450","v":1},null,"3 /",6,"+",{"$f":"+Y3448","v":120.14843750000006},null,null,"*",{"$f":"+W3450","v":1},null,")* 108 / (",null,null,{"$f":"+AQ3429","v":200000},null,null,"*",{"$f":"+AQ3428","v":8360},null,null,")"]
[null,null,"y=",{"$f":"+E3451","v":6.8320818032198378},null,null,"mm",null,{"$f":"IF(ABS(D3453)<ABS(M3453),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O3452","v":21.666666666666668},null,null,"mm",null,{"$f":"IF(ABS(D3453)<ABS(M3453),\"uygun.\",\"uygun değil.\")","v":"uygun."},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-AC3434","v":-0.27613412228796846}]
[null,null,"A = E * I / 108 * ( x = L ) v''' =",null,null,null,null,null,null,null,null,{"$f":"+W3434","v":5.384615384615385},null,null,"*",{"$f":"+Q3425","v":6.5},null,"²-",{"$f":"+AC3434","v":0.27613412228796846},null,null,"*",{"$f":"+P3456","v":6.5},null,"3+",{"$f":"+E3444","v":-36.020833333333343},null,null,"=",{"$f":"+L3456*P3456^2-S3456*W3456^3+Z3456","v":115.64583333333334},null,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+E3444","v":-36.020833333333343}]
[null,null,"x=",1,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D3459<=Q3425,\"\",\"azalt.\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-2*SQRT(ABS((CA3455/CA3453-(CA3454/CA3453)*(CA3454/CA3453)/3)/3))*COS(PI()/3-(ACOS((-(CA3456/CA3453+2*CA3454^3/CA3453^3/27-(CA3454/CA3453)*(CA3455/CA3453)/3)/2/SQRT(ABS((CA3455/CA3453-(CA3454/CA3453)*(CA3454/CA3453)/3))^3/27))))/3)-CA3454/CA3453/3","v":-2.438450077995892}]
[null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"-IF((CA3456/CA3453+2*CA3454^3/CA3453^3/27-(CA3454/CA3453)*(CA3455/CA3453)/3)>0,-1,1)*SQRT(ABS((CA3455/CA3453-(CA3454/CA3453)*(CA3454/CA3453)/3)/3))-CA3454/CA3453/3","v":0}]
[null,null,"L / 2 =",null,{"$f":"+Q3425/2","v":3.25},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Q3425","v":6.5},null,{"$f":"ABS(E3419)","v":135.55208333333326},null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SANAL"]
[null,null,"MB =",null,null,{"$f":"+F3464","v":1.7948717948717949},null,null,"*",{"$f":"+E3465","v":3.25},null,"3-",{"$f":"+M3464","v":6.9033530571992116E-2},null,null,"*",{"$f":"+J3466","v":3.25},null,"4+",{"$f":"+T3464","v":-36.020833333333343},null,null,"*",{"$f":"+Q3466","v":3.25},null,"=",{"$f":"+F3466*J3466^3-M3466*Q3466^4+T3466*X3466","v":-63.1549479166667},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SANAL"]
[null,null,"MA =",null,null,{"$f":"+F3466","v":1.7948717948717949},null,null,"*",{"$f":"+E3467","v":1.625},null,"3-",{"$f":"+M3466","v":6.9033530571992116E-2},null,null,"*",{"$f":"+J3468","v":1.625},null,"4+",{"$f":"+T3466","v":-36.020833333333343},null,null,"*",{"$f":"+Q3468","v":1.625},null,"=",{"$f":"+F3468*J3468^3-M3468*Q3468^4+T3468*X3468","v":-51.313395182291686},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CA3457<0,CA3459,IF(CA3457=0,CA3462,CA3465))","v":-2.438450077995892}]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AA3464)","v":135.55208333333326},null,null," /(",2.5,null,"*",{"$f":"+H3472","v":135.55208333333326},null,null,"+",3,"*",{"$f":"ABS(AA3468)","v":51.313395182291686},null,null,"+",4,"*",{"$f":"ABS(AA3466)","v":63.1549479166667},null,null,"+",3,"*",{"$f":"ABS(AA3470)","v":6.6428222656250568},null,null,")=",{"$f":"E3472*H3472/(L3472*O3472+S3472*U3472+Y3472*AA3472+AE3472*AG3472)","v":2.2138364779874196}]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 300",null,null,null,null,null,null,null,null,15,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK3550","v":1.1556600643657295}]
[null,null,null,null,null,null,null,null,null,null,"(1.ci bölge)",null,null,null,null,null,null,null,null,null,null,null,null,null,"(2.ci bölge)"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(G3478,$CG$6:$CG$120,0),0)","v":220},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(S3477,$CG$6:$CG$120,0),0)","v":150}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( x = L ; v1' ) = ( z = 0 ; v2' )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(G3478,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(S3477,$CG$6:$CG$120,0),0)","v":8360},null,null,null,"cm4"]
[]
[null,null,"SEHİM HESABI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"z = 0 ; v2 = 0"]
[null,null,"v1 =",null,{"$f":"+E3501","v":1.1751904698255697E-3},null,null,"*","x3"," /",6,"-",{"$f":"+M3501","v":1.9005212858384015E-4},null,null,"*","x4"," /",12,null,"+","C1","*","x","+","C2"]
[null,null,"v2'' =",null,{"$f":"+E3504/N3504","v":1.2943963930806037E-2},null,null,"*(",{"$f":"+I3504","v":6.5},null,"+","z",")-",{"$f":"+R3504*U3504/AC3504","v":2.7212918660287081E-2},null,null,"*(",{"$f":"+X3504","v":3.25},null,"+","z",")+",{"$f":"+AG3504/AM3504","v":1.8216323150533679E-2},null,null,"*","z","-",{"$f":"+AQ3504/AV3504/AX3504","v":7.1770334928229664E-4},null,null,"*","z²"]
[null,null,"v2 =",null,{"$f":"+E3506","v":1.2943963930806037E-2},null,null,"*(",{"$f":"+I3506","v":6.5},null,"+","z",")3"," /",6,"-",{"$f":"+Q3506","v":2.7212918660287081E-2},null,null,"*(",{"$f":"+U3506","v":3.25},null,"+","z",")3"," /",6,"+",{"$f":"+AC3506","v":1.8216323150533679E-2},null,null,"*","z3"," /",6,"-",{"$f":"+AK3506","v":7.1770334928229664E-4},null,null,"*","z4"," /",12,null,"+","D1","*","z","+","D2"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"z = 0 ; v2' =",null,null,null,{"$f":"+E3506","v":1.2943963930806037E-2},null,null,"*",{"$f":"+I3506","v":6.5},null,"² /",2,"-",{"$f":"+Q3506","v":2.7212918660287081E-2},null,null,"*",{"$f":"+U3506","v":3.25},null,"² /",2,"+","D1","=","D1","+",{"$f":"+G3511*K3511^2/N3511-P3511*T3511^2/W3511","v":0.12972301136363637}]
[null,null,"x = L ; v1 = 0",null,null,null,null,null,{"$f":"+E3502","v":1.1751904698255697E-3},null,null,"*",{"$f":"+N3490","v":6.5},null,"3 /",6,"-",{"$f":"+M3502","v":1.9005212858384015E-4},null,null,"*",{"$f":"+M3514","v":6.5},null,"4 /",12,null,"+","C1","*",{"$f":"+V3514","v":6.5},null,"=",0,null,null,"C1","=",{"$f":"-(I3514*M3514^3/P3514-R3514*V3514^4/Y3514)/AD3514","v":-3.9258774073269624E-3},null,null,null,null,"D1","=",{"$f":"+AL3514+AD3512","v":-0.12622067870001055}]
[null,null,"y = (",null,{"$f":"+G3516","v":1.1751904698255697E-3},null,null,"*","x3"," /",6,"-",{"$f":"+O3516","v":1.9005212858384015E-4},null,null,"*","x4"," /",12,null,"+",{"$f":"+AL3514","v":-3.9258774073269624E-3},null,null,"*","x",") * 108 / ( E )"]
[null,null,"y =",null,{"$f":"(E3519*I3519^3/L3519-N3519*R3519^4/U3519+X3519*AB3519)*100000000/AG3519","v":-1.8729250032023437},null,null,"mm"]
[null,null,"2.ci bölgede elastik eğri denklemi"]
[null,null,"z=",1,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D3526<=Y3490,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E3525","v":1.2943963930806037E-2},null,null,"*(",{"$f":"+I3525","v":6.5},null,"+",{"$f":"+D3526","v":1},null,")3"," /",6,"-",{"$f":"+Q3525","v":2.7212918660287081E-2},null,null,"*(",{"$f":"+U3525","v":3.25},null,"+",{"$f":"+L3527","v":1},null,")3"," /",6,"+",{"$f":"+AC3525","v":1.8216323150533679E-2},null,null,"*",{"$f":"+Y3527","v":1},null,"3 /",6,"-",{"$f":"+AK3525","v":7.1770334928229664E-4},null,null,"*",{"$f":"+AI3527","v":1},null,"4 /",12,null,"+",{"$f":"+AT3525","v":-0.12622067870001055},null,null,"*",{"$f":"+AR3527","v":1},null,"+",{"$f":"+AZ3525","v":-0.43676127018540678},null,null,")* 108 / (",null,null,{"$f":"+AG3519","v":200000},null,null,")"]
[null,null,"y=",{"$f":"+E3528","v":0.97365437009044875},null,null,"mm",null,{"$f":"IF(ABS(D3530)<ABS(M3530),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O3529","v":10},null,null,"mm",null,{"$f":"IF(ABS(D3530)<ABS(M3530),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"1.ci bölgede"]
[null,null,"2.ci bölgede"]
[null,null,"Vx =",null,{"$f":"+E3538","v":108.21153846153847},null,null,"-",{"$f":"+O3538","v":35},null,"*",{"$f":"+R3538","v":6.5},null,"+",{"$f":"+AA3538","v":152.28846153846155},null,null,"-",{"$f":"+AH3538","v":12},null,"*",{"$f":"+AK3538","v":1},null,"=",{"$f":"+E3539-I3539*L3539+O3539-S3539*V3539","v":21.000000000000014},null,null,"KN"]
[null,null,"Mmax =",null,null,{"$f":"+E3534","v":108.21153846153847},null,null,"*",{"$f":"+D3541","v":3.0917582417582419},null,"-",{"$f":"+L3534","v":35},null,"*",{"$f":"+J3542","v":3.0917582417582419},null,"² /",2,"=",{"$f":"+F3542*J3542-M3542*P3542^2/S3542","v":167.28195794590027},null,null,"KNm",null,null,null,{"$f":"F3489/M3479","v":3.0917582417582419},null,{"$f":"F3489*AB3542-M3479*AB3542^2/2","v":167.28195794590027},null,{"$f":"MAX(AD3542:AE3543)","v":167.28195794590027},null,{"$f":"INDEX(AB3542:AB3543,MATCH(AF3542,AD3542:AD3543,0),0)","v":3.0917582417582419}]
[null,null,"L / 4 =",null,{"$f":"+N3490/4","v":1.625},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,"MA =",null,{"$f":"+E3544","v":108.21153846153847},null,null,"*",{"$f":"+E3545","v":1.625},null,"-",{"$f":"+L3544","v":35},null,"*",{"$f":"+I3546","v":1.625},null,"² /",2,"=",{"$f":"+E3546*I3546-L3546*O3546^2/R3546","v":129.6328125},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,"MC =",null,{"$f":"+E3546","v":108.21153846153847},null,null,"*",{"$f":"+F3547","v":4.875},null,"-",{"$f":"+L3546","v":35},null,"*",{"$f":"+I3548","v":4.875},null,"² /",2,"=",{"$f":"+E3548*I3548-L3548*O3548^2/R3548","v":111.6328125},null,null,"KNm"]
[]
[null,null,null,null,null,null,null,null,10,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,"KN",null,null,null,null,null,null,null,"(1.ci bölge) sol konsol kiriş enkesiti",null,null,null,null,null,null,null,null,null,null,null,"(2.ci bölge) açıklık kiriş enkesiti",null,null,null,null,null,null,null,null,null,null,"(3.cü bölge) sağ konsol kiriş enkesiti"]
[null,null,null,null,null,null,null,null,null,null,8,null,"KN/m",null,null,null,null,null,null,null,null,35,null,"KN/m",null,null,null,null,null,null,null,null,12,null,"KN/m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(C3565,$CG$6:$CG$120,0),0)","v":300},null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(P3556,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(AM3565,$CG$6:$CG$120,0),0)","v":200}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,null,null,"z",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(C3565,$CG$6:$CG$120,0),0)","v":8360},null,null,null,"cm4",null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(P3556,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4",null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(AM3565,$CG$6:$CG$120,0),0)","v":1940},null,null,null,"cm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kirişlerin elastisite modülü)"]
[null,null,null,null,null,null,null,null,null,null,null,"( x = L ; v1' ) = ( z = 0 ; v2' )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( z = L ; v2' ) = ( m = 0 ; v3' )"]
[null,null,null,null,null,null,null,null,null,null,null,"( x = L ; v1 ) = ( z = 0 ; v2 ) = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( z = L ; v2 ) = ( m = 0 ; v3 ) = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AK3651","v":1.1645268748069091}]
[null,null,"v1'' =",null,{"$f":"-I3555","v":-10},null,"*","x"," /",{"$f":"+AY3569","v":8360},null,null,"-",{"$f":"+K3557","v":8},null,"*","x²"," /",2," /",{"$f":"+J3578","v":8360},null,null,"=",{"$f":"+E3578/J3578","v":-1.1961722488038277E-3},null,null,"*","x","-",{"$f":"+N3578/S3578/U3578","v":4.7846889952153111E-4},null,null,"*","x²",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+I3555","v":10},{"$f":"+BD3578+K3557*L3568","v":20},{"$f":"+BE3578-O3567","v":-111.09615384615384},{"$f":"+BF3578+V3557*W3568","v":116.40384615384616},{"$f":"+BG3578-AE3567","v":-33},{"$f":"+BH3578+AG3557*AH3568","v":-15}]
[null,null,"2.ci bölgede :"]
[null,null,"v2 =",null,{"$f":"+E3584","v":-1.0860121633362293E-4},null,null,"*(",{"$f":"+I3584","v":1.25},null,"+","z",")3"," /",6,"-",{"$f":"+Q3584","v":1.0860121633362293E-4},null,null,"*(",{"$f":"+U3584","v":0.625},null,"+","z",")3"," /",6,"+",{"$f":"+AC3584","v":1.4237201764352068E-3},null,null,"*","z3"," /",6,"-",{"$f":"+AK3584","v":1.9005212858384015E-4},null,null,"*","z4"," /",12,null,"+","D1","*","z","+","D2"]
[null,null,"v3'' =",null,{"$f":"-I3555","v":-10},null,"*(",{"$f":"+L3568+W3568","v":7.75},null,"+","m",")/",{"$f":"+BV3569","v":1940},null,null,"-",{"$f":"+K3557","v":8},null,"*",{"$f":"+L3568","v":1.25},null,"*(",{"$f":"+L3568/2+W3568","v":7.125},null,"+","m",")/",{"$f":"+M3587","v":1940},null,null,"+",{"$f":"+O3567","v":131.09615384615384},null,"*(",{"$f":"+W3568","v":6.5},null,"+","m",")/",{"$f":"+AB3587","v":1940},null,null,"-",{"$f":"+V3557","v":35},null,"*",{"$f":"+W3568","v":6.5},null,"*(",{"$f":"+W3568/2","v":3.25},null,"+","m",")/",{"$f":"+AN3587","v":1940},null,null,"+",{"$f":"+AE3567","v":149.40384615384616},null,"*","m"," /",{"$f":"+BC3587","v":1940},null,null,"-",{"$f":"+AG3557","v":12},null,"*","m²"," /",2," /",{"$f":"+BL3587","v":1940}]
[null,null,"v3 =",null,{"$f":"+E3589","v":-5.1546391752577319E-3},null,null,"*(",{"$f":"+I3589","v":7.75},null,"+","m",")3"," /",6,"-",{"$f":"+Q3589","v":5.1546391752577319E-3},null,null,"*(",{"$f":"+U3589","v":7.125},null,"+","m",")3"," /",6,"+",{"$f":"+AC3589","v":6.7575337034099917E-2},null,null,"*(",{"$f":"+AG3589","v":6.5},null,"+","m",")3"," /",6,"-",{"$f":"+AO3589","v":0.1172680412371134},null,null,"*(",{"$f":"+AS3589","v":3.25},null,"+","m",")3"," /",6,"+",{"$f":"+BA3589","v":7.7012291831879465E-2},null,null,"*","m3"," /",6,"-",{"$f":"+BI3589","v":3.092783505154639E-3},null,null,"*","m4"," /",12,null,"+","E1","*","m","+","E2"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"z = L ; v2 = 0",null,null,null,null,null,{"$f":"+E3585","v":-1.0860121633362293E-4},null,null,"*(",{"$f":"+I3585","v":1.25},null,"+",{"$f":"+W3568","v":6.5},null,")3"," /",6,"-",{"$f":"+Q3585","v":1.0860121633362293E-4},null,null,"*(",{"$f":"+U3585","v":0.625},null,"+",{"$f":"+P3594","v":6.5},null,")3"," /",6,"+",{"$f":"+AC3585","v":1.4237201764352068E-3},null,null,"*",{"$f":"+AC3594","v":6.5},null,"3 /",6,"-",{"$f":"+AK3585","v":1.9005212858384015E-4},null,null,"*",{"$f":"+AM3594","v":6.5},null,"4 /",12,null,"+","D1","*",{"$f":"+AV3594","v":6.5},null,"+","D2","=",0]
[null,null,"x = L ; v1' =",null,null,null,{"$f":"+W3579","v":-5.9808612440191385E-4},null,null,"*",{"$f":"+L3568","v":1.25},null,"²-",{"$f":"+AC3579","v":1.594896331738437E-4},null,null,"*",{"$f":"+K3597","v":1.25},null,"3+","C1","=","C1","+",{"$f":"G3597*K3597^2-N3597*R3597^3","v":-1.246012759170654E-3}]
[null,null,"z = L ; v2' =",null,null,null,{"$f":"+E3584","v":-1.0860121633362293E-4},null,null,"*(",{"$f":"+I3584","v":1.25},null,"+",{"$f":"+W3568","v":6.5},null,")²"," /",2,"-",{"$f":"+Q3584","v":1.0860121633362293E-4},null,null,"*(",{"$f":"+U3584","v":0.625},null,"+",{"$f":"+N3600","v":6.5},null,")²"," /",2,"+",{"$f":"+AC3584","v":1.4237201764352068E-3},null,null,"*",{"$f":"+AA3600","v":6.5},null,"² /",2,"-",{"$f":"+AK3584","v":1.9005212858384015E-4},null,null,"*",{"$f":"+AK3600","v":6.5},null,"3 /",3,"+","D1","=","D1","+",{"$f":"G3600*(K3600+N3600)^2/R3600-T3600*(X3600+AA3600)^2/AE3600+AG3600*AK3600^2/AN3600-AP3600*AT3600^3/AW3600","v":6.6603655335939725E-3}]
[null,null,"1.ci bölgede elastik eğri denklemi"]
[null,null,"x=",0,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D3606<=L3568,\"\",\"azalt.\")","v":""}]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"N3578*1000","v":8000},null,null," /",150,null,"=",{"$f":"+H3609/L3609","v":53.333333333333336},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E3608","v":1.6425319962761216},null,null,"mm",null,{"$f":"IF(ABS(D3610)<ABS(M3610),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O3609","v":53.333333333333336},null,null,"mm",null,{"$f":"IF(ABS(D3610)<ABS(M3610),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"E / 108 * y =",null,null,null,{"$f":"+E3585","v":-1.0860121633362293E-4},null,null,"*(",{"$f":"+I3585","v":1.25},null,"+","z",")3"," /",6,"-",{"$f":"+Q3585","v":1.0860121633362293E-4},null,null,"*(",{"$f":"+U3585","v":0.625},null,"+","z",")3"," /",6,"+",{"$f":"+AC3585","v":1.4237201764352068E-3},null,null,"*","z3"," /",6,"-",{"$f":"+AK3585","v":1.9005212858384015E-4},null,null,"*","z4"," /",12,null,"+","D1","*","z","+","D2"]
[null,null,"y = (",null,{"$f":"+E3613","v":-1.0860121633362293E-4},null,null,"*(",{"$f":"+I3613","v":1.25},null,"+",{"$f":"+D3614","v":1},null,")3"," /",6,"-",{"$f":"+Q3613","v":1.0860121633362293E-4},null,null,"*(",{"$f":"+U3613","v":0.625},null,"+",{"$f":"+L3615","v":1},null,")3"," /",6,"+",{"$f":"+AC3613","v":1.4237201764352068E-3},null,null,"*",{"$f":"+Y3615","v":1},null,"3 /",6,"-",{"$f":"+AK3613","v":1.9005212858384015E-4},null,null,"*",{"$f":"+AI3615","v":1},null,"4 /",12,null,"+",{"$f":"+AT3613","v":-3.3786290906458153E-3},null,null,"*",{"$f":"+AR3615","v":1},null,"+",{"$f":"+AZ3613","v":3.9770953247176365E-5},null,null,")* 108 / (",null,null,{"$f":"+AF3607","v":200000},null,null,")"]
[null,null,"3.ci bölgede elastik eğri denklemi"]
[null,null,"y = (",null,{"$f":"+G3620","v":-5.1546391752577319E-3},null,null,"*(",{"$f":"+K3620","v":7.75},null,"+","m",")3"," /",6,"-",{"$f":"+S3620","v":5.1546391752577319E-3},null,null,"*(",{"$f":"+W3620","v":7.125},null,"+","m",")3"," /",6,"+",{"$f":"+AE3620","v":6.7575337034099917E-2},null,null,"*(",{"$f":"+AI3620","v":6.5},null,"+","m",")3"," /",6,"-",{"$f":"+AQ3620","v":0.1172680412371134},null,null,"*(",{"$f":"+AU3620","v":3.25},null,"+","m",")3"," /",6,"+",{"$f":"+BC3620","v":7.7012291831879465E-2},null,null,"*","m3"," /",6,"-",{"$f":"+BK3620","v":3.092783505154639E-3},null,null,"*","m4"," /",12,"+",{"$f":"+AM3602","v":-0.51928591819622705},null,null,"*","m","+",{"$f":"+AZ3596","v":-1.7114036324097937},null,null,") * 108 / ( E )"]
[null,null,null,null,"*",{"$f":"+BR3623","v":1.5},null,"+",{"$f":"+BW3621","v":-1.7114036324097937},null,null,")* 108 / (",null,null,{"$f":"+BK3615","v":200000},null,null,")"]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"AH3568*1000","v":1500},null,null," /",150,null,"=",{"$f":"+H3626/L3626","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"x=",1,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D3630<=L3568,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+E3578","v":-10},null,"*",{"$f":"+D3630","v":1},null,"-",{"$f":"+N3578","v":8},null,"*",{"$f":"+D3630","v":1},null,"² /",2,"=",{"$f":"+E3631*H3631-K3631*N3631^2/Q3631","v":-14},null,null,"KNm"]
[null,null,"Mx =",null,{"$f":"+E3582","v":-10},null,"*(",{"$f":"+H3582","v":1.25},null,"+",{"$f":"+D3634","v":1},null,")-",{"$f":"+Q3582","v":8},null,"*",{"$f":"+T3582","v":1.25},null,"*(",{"$f":"+W3582","v":0.625},null,"+",{"$f":"+K3635","v":1},null,")+",{"$f":"+AF3582","v":131.09615384615384},null,null,"*",{"$f":"+W3635","v":1},null,"-",{"$f":"+AO3582","v":35},null,"*",{"$f":"+AD3635","v":1},null,"² /",2,"=",{"$f":"+E3635*(H3635+K3635)-N3635*Q3635*(T3635+W3635)+Z3635*AD3635-AG3635*AJ3635^2/AM3635","v":74.84615384615384},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+E3635","v":-10},null,"-",{"$f":"+N3635","v":8},null,"*",{"$f":"+Q3635","v":1.25},null,"+",{"$f":"+Z3635","v":131.09615384615384},null,null,"-",{"$f":"+AG3635","v":35},null,"*",{"$f":"+AJ3635","v":1},null,"=",{"$f":"+E3636-H3636*K3636+N3636-R3636*U3636","v":76.09615384615384},null,null,"KN"]
[null,null,"Vx =",null,{"$f":"+E3639","v":-10},null,"-",{"$f":"+N3639","v":8},null,"*",{"$f":"+Q3639","v":1.25},null,"+",{"$f":"+Z3639","v":131.09615384615384},null,null,"-",{"$f":"+AJ3639","v":35},null,"*",{"$f":"+AM3639","v":6.5},null,"+",{"$f":"+AV3639","v":149.40384615384616},null,null,"-",{"$f":"+BC3639","v":12},null,"*",{"$f":"+BF3639","v":1},null,"=",{"$f":"+E3640-H3640*K3640+N3640-R3640*U3640+X3640-AB3640*AE3640","v":21},null,null,"KN"]
[null,null,"z=",{"$f":"+BC3643","v":3.174175824175824},null,null,"m. ' deki max moment miktarı"]
[null,null,"MB =",null,null,{"$f":"+F3643","v":-10},null,"*(",{"$f":"+I3643","v":1.25},null,"+",{"$f":"+E3644","v":3.25},null,")-",{"$f":"+O3643","v":8},null,"*",{"$f":"+R3643","v":1.25},null,"*(",{"$f":"+U3643","v":0.625},null,"+",{"$f":"+L3645","v":3.25},null,")+",{"$f":"+AA3643","v":131.09615384615384},null,null,"*",{"$f":"+X3645","v":3.25},null,"-",{"$f":"+AH3643","v":35},null,"*",{"$f":"+AE3645","v":3.25},null,"² /",2,"=",{"$f":"+F3645*(I3645+L3645)-O3645*R3645*(U3645+X3645)+AA3645*AE3645-AH3645*AK3645^2/AN3645","v":157.46875},null,null,"KNm",null,null,null,{"$f":"+W3568","v":6.5},null,{"$f":"ABS(AK3555*AH3568+AG3557*AH3568*AH3568/2)","v":36},null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,"MC =",null,null,{"$f":"+F3647","v":-10},null,"*(",{"$f":"+I3647","v":1.25},null,"+",{"$f":"+F3648","v":4.875},null,")-",{"$f":"+O3647","v":8},null,"*",{"$f":"+R3647","v":1.25},null,"*(",{"$f":"+U3647","v":0.625},null,"+",{"$f":"+L3649","v":4.875},null,")+",{"$f":"+AA3647","v":131.09615384615384},null,null,"*",{"$f":"+X3649","v":4.875},null,"-",{"$f":"+AH3647","v":35},null,"*",{"$f":"+AE3649","v":4.875},null,"² /",2,"=",{"$f":"+F3649*(I3649+L3649)-O3649*R3649*(U3649+X3649)+AA3649*AE3649-AH3649*AK3649^2/AN3649","v":106.9453125},null,null,"KNm"]
[null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AP3643)","v":157.56936284868971},null,null," /(",2.5,null,"*",{"$f":"+H3651","v":157.56936284868971},null,null,"+",3,"*",{"$f":"ABS(AP3647)","v":115.5703125},null,null,"+",4,"*",{"$f":"ABS(AP3645)","v":157.46875},null,null,"+",3,"*",{"$f":"ABS(AP3649)","v":106.9453125},null,null,")=",{"$f":"E3651*H3651/(L3651*O3651+S3651*U3651+Y3651*AA3651+AE3651*AG3651)","v":1.1645268748069091}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,"Ma =",null,{"$f":"-F3686","v":86.260416666666629},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(K3657,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(J3666),ABS(Y3666))","v":62.562500000000014},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"x"]
[null,null,null,null,null,null,null,null,"A=",{"$f":"+F3687","v":51.187499999999986},null,null,"KN",null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+U3689","v":62.562500000000014},null,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",6.5,null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(K3657,$CG$6:$CG$120,0),0)","v":220}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sınır ve uygunluk şartları :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(K3657,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4"]
[null,null,null,null,null,null,null,null,"x = 0 ; v' = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v'' = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[]
[]
[null,null,null,null,null,null,null,null,"x = 0 ; v = 0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v = 0"]
[null,null,null,"SEHİM HESABI"]
[null,null,null,"v'' =",null,"Ma +",null,"A","*","x","-","q","*","x"," /",{"$f":"+Q3667","v":6.5},null,"*","x"," /",2,"*","x"," /",3,"=","Ma +",null,"A","*","x","-","q","*","x3","*",{"$f":"1/(P3677*U3677*Y3677)","v":2.564102564102564E-2},null,null,"=","Ma +",null,"A","*","x","-",{"$f":"+Y3656","v":35},null,"*","x3","*",{"$f":"+AK3677","v":2.564102564102564E-2},null,null,"=","Ma +",null,"A","*","x","-",{"$f":"+AU3677*AZ3677","v":0.89743589743589736},null,null,"*","x3"]
[null,null,null,"v' =",null,"Ma *",null,"x","+","A","*","x²"," /",2,"-",{"$f":"+BJ3677","v":0.89743589743589736},null,null,"*","x4"," /",4,"+","C1"]
[null,null,null,"v =",null,"Ma *",null,"x²"," /",2,"+","A","*","x3"," /",6,"-",{"$f":"+P3678","v":0.89743589743589736},null,null,"*","x5"," /",20,null,"+","C1","*","x","+","C2"]
[null,null,null,"sınır ve uygunluk şartları :"]
[null,null,null,"x = 0 ; v = 0",null,null,null,null,null,"C2 = 0"]
[null,null,null,"x = 0 ; v' = 0",null,null,null,null,null,"C1 = 0"]
[null,null,null,"x = L ; v = 0",null,null,null,null,null,"Ma *",null,{"$f":"+Q3667","v":6.5},null,"² /",2,"+","A","*",{"$f":"+L3683","v":6.5},null,"3 /",6,"-",{"$f":"+R3679","v":0.89743589743589736},null,null,"*",{"$f":"+S3683","v":6.5},null,"5 /",20,null,"=",0,null,null,"Ma *",null,{"$f":"+L3683^2/O3683","v":21.125},null,"+","A","*",{"$f":"+S3683^3/V3683","v":45.770833333333336},null,"-",{"$f":"+X3683*AB3683^5/AE3683","v":520.64322916666663},null,null,"=",0,null,"1.ci denklem"]
[null,null,null,"x = L ; v'' = 0",null,null,null,null,null,"Ma +",null,"A","*",{"$f":"+Q3667","v":6.5},null,"-",{"$f":"+BJ3677","v":0.89743589743589736},null,null,"*",{"$f":"+N3684","v":6.5},null,"3=","Ma +",null,"A","*",{"$f":"+N3684","v":6.5},null,"-",{"$f":"+Q3684*U3684^3","v":246.45833333333331},null,null,"=",0,null,"2.ci denklem"]
[null,null,null,"iki adet denklem iki adet bilinmeyen çözülürse :"]
[null,null,null,"Ma =",null,{"$f":"+R3686","v":-86.260416666666629},null,null,null,null,{"$f":"+AM3683","v":21.125},{"$f":"+AR3683","v":45.770833333333336},{"$f":"+AU3683","v":520.64322916666663},null,null,{"$f":"MINVERSE(K3686:L3687)","v":7.1005917159763315E-2},-0.49999999999999989,{"$f":"MMULT(P3686:Q3687,M3686:M3687)","v":-86.260416666666629}]
[null,null,null,"A =",null,{"$f":"+R3687","v":51.187499999999986},null,null,null,null,1,{"$f":"+AB3684","v":6.5},{"$f":"+AE3684","v":246.45833333333331},null,null,-1.0923987255348201E-2,0.23076923076923073,51.187499999999986]
[null,null,null,"düşey denge denkleminden"]
[null,null,null,"A","+","B","-",{"$f":"+Y3656","v":35},null,"*",{"$f":"+Q3667","v":6.5},null," /",2,"=",0,null,null,"B","=",{"$f":"+H3689*K3689/N3689-F3687","v":62.562500000000014}]
[null,null,null,"elastik eğri denklemi"]
[null,null,null,"E * I / 108 * y =",null,null,null,null,"Ma *",null,"x²"," /",2,"+","A","*","x3"," /",6,"-",{"$f":"+R3679","v":0.89743589743589736},null,null,"*","x5"," /",20,null,"+","C1","*","x","+","C2"]
[null,null,null,"y = (",null,{"$f":"+F3686","v":-86.260416666666629},null,null,"*","x²"," /",2,"+",{"$f":"+F3687","v":51.187499999999986},null,null,"*","x3"," /",6,"-",{"$f":"+U3691","v":0.89743589743589736},null,null,"*","x5"," /",20,null,") * 108 / ( E * I )"]
[null,null,null,"x=",1,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(E3693<=Q3667,\"\",\"azalt.\")","v":""}]
[null,null,null,"y = (",null,{"$f":"+F3692","v":-86.260416666666629},null,null,"*",{"$f":"+E3693","v":1},null,"² /",2,"+",{"$f":"+N3692","v":51.187499999999986},null,null,"*",{"$f":"+J3694","v":1},null,"3 /",6,"-",{"$f":"+V3692","v":0.89743589743589736},null,null,"*",{"$f":"+S3694","v":1},null,"5 /",20,null,")* 108 / (",null,null,{"$f":"+AQ3671","v":200000},null,null,"*",{"$f":"+AQ3670","v":92080},null,null,")"]
[null,null,null,"y =",null,{"$f":"(F3694*J3694^2/M3694+O3694*S3694^3/V3694-X3694*AB3694^5/AE3694)*100000000/(AJ3694*AN3694)","v":-0.18811810451892436},null,null,"mm"]
[null,null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"Q3667*1000","v":6500},null,null," /",300,null,"=",{"$f":"+I3696/M3696","v":21.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,null,"y=",{"$f":"+F3695","v":-0.18811810451892436},null,null,"mm",null,{"$f":"IF(ABS(E3697)<ABS(N3697),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+P3696","v":21.666666666666668},null,null,"mm",null,{"$f":"IF(ABS(E3697)<ABS(N3697),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,null,"ARA KESİT TESİRLERİ"]
[null,null,null,"x=",1,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(E3699<=Q3667,\"\",\"azalt.\")","v":""}]
[null,null,null,"Mx =",null,"Ma +",null,"A","*","x","-",{"$f":"+BJ3677","v":0.89743589743589736},null,null,"*","x3","=",{"$f":"+F3686","v":-86.260416666666629},null,null,"+",{"$f":"+F3687","v":51.187499999999986},null,null,"*",{"$f":"+E3699","v":1},null,"-",{"$f":"+L3700","v":0.89743589743589736},null,null,"*",{"$f":"+E3699","v":1},null,"3=",{"$f":"R3700+V3700*Z3700-AC3700*AG3700^3","v":-35.970352564102541},null,null,"KNm"]
[null,null,null,"Vx =",null,{"$f":"+V3700","v":51.187499999999986},null,null,"-",{"$f":"+Y3656","v":35},null,"*",{"$f":"+E3699","v":1},null," /",{"$f":"+Q3667","v":6.5},null,"*",{"$f":"+E3699","v":1},null," /",2,"=",{"$f":"+F3701-J3701*M3701/P3701*S3701/V3701","v":48.495192307692292},null,null,"KN"]
[null,null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,null,"x=",{"$f":"+AM3704","v":0},null,null,"m. ' deki max moment miktarı"]
[null,null,null,"Mmax =",null,null,{"$f":"+R3700","v":-86.260416666666629},null,null,"+",{"$f":"+V3700","v":51.187499999999986},null,null,"*",{"$f":"+E3703","v":0},null,"-",{"$f":"+AC3700","v":0.89743589743589736},null,null,"*",{"$f":"+O3704","v":0},null,"3=",{"$f":"+G3704+K3704*O3704-R3704*V3704^3","v":-86.260416666666629},null,null,"KNm",null,null,null,null,{"$f":"SQRT(J3666*2*Q3667/Y3656)","v":4.3603325561245887},null,{"$f":"ABS(F3686+F3687*AG3704-BJ3677*AG3704^3)","v":62.535931811084936},null,{"$f":"MAX(AI3704:AJ3705)","v":86.260416666666629},null,{"$f":"INDEX(AG3704:AG3705,MATCH(AK3704,AI3704:AI3705,0),0)","v":0}]
[null,null,null,"L / 2 =",null,{"$f":"+Q3667/2","v":3.25},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,{"$f":"ABS(E3661)","v":86.260416666666629}]
[null,null,null,"MB =",null,{"$f":"+G3704","v":-86.260416666666629},null,null,"+",{"$f":"+K3704","v":51.187499999999986},null,null,"*",{"$f":"+F3705","v":3.25},null,"-",{"$f":"+R3704","v":0.89743589743589736},null,null,"*",{"$f":"+N3706","v":3.25},null,"3=",{"$f":"+F3706+J3706*N3706-Q3706*U3706^3","v":49.29166666666665},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,"L / 4 =",null,{"$f":"+Q3667/4","v":1.625},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,"MA =",null,{"$f":"+F3706","v":-86.260416666666629},null,null,"+",{"$f":"+J3706","v":51.187499999999986},null,null,"*",{"$f":"+F3707","v":1.625},null,"-",{"$f":"+Q3706","v":0.89743589743589736},null,null,"*",{"$f":"+N3708","v":1.625},null,"3=",{"$f":"+F3708+J3708*N3708-Q3708*U3708^3","v":-6.9316406249999902},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,"3 * L / 4 =",null,null,{"$f":"3*Q3667/4","v":4.875},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,"MC =",null,{"$f":"+F3708","v":-86.260416666666629},null,null,"+",{"$f":"+J3708","v":51.187499999999986},null,null,"*",{"$f":"+G3709","v":4.875},null,"-",{"$f":"+Q3708","v":0.89743589743589736},null,null,"*",{"$f":"+N3710","v":4.875},null,"3=",{"$f":"+F3710+J3710*N3710-Q3710*U3710^3","v":59.304036458333329},null,null,"KNm"]
[null,null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(Y3704)","v":86.260416666666629},null,null," /(",2.5,null,"*",{"$f":"+I3712","v":86.260416666666629},null,null,"+",3,"*",{"$f":"ABS(X3708)","v":6.9316406249999902},null,null,"+",4,"*",{"$f":"ABS(X3706)","v":49.29166666666665},null,null,"+",3,"*",{"$f":"ABS(X3710)","v":59.304036458333329},null,null,")=",{"$f":"F3712*I3712/(M3712*P3712+T3712*V3712+Z3712*AB3712+AF3712*AH3712)","v":1.7632241813602012}]
[]
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK KONSOL KİRİŞ SEHİM HESABI (değişken kesit)\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2. bölge kiriş enkesiti",null,null,null,null,null,null,null,null,null,"1. bölge kiriş enkesiti"]
[null,null,null,null,null,null,"(moment diyagramı)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AT3721","v":264.375},null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,35,null,"KN/m"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AA3717*AI3730+AH3718*AI3730*AI3730/2","v":264.375},null,"KNm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(AC3725,$CG$6:$CG$120,0),0)","v":300},null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(AK3725,$CG$6:$CG$120,0),0)","v":600}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(AC3725,$CG$6:$CG$120,0),0)","v":7.1},null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(AK3725,$CG$6:$CG$120,0),0)","v":12}]
[null,null,null,null,null,null,null,"(kesme kuvveti diyagramı)"]
[null,null,{"$f":"+AQ3727","v":202.5},null,"KN",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+AQ3727","v":202.5},null,"KN",null,null,null,null,null,null,null,"IPE 300",null,null,null,null,null,null,null,"IPE 600"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"z",null,null,null,null,null,null,null,"x",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(AC3725,$CG$6:$CG$120,0),0)","v":10.7},null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(AK3725,$CG$6:$CG$120,0),0)","v":19}]
[null,null,null,null,null,null,null,null,null,null,null,"+",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(2.ci bölge)",null,null,null,null,null,null,null,null,"(1.ci bölge)",null,null,null,"A=",{"$f":"+AA3717+AH3718*AI3730","v":202.5},null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.8,null,"m",null,null,null,null,null,{"$f":"+AI3730-AE3728","v":0.7},null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(AC3725,$CG$6:$CG$120,0),0)","v":150},null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(AK3725,$CG$6:$CG$120,0),0)","v":220}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(AC3725,$CG$6:$CG$120,0),0)","v":8360},null,null,null,"cm4",null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(AK3725,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4"]
[null,null,"SEHİM HESABI",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,"Mx1 = -Ma + A * x =",null,null,null,null,null,{"$f":"-AT3721","v":-264.375},null,"+",{"$f":"+AQ3727","v":202.5},null,"*","x","-",{"$f":"+AH3718","v":35},null,"*","x²"," /",2,null,"(1.ci bölge)"]
[null,null,"Mx2 =",null," -Ma+",null,"A","*(",{"$f":"+AM3728","v":0.7},null,"+","z",")-",{"$f":"+AH3718","v":35},null,"*",{"$f":"+AM3728","v":0.7},null,"*(",{"$f":"+AM3728/2","v":0.35},null,"+","z",")-",{"$f":"+AH3718","v":35},null,"*","z²"," /",2,"=",{"$f":"-AT3721","v":-264.375},null,"+",{"$f":"+AQ3727","v":202.5},null,"*(",{"$f":"+I3734","v":0.7},null,"+","z",")-",{"$f":"+N3734*Q3734","v":24.5},null,"*(",{"$f":"+T3734","v":0.35},null,"+","z",")-",{"$f":"+Y3734","v":35},null,"*","z²"," /",2]
[null,null,"Mx2 =",null,{"$f":"+AF3734","v":-264.375},null,"+",{"$f":"+AI3734*AL3734","v":141.75},null,"+",{"$f":"+AI3734","v":202.5},null,"*","z","-",{"$f":"+AQ3734*AT3734","v":8.5749999999999993},null,"-",{"$f":"+AQ3734","v":24.5},null,"*","z","-",{"$f":"+AY3734","v":35},null,"*","z²"," /",2,"=",{"$f":"+E3735+H3735-P3735","v":-131.19999999999999},null,"+",{"$f":"+K3735-S3735","v":178},null,"*","z","-",{"$f":"+X3735","v":35},null,"*","z²"," /",2,null,"(2.ci bölge)"]
[null,null,"1.ci bölgede :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"moment aktaran profil birleşimleri "]
[null,null,"v1'' =",null,{"$f":"+L3733","v":202.5},null,"*","x"," /",{"$f":"+BM3731","v":92080},null,null,null,"+",{"$f":"+I3733","v":-264.375},null," /",{"$f":"+J3737","v":92080},null,null,null,"-",{"$f":"+Q3733","v":35},null,"*","x²"," /",2," /",{"$f":"+R3737","v":92080},null,null,null,"=",{"$f":"-W3737/AB3737/AD3737","v":-1.9005212858384015E-4},null,null,"*","x²","+",{"$f":"+E3737/J3737","v":2.1991746307558646E-3},null,null,"*","x","+",{"$f":"+O3737/R3737","v":-2.8711446568201564E-3}]
[null,null,"v1' =",null,{"$f":"+AI3737","v":-1.9005212858384015E-4},null,null,"*","x3"," /",3,"+",{"$f":"+AO3737","v":2.1991746307558646E-3},null,null,"*","x²"," /",2,"+",{"$f":"+AU3737","v":-2.8711446568201564E-3},null,null,"*","x","+","C1"]
[null,null,"v1 =",null,{"$f":"+E3738","v":-1.9005212858384015E-4},null,null,"*","x4"," /",12,null,"+",{"$f":"+M3738","v":2.1991746307558646E-3},null,null,"*","x3"," /",6,"+",{"$f":"+U3738","v":-2.8711446568201564E-3},null,null,"*","x²"," /",2,"+","C1","*","x","+","C2"]
[null,null,"2.ci bölgede :"]
[null,null,"v2'' =",null,{"$f":"-AM3735","v":-35},null,"*","z²"," /",2," /",{"$f":"+BB3731","v":8360},null,null,null,"+",{"$f":"+AH3735","v":178},null,"*","z"," /",{"$f":"+L3741","v":8360},null,null,null,"+",{"$f":"+AE3735","v":-131.19999999999999},null," /",{"$f":"+V3741","v":8360},null,null,null,"=",{"$f":"+E3741/J3741/L3741","v":-2.0933014354066986E-3},null,null,"*","z²","+",{"$f":"+Q3741/V3741","v":2.1291866028708133E-2},null,null,"*","z","+",{"$f":"+AA3741/AD3741","v":-1.5693779904306218E-2}]
[null,null,"v2' =",null,{"$f":"+AI3741","v":-2.0933014354066986E-3},null,null,"*","z3"," /",3,"+",{"$f":"+AO3741","v":2.1291866028708133E-2},null,null,"*","z²"," /",2,"+",{"$f":"+AU3741","v":-1.5693779904306218E-2},null,null,"*","z","+","D1"]
[null,null,"v2 =",null,{"$f":"+E3742","v":-2.0933014354066986E-3},null,null,"*","z4"," /",12,null,"+",{"$f":"+M3742","v":2.1291866028708133E-2},null,null,"*","z3"," /",6,"+",{"$f":"+U3742","v":-1.5693779904306218E-2},null,null,"*","z²"," /",2,"+","D1","*","z","+","D2"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"x = 0 ; v1' = 0",null,null,null,null,null,"C1 = 0"]
[null,null,"x = 0 ; v1 = 0",null,null,null,null,null,"C2 = 0"]
[null,null,"x = L ; v1' =",null,null,null,{"$f":"+E3738","v":-1.9005212858384015E-4},null,null,"*",{"$f":"+AM3728","v":0.7},null,"3 /",6,"+",{"$f":"+M3738","v":2.1991746307558646E-3},null,null,"*",{"$f":"+AM3728","v":0.7},null,"² /",2,"+",{"$f":"+U3738","v":-2.8711446568201564E-3},null,null,"*",{"$f":"+T3747","v":0.7},null,"=",{"$f":"G3747*K3747^3/N3747+P3747*T3747^2/W3747+Y3747*AC3747","v":-1.4818681219229653E-3}]
[null,null,"z = 0 ; v2' =",null,null,null,"D1"]
[null,null,"( x = L ; v1' ) = ( x = L ; v2' )",null,null,null,null,null,null,null,null,null,"D1","=",{"$f":"+AF3747","v":-1.4818681219229653E-3}]
[null,null,"x = L ; v1 =",null,null,null,{"$f":"+E3739","v":-1.9005212858384015E-4},null,null,"*",{"$f":"+AM3728","v":0.7},null,"4 /",24,null,"+",{"$f":"+N3739","v":2.1991746307558646E-3},null,null,"*",{"$f":"+AM3728","v":0.7},null,"3/",6,"+",{"$f":"+V3739","v":-2.8711446568201564E-3},null,null,"*",{"$f":"+U3750","v":0.7},null,"² /",2,"=",{"$f":"G3750*K3750^4/N3750+Q3750*U3750^3/X3750+Z3750*AD3750^2/AG3750","v":-5.796122710324355E-4}]
[null,null,"z = 0 ; v2 =",null,null,null,"D2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca konsol kirişte Cb = 1 alınır."]
[null,null,"( x = L ; v1 ) = ( z = 0 ; v2 )",null,null,null,null,null,null,null,null,null,"D2","=",{"$f":"+AI3750","v":-5.796122710324355E-4}]
[null,null,"1.ci bölgede :"]
[null,null,"E / 108 * y =",null,null,null,{"$f":"+E3739","v":-1.9005212858384015E-4},null,null,"*","x4"," /",24,null,"+",{"$f":"+N3739","v":2.1991746307558646E-3},null,null,"*","x3"," /",6,"+",{"$f":"+V3739","v":-2.8711446568201564E-3},null,null,"*","x²"," /",2,"+","C1","*","x","+","C2"]
[null,null,"y = (",null,{"$f":"+G3754","v":-1.9005212858384015E-4},null,null,"*","x4"," /",24,null,"+",{"$f":"+P3754","v":2.1991746307558646E-3},null,null,"*","x3"," /",6,"+",{"$f":"+X3754","v":-2.8711446568201564E-3},null,null,"*","x²"," /",2,") * 108 /  E "]
[null,null,"x=",0.7,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,{"$f":"IF(D3756<=AM3728,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E3755","v":-1.9005212858384015E-4},null,null,"*",{"$f":"+D3756","v":0.7},null,"4 /",24,null,"+",{"$f":"+N3755","v":2.1991746307558646E-3},null,null,"*",{"$f":"+D3756","v":0.7},null,"3/",6,"+",{"$f":"+V3755","v":-2.8711446568201564E-3},null,null,"*",{"$f":"+S3757","v":0.7},null,"² /",2,")* 108 /",null,null,{"$f":"+AH3732","v":200000}]
[null,null,"y =",null,{"$f":"(E3757*I3757^4/L3757+O3757*S3757^3/V3757+X3757*AB3757^2/AE3757)*100000000/AI3757","v":-0.28980613551621776},null,null,"mm"]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"AI3730*1000","v":1500},null,null," /",150,null,"=",{"$f":"+H3759/L3759","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E3758","v":-0.28980613551621776},null,null,"mm",null,{"$f":"IF(ABS(D3760)<ABS(M3760),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O3759","v":10},null,null,"mm",null,{"$f":"IF(ABS(D3760)<ABS(M3760),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"2.ci bölgede :"]
[null,null,"E / 108 * y =",null,null,null,{"$f":"+E3743","v":-2.0933014354066986E-3},null,null,"*","z4"," /",12,null,"+",{"$f":"+N3743","v":2.1291866028708133E-2},null,null,"*","z3"," /",6,"+",{"$f":"+V3743","v":-1.5693779904306218E-2},null,null,"*","z²"," /",2,"+","D1","*","z","+","D2"]
[null,null,"y = (",null,{"$f":"+G3762","v":-2.0933014354066986E-3},null,null,"*","z4"," /",12,null,"+",{"$f":"+P3762","v":2.1291866028708133E-2},null,null,"*","z3"," /",6,"+",{"$f":"+X3762","v":-1.5693779904306218E-2},null,null,"*","z²"," /",2,"+",{"$f":"+O3749","v":-1.4818681219229653E-3},null,null,"*","z","+",{"$f":"+O3752","v":-5.796122710324355E-4},null,null,") * 108 /  E "]
[null,null,"z=",0.8,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,{"$f":"IF(D3764>AE3728,\"azalt.\",\"\")","v":""}]
[null,null,"y = (",null,{"$f":"+E3763","v":-2.0933014354066986E-3},null,null,"*",{"$f":"+D3764","v":0.8},null,"4 /",12,null,"+",{"$f":"+N3763","v":2.1291866028708133E-2},null,null,"*",{"$f":"+D3764","v":0.8},null,"3/",6,"+",{"$f":"+V3763","v":-1.5693779904306218E-2},null,null,"*",{"$f":"+S3765","v":0.8},null,"² /",2,"+",{"$f":"+AD3763","v":-1.4818681219229653E-3},null,null,"*",{"$f":"+AB3765","v":0.8},null,"+",{"$f":"+AJ3763","v":-5.796122710324355E-4},null,null,")* 108 /",null,null,{"$f":"+AI3757","v":200000}]
[null,null,"y =",null,{"$f":"(E3765*I3765^4/L3765+O3765*S3765^3/V3765+X3765*AB3765^2/AE3765+AG3765*AK3765+AN3765)*100000000/AT3765","v":-2.5208308962471264},null,null,"mm"]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"AI3730*1000","v":1500},null,null," /",150,null,"=",{"$f":"+H3767/L3767","v":10},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E3766","v":-2.5208308962471264},null,null,"mm",null,{"$f":"IF(ABS(D3768)<ABS(M3768),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O3767","v":10},null,null,"mm",null,{"$f":"IF(ABS(D3768)<ABS(M3768),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[]
[]
[null,"SİNÜZOİDAL YÜKLÜ ÇELİK BASİT KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"q=",50,null,"KN/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kiriş enkesiti"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"q * sin ( p * x / L )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"eğilme ve kesme tasarımında kullanılacak değerler"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cb =",null,{"$f":"+AL3827","v":1.1635872746807807}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max =",null,{"$f":"ABS(AF3819)","v":324.22778765548088},null,null,"KNm",null,"(max moment)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(Q3781,$CG$6:$CG$120,0),0)","v":600},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vmax =",null,null,{"$f":"MAX(ABS(J3783),ABS(Y3783))","v":127.32395447351627},null,null,"KN",null,"(max kesme kuvveti)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(Q3781,$CG$6:$CG$120,0),0)","v":12}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,"IPE 600"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(Q3781,$CG$6:$CG$120,0),0)","v":19}]
[null,null,null,null,null,null,null,null,"A=",{"$f":"+AL3811","v":127.32395447351627},null,null,"KN",null,null,null,null,null,null,null,null,null,null,"B=",{"$f":"+H3812","v":127.32395447351627},null,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",8,null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(Q3781,$CG$6:$CG$120,0),0)","v":220}]
[null,null,null,null,null,null,null,null,"x = 0 ; v'' = 0",null,null,null,null,null,"sınır ve uygunluk şartları :",null,null,null,null,null,null,null,null,"x = L ; v'' = 0"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(Q3781,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[]
[null,null,null,null,null,null,null,null,"x = 0 ; v = 0",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"x = L ; v = 0"]
[null,null,null,"SEHİM HESABI"]
[null,null,null,"v'''' =",null," - q * sin ( p * x / L )"]
[null,null,null,"v''' =",null,"q * L / p * cos ( p * x / L ) + C1"]
[null,null,null,"v'' =",null,"q * L² / p² * sin ( p * x / L ) + C1 * x + C2"]
[null,null,null,"v' =",null," - q * L3 / p3 * cos ( p * x / L ) + C1 * x² / 2 + C2 * x + C3"]
[null,null,null,"v =",null,"q * L4 / p4 * sin ( p * x / L ) + C1 * x3 / 6 + C2 * x² / 2 + C3 * x + C4"]
[null,null,null,"sınır ve uygunluk şartları :"]
[null,null,null,"x = 0 ; v = 0",null,null,null,null,null,"C4 = 0"]
[null,null,null,"x = 0 ; v'' = 0",null,null,null,null,null,"C2 = 0"]
[null,null,null,"x = L ; v'' = 0",null,null,null,null,null,{"$f":"+Q3773","v":50},null,"*",{"$f":"+R3784","v":8},null,"² /","p²","*","sin  (",null,"p","*",{"$f":"+R3784","v":8},null," /",{"$f":"+R3784","v":8},null,")+","C1","*",{"$f":"+R3784","v":8},null,"=",0,null,null,"C1","=",{"$f":"-(J3800*M3800^2/PI()^2*SIN(PI()*V3800/Y3800))/AD3800","v":-4.9653396635569072E-15}]
[null,null,null,"x = L ; v = 0",null,null,null,null,null,{"$f":"+Q3773","v":50},null,"*",{"$f":"+R3784","v":8},null,"4 /","p4","*","sin  (",null,"p","*",{"$f":"+R3784","v":8},null," /",{"$f":"+R3784","v":8},null,")+",{"$f":"+AL3800","v":-4.9653396635569072E-15},null,null,"*",{"$f":"+R3784","v":8},null,"3 /",6,"+","C3","*",{"$f":"+R3784","v":8},null,"=",0,null,null,"C3","=",{"$f":"-(J3801*M3801^4/PI()^4*SIN(PI()*V3801/Y3801)+AB3801*AF3801^3/AI3801)/AM3801","v":2.0765601196479029E-14}]
[null,null,null,"elastik eğri denklemi"]
[null,null,null,"E * I / 108 * y =",null,null,null,null,"q * L4 / p4 * sin ( p * x / L ) + C1 * x3 / 6 + C2 * x² / 2 + C3 * x + C4"]
[null,null,null,"y = (",null,{"$f":"+Q3773","v":50},null,"*",{"$f":"+R3784","v":8},null,"4 /","p4","*","sin  (",null,"p","*","x"," /",{"$f":"+R3784","v":8},null,")+",{"$f":"+AL3800","v":-4.9653396635569072E-15},null,null,"*","x3"," /",6,"+",{"$f":"+AU3801","v":2.0765601196479029E-14},null,null,"*","x",") * 108 / ( E * I )"]
[null,null,null,"x=",3.25,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(E3805<=R3784,\"\",\"azalt.\")","v":""}]
[null,null,null,"y = (",null,{"$f":"+F3804","v":50},null,"*",{"$f":"+I3804","v":8},null,"4 /","p4","*","sin  (",null,"p","*",{"$f":"+E3805","v":3.25},null," /",{"$f":"+T3804","v":8},null,")+",{"$f":"+W3804","v":-4.9653396635569072E-15},null,null,"*",{"$f":"+E3805","v":3.25},null,"3 /",6,"+",{"$f":"+AE3804","v":2.0765601196479029E-14},null,null,"*",{"$f":"+AB3806","v":3.25},null,")* 108 / (",null,null,{"$f":"+AQ3788","v":200000},null,null,"*",{"$f":"+AQ3787","v":92080},null,null,")"]
[null,null,null,"y =",null,{"$f":"(F3806*I3806^4/PI()^4*SIN(PI()*R3806/U3806)+X3806*AB3806^3/AE3806+AG3806*AK3806)*100000000/(AP3806*AT3806)","v":10.924964037302967},null,null,"mm"]
[null,null,null,"ymax = L / 300 =",null,null,null,null,{"$f":"R3784*1000","v":8000},null,null," /",300,null,"=",{"$f":"+I3808/M3808","v":26.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,null,"y=",{"$f":"+F3807","v":10.924964037302967},null,null,"mm",null,{"$f":"IF(ABS(E3809)<ABS(N3809),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+P3808","v":26.666666666666668},null,null,"mm",null,{"$f":"IF(ABS(E3809)<ABS(N3809),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,null,"MESNET TEPKİLERİ"]
[null,null,null,"A = ( x = 0 ; v''' = 0 )",null,null,null,null,null,null,null,"A","=",{"$f":"+Q3773","v":50},null,"*",{"$f":"+R3784","v":8},null," /","p","*","cos (",null,"p","*",0," /",{"$f":"+R3784","v":8},null,")+",{"$f":"+AL3800","v":-4.9653396635569072E-15},null,null,null,null,"A","=",{"$f":"N3811*Q3811/PI()*COS(PI()*Z3811/AB3811)+AE3811","v":127.32395447351627},null,null,"KN"]
[null,null,null,"A","=","B","=",{"$f":"+AL3811","v":127.32395447351627},null,null,"KN"]
[null,null,null,"ARA KESİT TESİRLERİ"]
[null,null,null,"x=",1,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(E3814<=R3784,\"\",\"azalt.\")","v":""}]
[null,null,null,"Mx =",null,"q * L² / p² * sin ( p * x / L ) + C1 * x + C2 =",null,null,null,null,null,null,null,null,null,null,null,{"$f":"+Q3773","v":50},null,"*",{"$f":"+R3784","v":8},null,"² /","p²","*","sin  (",null,"p","*",{"$f":"+E3814","v":1},null," /",{"$f":"+R3784","v":8},null,")+",{"$f":"+AL3800","v":-4.9653396635569072E-15},null,null,"*",{"$f":"+E3814","v":1},null,"=",{"$f":"R3815*U3815^2/PI()^2*SIN(PI()*AD3815/AG3815)+AJ3815*AN3815","v":124.07660264813892},null,null,"KNm"]
[null,null,null,"Vx =",null,"q * L / p * cos ( p * x / L ) + C1 =",null,null,null,null,null,null,null,null,null,{"$f":"+Q3773","v":50},null,"*",{"$f":"+R3784","v":8},null," /","p","*","cos (",null,"p","*",{"$f":"+E3814","v":1},null," /",{"$f":"+R3784","v":8},null,")+",{"$f":"+AJ3815","v":-4.9653396635569072E-15},null,null,"=",{"$f":"P3816*S3816/PI()*COS(PI()*AB3816/AE3816)+AH3816","v":117.63199553648056},null,null,"KN"]
[null,null,null,"EĞİLME HESABINDA KULLANILMAK ÜZERE Cb KATSAYISI İÇİN ( Mmax ; MA ; MB ; MC ) HESABI (Çelik yönetmelik madde 9.1.(c) uyarınca)"]
[null,null,null,"x=",{"$f":"+R3784/2","v":4},null,null,"m. ' deki max moment miktarı"]
[null,null,null,"Mmax =",null,null,{"$f":"+R3815","v":50},null,"*",{"$f":"+U3815","v":8},null,"² /","p²","*","sin  (",null,"p","*",{"$f":"+E3818","v":4},null," /",{"$f":"+AG3815","v":8},null,")+",{"$f":"+AJ3815","v":-4.9653396635569072E-15},null,null,"*",{"$f":"+S3819","v":4},null,"=",{"$f":"G3819*J3819^2/PI()^2*SIN(PI()*S3819/V3819)+Y3819*AC3819","v":324.22778765548088},null,null,"KNm"]
[null,null,null,"L / 2 =",null,{"$f":"+R3784/2","v":4},null,null,"m. ' deki moment miktarı"]
[null,null,null,"MB =",null,{"$f":"+G3819","v":50},null,"*",{"$f":"+J3819","v":8},null,"² /","p²","*","sin  (",null,"p","*",{"$f":"+F3820","v":4},null," /",{"$f":"+V3819","v":8},null,")+",{"$f":"+Y3819","v":-4.9653396635569072E-15},null,null,"*",{"$f":"+R3821","v":4},null,"=",{"$f":"F3821*I3821^2/PI()^2*SIN(PI()*R3821/U3821)+X3821*AB3821","v":324.22778765548088},null,null,"KNm",null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca"]
[null,null,null,"L / 4 =",null,{"$f":"+R3784/4","v":2},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MA = L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,"MA =",null,{"$f":"+F3821","v":50},null,"*",{"$f":"+I3821","v":8},null,"² /","p²","*","sin  (",null,"p","*",{"$f":"+F3822","v":2},null," /",{"$f":"+U3821","v":8},null,")+",{"$f":"+X3821","v":-4.9653396635569072E-15},null,null,"*",{"$f":"+R3823","v":2},null,"=",{"$f":"F3823*I3823^2/PI()^2*SIN(PI()*R3823/U3823)+X3823*AB3823","v":229.2636673003025},null,null,"KNm",null,null,null,null,null,null,null,null,null,"( MB = L / 2 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,"3 * L / 4 =",null,null,{"$f":"3*R3784/4","v":6},null,null,"m. ' deki moment miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"( MC = 3 * L / 4 mesafedeki gerekli eğilme momentinin mutlak değeri )"]
[null,null,null,"MC =",null,{"$f":"+F3823","v":50},null,"*",{"$f":"+I3823","v":8},null,"² /","p²","*","sin  (",null,"p","*",{"$f":"+G3824","v":6},null," /",{"$f":"+U3823","v":8},null,")+",{"$f":"+X3823","v":-4.9653396635569072E-15},null,null,"*",{"$f":"+R3825","v":6},null,"=",{"$f":"F3825*I3825^2/PI()^2*SIN(PI()*R3825/U3825)+X3825*AB3825","v":229.2636673003025},null,null,"KNm"]
[null,null,null,"Cb = 12,5 * Mmax / ( 2,5 * Mmax + 3 * MA + 4 * MB + 3 * MC )"]
[null,null,null,"Cb =",null,12.5,null,"*",{"$f":"ABS(AF3819)","v":324.22778765548088},null,null," /(",2.5,null,"*",{"$f":"+I3827","v":324.22778765548088},null,null,"+",3,"*",{"$f":"ABS(AE3823)","v":229.2636673003025},null,null,"+",4,"*",{"$f":"ABS(AE3821)","v":324.22778765548088},null,null,"+",3,"*",{"$f":"ABS(AE3825)","v":229.2636673003025},null,null,")=",{"$f":"F3827*I3827/(M3827*P3827+T3827*V3827+Z3827*AB3827+AF3827*AH3827)","v":1.1635872746807807}]
[]
[]
[null,"TEKİL & YAYILI YÜKLÜ ÇELİK KONSOL KİRİŞ SEHİM HESABI\n(inş.müh. Gürcan BERBEROĞLU tel:0532 366 02 04   www.betoncelik.com )                 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not : sehim hesabında (G + Q) yük terimleri kullanılmalı.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dikkat sadece sarı hücrelere data girilecek."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"q=",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kiriş enkesiti"]
[null,null,null,null,null,null,null,null,null,null,"(1.ci bölge)",null,null,null,null,null,"(2.ci bölge)",null,null,null,null,"(3.cü bölge)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,"KN",null,null,8,null,"KN",null,null,15,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,10,null,"KN/m",null,null,20,null,"KN/m",null,null,30,null,"KN/m"]
[]
[null,null,"Ma =",null,{"$f":"L3835*L3843*L3843/2+Q3835*Q3843*(Q3843/2+L3843)+V3835*V3843*(V3843/2+Q3843+L3843)+O3834*L3843+T3834*(Q3843+L3843)+Y3834*Q3845","v":83.737500000000011},null,null,"KNm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CI$6:$CI$120,MATCH(P3839,$CG$6:$CG$120,0),0)","v":600}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CK$6:$CK$120,MATCH(P3839,$CG$6:$CG$120,0),0)","v":12}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPE 600",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Çelik yönetmelik madde 9.1.(c) uyarınca konsol kirişte Cb = 1 alınır."]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"x",null,null,null,"z",null,null,null,null,"m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CL$6:$CL$120,MATCH(P3839,$CG$6:$CG$120,0),0)","v":19}]
[null,null,null,null,null,null,null,null,"A=",{"$f":"+L3835*L3843+Q3835*Q3843+V3835*V3843+O3834+T3834+Y3834","v":61.5},null,null,"KN"]
[null,null,null,null,null,null,null,null,null,null,null,0.8,null,"m",null,null,0.65,null,"m",null,null,0.45,null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INDEX($CJ$6:$CJ$120,MATCH(P3839,$CG$6:$CG$120,0),0)","v":220}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L=",{"$f":"+L3843+Q3843+V3843","v":1.9000000000000001},null,"m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ix =",null,{"$f":"INDEX($CM$6:$CM$120,MATCH(P3839,$CG$6:$CG$120,0),0)","v":92080},null,null,null,"cm4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sınır ve uygunluk şartları :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E =",null,200000,null,null,null,"N/mm²",null,null,"(kiriş elastisite modülü)"]
[null,null,null,null,null,null,null,null,"x = 0 ; v' = 0",null,null,null,null,"(x = L ; v1' ) = ( z = 0 ; v2' )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"(x = L ; v1 ) = ( z = 0 ; v2 )"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(z = L ; v2' ) = ( m = 0 ; v3' )"]
[null,null,null,null,null,null,null,null,"x = 0 ; v = 0",null,null,null,null,null,null,null,null,"(z = L ; v2 ) = ( m = 0 ; v3 )"]
[null,null,"SEHİM HESABI"]
[null,null,"1.ci bölgede :"]
[null,null,"v1'' =",null,{"$f":"-E3837","v":-83.737500000000011},null,"+",{"$f":"+J3842","v":61.5},null,"*","x","-",{"$f":"+L3835","v":10},null,"*","x²"," /",2]
[null,null,"v1' =",null,{"$f":"+E3854","v":-83.737500000000011},null,"*","x","+",{"$f":"+H3854","v":61.5},null,"*","x²"," /",2,"-",{"$f":"+M3854","v":10},null,"*","x3"," /",6,"+","C1"]
[null,null,"v1 =",null,{"$f":"+E3855","v":-83.737500000000011},null,"*","x²"," /",2,"+",{"$f":"+J3855","v":61.5},null,"*","x3"," /",6,"-",{"$f":"+Q3855","v":10},null,"*","x4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"2.ci bölgede :"]
[null,null,"v2'' =",null,{"$f":"-E3837","v":-83.737500000000011},null,"+",{"$f":"+J3842","v":61.5},null,"*(",{"$f":"+L3843","v":0.8},null,"+","z",")-",{"$f":"+L3835","v":10},null,"*",{"$f":"+L3843","v":0.8},null,"*(",{"$f":"+L3843/2","v":0.4},null,"+","z",")-",{"$f":"+O3834","v":4},null,"*","z","-",{"$f":"+Q3835","v":20},null,"*","z²"," /",2]
[null,null,"v2' =",null,{"$f":"+E3858","v":-83.737500000000011},null,"*","x","+",{"$f":"+H3858","v":61.5},null,"*(",{"$f":"+K3858","v":0.8},null,"+","z",")²"," /",2,"-",{"$f":"+P3858*S3858","v":8},null,"*(",{"$f":"+V3858","v":0.4},null,"+","z",")²"," /",2,"-",{"$f":"+AA3858","v":4},null,"*","z²"," /",2,"-",{"$f":"+AF3858","v":20},null,"*","z3"," /",6,"+","D1"]
[null,null,"v2 =",null,{"$f":"+E3859","v":-83.737500000000011},null,"*","x²"," /",2,"+",{"$f":"+J3859","v":61.5},null,"*(",{"$f":"+M3859","v":0.8},null,"+","z",")3"," /",6,"-",{"$f":"+U3859","v":8},null,"*(",{"$f":"+X3859","v":0.4},null,"+","z",")3"," /",6,"-",{"$f":"+AF3859","v":4},null,"*","z3"," /",6,"-",{"$f":"+AM3859","v":20},null,"*","z4"," /",24,null,"+","D1","*","z","+","D2"]
[null,null,"3.ci bölgede :"]
[null,null,"v3'' =",null,{"$f":"-E3837","v":-83.737500000000011},null,"+",{"$f":"+J3842","v":61.5},null,"*(",{"$f":"+L3843+Q3843","v":1.4500000000000002},null,"+","m",")-",{"$f":"+L3835","v":10},null,"*",{"$f":"+L3843","v":0.8},null,"*(",{"$f":"+L3843/2+Q3843","v":1.05},null,"+","m",")-",{"$f":"+O3834","v":4},null,"*(",{"$f":"+Q3843","v":0.65},null,"+","m",")-",{"$f":"+Q3835","v":20},null,"*",{"$f":"+Q3843","v":0.65},null,"*(",{"$f":"+Q3843/2","v":0.32500000000000001},null,"+","m",")-",{"$f":"+T3834","v":8},null,"*","m","-",{"$f":"+V3835","v":30},null,"*","m²"," /",2]
[null,null,"v3' =",null,{"$f":"+E3862","v":-83.737500000000011},null,"*","m","+",{"$f":"+H3862","v":61.5},null,"*(",{"$f":"+K3862","v":1.4500000000000002},null,"+","m",")²"," /",2,"-",{"$f":"+P3862*S3862","v":8},null,"*(",{"$f":"+V3862","v":1.05},null,"+","m",")²"," /",2,"-",{"$f":"+AA3862","v":4},null,"*(",{"$f":"+AD3862","v":0.65},null,"+","m",")²"," /",2,"-",{"$f":"+AI3862*AL3862","v":13},null,"*(",{"$f":"+AO3862","v":0.32500000000000001},null,"+","m",")²"," /",2,"-",{"$f":"+AT3862","v":8},null,"*","m²"," /",2,"-",{"$f":"+AY3862","v":30},null,"*","m3"," /",6,"+","E1"]
[null,null,"v3 =",null,{"$f":"+E3863","v":-83.737500000000011},null,"*","m²"," /",2,"+",{"$f":"+J3863","v":61.5},null,"*(",{"$f":"+M3863","v":1.4500000000000002},null,"+","m",")3"," /",6,"-",{"$f":"+U3863","v":8},null,"*(",{"$f":"+X3863","v":1.05},null,"+","m",")3"," /",6,"-",{"$f":"+AF3863","v":4},null,"*(",{"$f":"+AI3863","v":0.65},null,"+","m",")3"," /",6,"-",{"$f":"+AQ3863","v":13},null,"*(",{"$f":"+AT3863","v":0.32500000000000001},null,"+","m",")3"," /",6,"-",{"$f":"+BB3863","v":8},null,"*","m3"," /",6,"-",{"$f":"+BI3863","v":30},null,"*","m4"," /",24,null,"+","E1","*","m","+","E2"]
[null,null,"sınır ve uygunluk şartları :"]
[null,null,"x = 0 ; v1 = 0",null,null,null,null,null,"C2 = 0"]
[null,null,"x = 0 ; v1' = 0",null,null,null,null,null,"C1 = 0"]
[null,null,"x = L ; v1 =",null,null,null,{"$f":"+E3856","v":-83.737500000000011},null,"*",{"$f":"+L3843","v":0.8},null,"² /",2,"+",{"$f":"+L3856","v":61.5},null,"*",{"$f":"+J3868","v":0.8},null,"3 /",6,"-",{"$f":"+S3856","v":10},null,"*",{"$f":"+R3868","v":0.8},null,"4 /",24,null,"=",{"$f":"G3868*J3868^2/M3868+O3868*R3868^3/U3868-W3868*Z3868^4/AC3868","v":-21.718666666666675}]
[null,null,"z = 0 ; v2 =",null,null,null,{"$f":"+L3860","v":61.5},null,"*",{"$f":"+O3860","v":0.8},null,"3 /",6,"-",{"$f":"+W3860","v":8},null,"*",{"$f":"+Z3860","v":0.4},null,"3 /",6,"+","D2","=","D2","+",{"$f":"+G3869*J3869^3/M3869-O3869*R3869^3/U3869","v":5.1626666666666674}]
[null,null,"(x = L ; v1 ) = ( z = 0 ; v2 )",null,null,null,null,null,null,null,null,null,{"$f":"+AF3868","v":-21.718666666666675},null,null,"=","D2","+",{"$f":"+AA3869","v":5.1626666666666674},null,null,null,null,"D2","=",{"$f":"+M3870-S3870","v":-26.881333333333341}]
[null,null,"x = L ; v1' =",null,null,null,{"$f":"+E3855","v":-83.737500000000011},null,"*",{"$f":"+L3843","v":0.8},null,"+",{"$f":"+J3855","v":61.5},null,"*",{"$f":"+J3871","v":0.8},null,"² /",2,"-",{"$f":"+Q3855","v":10},null,"*",{"$f":"+P3871","v":0.8},null,"3 /",6,"=",{"$f":"G3871*J3871+M3871*P3871^2/S3871-U3871*X3871^3/AA3871","v":-48.163333333333334}]
[null,null,"z = 0 ; v2' =",null,null,null,{"$f":"+J3859","v":61.5},null,"*",{"$f":"+M3859","v":0.8},null,"² /",2,"-",{"$f":"+U3859","v":8},null,"*",{"$f":"+X3859","v":0.4},null,"² /",2,"+","D1","=","D1","+",{"$f":"+G3872*J3872^2/M3872-O3872*R3872^2/U3872","v":19.040000000000003}]
[null,null,"(x = L ; v1' ) = ( z = 0 ; v2' )",null,null,null,null,null,null,null,null,null,{"$f":"+AC3871","v":-48.163333333333334},null,null,"=","D1","+",{"$f":"+AA3872","v":19.040000000000003},null,null,null,null,"D1","=",{"$f":"+M3873-S3873","v":-67.203333333333333}]
[null,null,"z = L ; v2 =",null,null,null,{"$f":"+E3860","v":-83.737500000000011},null,"*",{"$f":"+Q3843","v":0.65},null,"² /",2,"+",{"$f":"+L3860","v":61.5},null,"*(",{"$f":"+O3860","v":0.8},null,"+",{"$f":"+J3874","v":0.65},null,")3"," /",6,"-",{"$f":"+W3860","v":8},null,"*(",{"$f":"+Z3860","v":0.4},null,"+",{"$f":"+U3874","v":0.65},null,")3"," /",6,"-",{"$f":"+AH3860","v":4},null,"*",{"$f":"+AG3874","v":0.65},null,"3 /",6,"-",{"$f":"+AO3860","v":20},null,"*",{"$f":"+AP3874","v":0.65},null,"4 /",24,null,"+",{"$f":"+Z3873","v":-67.203333333333333},null,null,"*",{"$f":"+AX3874","v":0.65},null,"+",{"$f":"+Z3870","v":-26.881333333333341},null,null,"=",{"$f":"G3874*J3874^2/M3874+O3874*(R3874+U3874)^3/Y3874-AA3874*(AD3874+AG3874)^3/AK3874-AM3874*AP3874^3/AS3874-AU3874*AX3874^4/BA3874+BD3874*BH3874+BK3874","v":-58.879979166666672}]
[null,null,"m = 0 ; v3 =",null,null,null,{"$f":"+L3864","v":61.5},null,"*",{"$f":"+O3864","v":1.4500000000000002},null,"3 /",6,"-",{"$f":"+W3864","v":8},null,"*",{"$f":"+Z3864","v":1.05},null,"3 /",6,"-",{"$f":"+AH3864","v":4},null,"*",{"$f":"+AK3864","v":0.65},null,"3 /",6,"-",{"$f":"+AS3864","v":13},null,"*",{"$f":"+AV3864","v":0.32500000000000001},null,"3 /",6,"+","E2","=","E2","+",{"$f":"G3875*J3875^3/M3875-O3875*R3875^3/U3875-W3875*Z3875^3/AC3875-AE3875*AH3875^3/AK3875","v":29.447445312500012}]
[null,null,"(z = L ; v2 ) = ( m = 0 ; v3 )",null,null,null,null,null,null,null,null,null,{"$f":"+BO3874","v":-58.879979166666672},null,null,"=","E2","+",{"$f":"+AQ3875","v":29.447445312500012},null,null,null,null,"E2","=",{"$f":"+M3876-S3876","v":-88.32742447916668}]
[null,null,"z = L ; v2' =",null,null,null,{"$f":"+E3859","v":-83.737500000000011},null,"*",{"$f":"+Q3843","v":0.65},null,"+",{"$f":"+J3859","v":61.5},null,"*(",{"$f":"+M3859","v":0.8},null,"+",{"$f":"+J3877","v":0.65},null,")²"," /",2,"-",{"$f":"+U3859","v":8},null,"*(",{"$f":"+X3859","v":0.4},null,"+",{"$f":"+S3877","v":0.65},null,")²"," /",2,"-",{"$f":"+AF3859","v":4},null,"*",{"$f":"+AE3877","v":0.65},null,"² /",2,"-",{"$f":"+AM3859","v":20},null,"*",{"$f":"+AN3877","v":0.65},null,"3 /",6,"+",{"$f":"+Z3873","v":-67.203333333333333},null,null,"=",{"$f":"G3877*J3877+M3877*(P3877+S3877)^2/W3877-Y3877*(AB3877+AE3877)^2/AI3877-AK3877*AN3877^2/AQ3877-AS3877*AV3877^3/AY3877+BA3877","v":-63.15124999999999}]
[null,null,"m = 0 ; v3' =",null,null,null,{"$f":"+J3863","v":61.5},null,"*",{"$f":"+M3863","v":1.4500000000000002},null,"² /",2,"-",{"$f":"+U3863","v":8},null,"*",{"$f":"+X3863","v":1.05},null,"² /",2,"-",{"$f":"+AF3863","v":4},null,"*",{"$f":"+AI3863","v":0.65},null,"² /",2,"-",{"$f":"+AQ3863","v":13},null,"*",{"$f":"+AT3863","v":0.32500000000000001},null,"² /",2,"+","E1","=","E1","+",{"$f":"G3878*J3878^2/M3878-O3878*R3878^2/U3878-W3878*Z3878^2/AC3878-AE3878*AH3878^2/AK3878","v":58.710312500000022}]
[null,null,"(z = L ; v2' ) = ( m = 0 ; v3' )",null,null,null,null,null,null,null,null,null,{"$f":"+BE3877","v":-63.15124999999999},null,null,"=","E1","+",{"$f":"+AQ3878","v":58.710312500000022},null,null,null,null,"E1","=",{"$f":"+M3879-S3879","v":-121.86156250000002}]
[null,null,"1.ci bölgede elastik eğri denklemi"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E3856","v":-83.737500000000011},null,"*","x²"," /",2,"+",{"$f":"+L3856","v":61.5},null,"*","x3"," /",6,"-",{"$f":"+S3856","v":10},null,"*","x4"," /",24,null,"+","C1","*","x","+","C2"]
[null,null,"y = (",null,{"$f":"+H3881","v":-83.737500000000011},null,"*","x²"," /",2,"+",{"$f":"+O3881","v":61.5},null,"*","x3"," /",6,"-",{"$f":"+V3881","v":10},null,"*","x4"," /",24,null,") * 108 / ( E * I )"]
[null,null,"x=",0.8,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D3883<=L3843,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E3882","v":-83.737500000000011},null,"*",{"$f":"+D3883","v":0.8},null,"² /",2,"+",{"$f":"+L3882","v":61.5},null,"*",{"$f":"+H3884","v":0.8},null,"3 /",6,"-",{"$f":"+S3882","v":10},null,"*",{"$f":"+P3884","v":0.8},null,"4 /",24,null,")* 108 / (",null,null,{"$f":"+AQ3847","v":200000},null,null,"*",{"$f":"+AQ3846","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E3884*H3884^2/K3884+M3884*P3884^3/S3884-U3884*X3884^4/AA3884)*100000000/(AF3884*AJ3884)","v":-0.11793368085722565},null,null,"mm"]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"Q3845*1000","v":1900.0000000000002},null,null," /",150,null,"=",{"$f":"+H3886/L3886","v":12.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E3885","v":-0.11793368085722565},null,null,"mm",null,{"$f":"IF(ABS(D3887)<ABS(M3887),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O3886","v":12.666666666666668},null,null,"mm",null,{"$f":"IF(ABS(D3887)<ABS(M3887),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"2.ci bölgede elastik eğri denklemi"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E3860","v":-83.737500000000011},null,"*","x²"," /",2,"+",{"$f":"+L3860","v":61.5},null,"*(",{"$f":"+O3860","v":0.8},null,"+","z",")3"," /",6,"-",{"$f":"+W3860","v":8},null,"*(",{"$f":"+Z3860","v":0.4},null,"+","z",")3"," /",6,"-",{"$f":"+AH3860","v":4},null,"*","z3"," /",6,"-",{"$f":"+AO3860","v":20},null,"*","z4"," /",24,null,"+","D1","*","z","+","D2"]
[null,null,"y = (",null,{"$f":"+H3889","v":-83.737500000000011},null,"*","x²"," /",2,"+",{"$f":"+O3889","v":61.5},null,"*(",{"$f":"+R3889","v":0.8},null,"+","z",")3"," /",6,"-",{"$f":"+Z3889","v":8},null,"*(",{"$f":"+AC3889","v":0.4},null,"+","z",")3"," /",6,"-",{"$f":"+AK3889","v":4},null,"*","z3"," /",6,"-",{"$f":"+AR3889","v":20},null,"*","z4"," /",24,null,"+",{"$f":"+Z3873","v":-67.203333333333333},null,null,"*","z","+",{"$f":"+Z3870","v":-26.881333333333341},null,null,") * 108 / ( E * I )"]
[null,null,"z=",0.65,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D3891<=Q3843,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E3890","v":-83.737500000000011},null,"*",{"$f":"+D3891","v":0.65},null,"² /",2,"+",{"$f":"+L3890","v":61.5},null,"*(",{"$f":"+O3890","v":0.8},null,"+",{"$f":"+H3892","v":0.65},null,")3"," /",6,"-",{"$f":"+W3890","v":8},null,"*(",{"$f":"+Z3890","v":0.4},null,"+",{"$f":"+S3892","v":0.65},null,")3"," /",6,"-",{"$f":"+AH3890","v":4},null,"*",{"$f":"+AE3892","v":0.65},null,"3 /",6,"-",{"$f":"+AO3890","v":20},null,"*",{"$f":"+AN3892","v":0.65},null,"4 /",24,null,"+",{"$f":"+AW3890","v":-67.203333333333333},null,null,"*",{"$f":"+AV3892","v":0.65},null,"+",{"$f":"+BC3890","v":-26.881333333333341},null,null,")* 108 / (",null,null,{"$f":"+AF3884","v":200000},null,null,"*",{"$f":"+AJ3884","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E3892*H3892^2/K3892+M3892*(P3892+S3892)^3/W3892-Y3892*(AB3892+AE3892)^3/AI3892-AK3892*AN3892^3/AQ3892-AS3892*AV3892^4/AY3892+BB3892*BF3892+BI3892)*100000000/(BO3892*BS3892)","v":-0.31972186775991895},null,null,"mm"]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"Q3845*1000","v":1900.0000000000002},null,null," /",150,null,"=",{"$f":"+H3894/L3894","v":12.666666666666668},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E3893","v":-0.31972186775991895},null,null,"mm",null,{"$f":"IF(ABS(D3895)<ABS(M3895),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O3894","v":12.666666666666668},null,null,"mm",null,{"$f":"IF(ABS(D3895)<ABS(M3895),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"3.ci bölgede elastik eğri denklemi"]
[null,null,"E * I / 108 * y =",null,null,null,null,{"$f":"+E3864","v":-83.737500000000011},null,"*","m²"," /",2,"+",{"$f":"+L3864","v":61.5},null,"*(",{"$f":"+O3864","v":1.4500000000000002},null,"+","m",")3"," /",6,"-",{"$f":"+W3864","v":8},null,"*(",{"$f":"+Z3864","v":1.05},null,"+","m",")3"," /",6,"-",{"$f":"+AH3864","v":4},null,"*(",{"$f":"+AK3864","v":0.65},null,"+","m",")3"," /",6,"-",{"$f":"+AS3864","v":13},null,"*(",{"$f":"+AV3864","v":0.32500000000000001},null,"+","m",")3"," /",6,"-",{"$f":"+BD3864","v":8},null,"*","m3"," /",6,"-",{"$f":"+BK3864","v":30},null,"*","m4"," /",24,null,"+","E1","*","m","+","E2"]
[null,null,"y = (",null,{"$f":"+H3897","v":-83.737500000000011},null,"*","m²"," /",2,"+",{"$f":"+O3897","v":61.5},null,"*(",{"$f":"+R3897","v":1.4500000000000002},null,"+","m",")3"," /",6,"-",{"$f":"+Z3897","v":8},null,"*(",{"$f":"+AC3897","v":1.05},null,"+","m",")3"," /",6,"-",{"$f":"+AK3897","v":4},null,"*(",{"$f":"+AN3897","v":0.65},null,"+","m",")3"," /",6,"-",{"$f":"+AV3897","v":13},null,"*(",{"$f":"+AY3897","v":0.32500000000000001},null,"+","m",")3"," /",6,"-",{"$f":"+BG3897","v":8},null,"*","m3"," /",6,"-",{"$f":"+BN3897","v":30},null,"*","m4"," /",24,null,"+",{"$f":"+Z3879","v":-121.86156250000002},null,null,"*","m","+"]
[null,null,null,"+",{"$f":"+Z3876","v":-88.32742447916668},null,null,") * 108 / ( E * I )"]
[null,null,"m=",0.45,null,null,"m. ' deki sehim miktarı",null,null,null,null,null,null,null,null,{"$f":"IF(D3900<=V3843,\"\",\"azalt.\")","v":""}]
[null,null,"y = (",null,{"$f":"+E3898","v":-83.737500000000011},null,"*",{"$f":"+D3900","v":0.45},null,"² /",2,"+",{"$f":"+L3898","v":61.5},null,"*(",{"$f":"+O3898","v":1.4500000000000002},null,"+",{"$f":"+H3901","v":0.45},null,")3"," /",6,"-",{"$f":"+W3898","v":8},null,"*(",{"$f":"+Z3898","v":1.05},null,"+",{"$f":"+S3901","v":0.45},null,")3"," /",6,"-",{"$f":"+AH3898","v":4},null,"*(",{"$f":"+AK3898","v":0.65},null,"+",{"$f":"+AE3901","v":0.45},null,")3"," /",6,"-",{"$f":"+AS3898","v":13},null,"*(",{"$f":"+AV3898","v":0.32500000000000001},null,"+",{"$f":"+AQ3901","v":0.45},null,")3"," /",6,"-",{"$f":"+BD3898","v":8},null,"*",{"$f":"+BC3901","v":0.45},null,"3 /",6,"-",{"$f":"+BK3898","v":30},null,"*",{"$f":"+BL3901","v":0.45},null,"4 /",24,null,"+"]
[null,null,null,"+",{"$f":"+BS3898","v":-121.86156250000002},null,null,"*",{"$f":"+BT3901","v":0.45},null,"+",{"$f":"+E3899","v":-88.32742447916668},null,null,")* 108 / (",null,null,{"$f":"+BO3892","v":200000},null,null,"*",{"$f":"+BS3892","v":92080},null,null,")"]
[null,null,"y =",null,{"$f":"(E3901*H3901^2/K3901+M3901*(P3901+S3901)^3/W3901-Y3901*(AB3901+AE3901)^3/AI3901-AK3901*(AN3901+AQ3901)^3/AU3901-AW3901*(AZ3901+BC3901)^3/BG3901-BI3901*BL3901^3/BO3901-BQ3901*BT3901^4/BW3901+E3902*I3902+L3902)*100000000/(R3902*V3902)","v":-0.47734274600438031},null,null,"mm"]
[null,null,"ymax = L / 150 =",null,null,null,null,{"$f":"Q3855*1000","v":10000},null,null," /",150,null,"=",{"$f":"+H3904/L3904","v":66.666666666666671},null,null,"mm",null,null,"(izin verilebilir çelik kiriş max sehim miktarı)"]
[null,null,"y=",{"$f":"+E3903","v":-0.47734274600438031},null,null,"mm",null,{"$f":"IF(ABS(D3905)<ABS(M3905),\"<\",\">\")","v":"<"},"ymax =",null,null,{"$f":"+O3904","v":66.666666666666671},null,null,"mm",null,{"$f":"IF(ABS(D3905)<ABS(M3905),\"uygun.\",\"uygun değil.\")","v":"uygun."}]
[null,null,"ARA KESİT TESİRLERİ"]
[null,null,"x=",0.3,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D3907<=L3843,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+E3854","v":-83.737500000000011},null,"+",{"$f":"+H3854","v":61.5},null,"*",{"$f":"+D3907","v":0.3},null,"-",{"$f":"+M3854","v":10},null,"*",{"$f":"+K3908","v":0.3},null,"² /",2,"=",{"$f":"E3908+H3908*K3908-N3908*Q3908^2/T3908","v":-65.737500000000011},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+H3908","v":61.5},null,"-",{"$f":"+N3908","v":10},null,"*",{"$f":"+Q3908","v":0.3},null,"=",{"$f":"+E3909-H3909*K3909","v":58.5},null,null,"KN"]
[null,null,"z=",0.3,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D3910<=Q3843,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+E3858","v":-83.737500000000011},null,"+",{"$f":"+H3858","v":61.5},null,"*(",{"$f":"+K3858","v":0.8},null,"+",{"$f":"+D3910","v":0.3},null,")-",{"$f":"+P3858","v":10},null,"*",{"$f":"+S3858","v":0.8},null,"*(",{"$f":"+V3858","v":0.4},null,"+",{"$f":"+N3911","v":0.3},null,")-",{"$f":"+AA3858","v":4},null,"*",{"$f":"+Z3911","v":0.3},null,"-",{"$f":"+AF3858","v":20},null,"*",{"$f":"+AF3911","v":0.3},null,"² /",2,"=",{"$f":"E3911+H3911*(K3911+N3911)-Q3911*T3911*(W3911+Z3911)-AC3911*AF3911-AI3911*AL3911^2/AO3911","v":-23.787500000000005},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+H3911","v":61.5},null,"-",{"$f":"+Q3911","v":10},null,"*",{"$f":"+T3911","v":0.8},null,"-",{"$f":"+AC3911","v":4},null,"-",{"$f":"+AI3911","v":20},null,"*",{"$f":"+D3910","v":0.3},null,"=",{"$f":"+E3912-H3912*K3912-N3912-Q3912*T3912","v":43.5},null,null,"KN"]
[null,null,"m=",0.3,null,null,"m. ' deki moment ve kesme kuvveti miktarı",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(D3913<=V3843,\"\",\"azalt.\")","v":""}]
[null,null,"Mx =",null,{"$f":"+E3862","v":-83.737500000000011},null,"+",{"$f":"+H3862","v":61.5},null,"*(",{"$f":"+K3862","v":1.4500000000000002},null,"+",{"$f":"+D3913","v":0.3},null,")-",{"$f":"+P3862","v":10},null,"*",{"$f":"+S3862","v":0.8},null,"*(",{"$f":"+V3862","v":1.05},null,"+",{"$f":"+N3914","v":0.3},null,")-",{"$f":"+AA3862","v":4},null,"*(",{"$f":"+AD3862","v":0.65},null,"+",{"$f":"+Z3914","v":0.3},null,")-",{"$f":"+AI3862","v":20},null,"*",{"$f":"+AL3862","v":0.65},null,"*(",{"$f":"+AO3862","v":0.32500000000000001},null,"+",{"$f":"+AI3914","v":0.3},null,")-",{"$f":"+AT3862","v":8},null,"*",{"$f":"+AU3914","v":0.3},null,"-",{"$f":"+AY3862","v":30},null,"*",{"$f":"+BA3914","v":0.3},null,"² /",2,"=",{"$f":"E3914+H3914*(K3914+N3914)-Q3914*T3914*(W3914+Z3914)-AC3914*(AF3914+AI3914)-AL3914*AO3914*(AR3914+AU3914)-AX3914*BA3914-BD3914*BG3914^2/BJ3914","v":-2.5874999999999986},null,null,"KNm"]
[null,null,"Vx =",null,{"$f":"+H3914","v":61.5},null,"-",{"$f":"+Q3914","v":10},null,"*",{"$f":"+T3914","v":0.8},null,"-",{"$f":"+AC3914","v":4},null,"-",{"$f":"+AL3914","v":20},null,"*",{"$f":"+AO3914","v":0.65},null,"-",{"$f":"+AX3914","v":8},null,"-",{"$f":"+BD3914","v":30},null,"*",{"$f":"+BG3914","v":0.3},null,"=",{"$f":"E3915-H3915*K3915-N3915-Q3915*T3915-W3915-Z3915*AC3915","v":19.5},null,null,"KN"]